% Copyright 2018-2026 by Romano Giannetti
% Copyright 2015-2026 by Stefan Lindner
% Copyright 2013-2026 by Stefan Erhardt
% Copyright 2007-2026 by Massimo Redaelli
%
% This file may be distributed and/or modified
%
% 1. under the LaTeX Project Public License and/or
% 2. under the GNU Public License.
%
% See the files gpl-3.0_license.txt and lppl-1-3c_license.txt for more details.


%%%%%
%%%%%
%%%%%
%%%%% Se c'è l'opzione symbol, fallback to siunitx con warning
%%%%%
%%%%%

\NeedsTeXFormat{LaTeX2e}

\def\pgfcircversion{0.4}
\def\pgfcircversiondate{2012/12/20}

%% Version 2.0 of pgf/TikZ is required
\RequirePackage{tikz}
\usetikzlibrary{calc}
\usepgflibrary{decorations.pathmorphing,arrows}

\DeclareOption{european}{
	\ctikzset{voltage=european} \ctikzset{current=european} \ctikzset{inductor=european}
	 \ctikzset{resistor=european} \ctikzset{logic ports=european} \ctikzset{gas filled surge arrester = european} 
}

\DeclareOption{american}{
	\ctikzset{voltage=american} \ctikzset{current=american} \ctikzset{resistor=american} \ctikzset{inductor=american} \ctikzset{gas filled surge arrester = american}
	\ctikzset{logic ports = american}
}

\DeclareOption{fulldiodes}{
	\ctikzset{diode = full}
}

\DeclareOption{emptydiodes}{
	\ctikzset{diode = empty}
}

\DeclareOption{europeanvoltages}{
	\ctikzset{voltage=european}
}

\DeclareOption{americanvoltages}{
	\ctikzset{voltage=american}
}

\DeclareOption{europeancurrents}{
	\ctikzset{current = european}
}

\DeclareOption{americancurrents}{
	\ctikzset{current = american}
}

\DeclareOption{europeanvoltages}{
	\ctikzset{voltage = european}
}

\DeclareOption{americanresistors}{
	\ctikzset{resistor = american}
}

\DeclareOption{europeanresistors}{
	\ctikzset{resistor = european}
}

\DeclareOption{americaninductors}{
	\ctikzset{inductor = american}
}

\DeclareOption{europeaninductors}{
	\ctikzset{inductor = european}
}

\DeclareOption{cuteinductors}{
	\ctikzset{inductor = cute}
}

\DeclareOption{americanports}{
	\ctikzset{logic ports = american}
}

\DeclareOption{europeanports}{
	\ctikzset{logic ports = european}
}

\DeclareOption{americangfsurgearrester}{
	\ctikzset{gas filled surge arrester = american}
}

\DeclareOption{europeangfsurgearrester}{
	\ctikzset{gas filled surge arrester = european}
}


\DeclareOption{siunitx}{
	\pgf@circ@siunitxtrue
}

\DeclareOption{nosiunitx}{
	\pgf@circ@siunitxfalse
}

\DeclareOption{arrowmos}{
	\pgf@circuit@mos@arrowstrue
}

\DeclareOption{noarrowmos}{
	\pgf@circuit@mos@arrowsfalse
}

\DeclareOption{straightlabels}{
	\ctikzset{label/align = straight}
}

\DeclareOption{rotatelabels}{
	\ctikzset{label/align = rotate}
}

\DeclareOption{smartlabels}{
	\ctikzset{label/align = smart}
}



\DeclareOption{fulldiode}{
	\ctikzset{diode = full}
}

\DeclareOption{emptydiode}{
	\ctikzset{diode = empty}
}

\DeclareOption{europeanvoltage}{
	\ctikzset{voltage=european}
}

\DeclareOption{americanvoltage}{
	\ctikzset{voltage=american}
}

\DeclareOption{europeancurrent}{
	\ctikzset{current = european}
}

\DeclareOption{americancurrent}{
	\ctikzset{current = american}
}

\DeclareOption{europeanvoltage}{
	\ctikzset{voltage = european}
}

\DeclareOption{americanresistor}{
	\ctikzset{resistor = american}
}

\DeclareOption{europeanresistor}{
	\ctikzset{resistor = european}
}

\DeclareOption{americaninductor}{
	\ctikzset{inductor = american}
}

\DeclareOption{europeaninductor}{
	\ctikzset{inductor = european}
}

\DeclareOption{cuteinductor}{
	\ctikzset{inductor = cute}
}

\DeclareOption{americanport}{
	\ctikzset{logic ports = american}
}

\DeclareOption{europeanport}{
	\ctikzset{logic ports = european}
}

\DeclareOption{europeanport}{
	\ctikzset{logic ports = european}
}

\DeclareOption{betterproportions}{
	\ctikzset{monopoles/ground/width/.initial=.15}

	\ctikzset{bipoles/resistor/height/.initial=.23}
	\ctikzset{bipoles/resistor/width/.initial=.6}
	\ctikzset{bipoles/capacitor/height/.initial=.4}
	\ctikzset{bipoles/capacitor/width/.initial=.1}
	\ctikzset{bipoles/potentiometer/height/.initial=.6}
	\ctikzset{bipoles/potentiometer/height 2/.initial=.23}
	\ctikzset{bipoles/potentiometer/width/.initial=.6}
	\ctikzset{bipoles/photoresistor/height/.initial=.6}
	\ctikzset{bipoles/photoresistor/height 2/.initial=.23}
	\ctikzset{bipoles/photoresistor/width/.initial=.6}
	\ctikzset{bipoles/thermistor/main/.initial=.7}
	\ctikzset{bipoles/thermistor/height/.initial=.328}%.23/.7
	\ctikzset{bipoles/thermistor/width/.initial=.6}
	\ctikzset{bipoles/thermistorntc/width/.initial=.6}
	\ctikzset{bipoles/thermistorntc/main/.initial=.7}
	\ctikzset{bipoles/thermistorntc/height/.initial=.328}%.23/.7
	\ctikzset{bipoles/thermistorntc/height 2/.initial=.75}%.23/.7
	\ctikzset{bipoles/thermistorptc/width/.initial=.6}
	\ctikzset{bipoles/thermistorptc/main/.initial=.7}
	\ctikzset{bipoles/thermistorptc/height/.initial=.328}%.23/.7
	\ctikzset{bipoles/varistor/main/.initial=.7}
	\ctikzset{bipoles/varistor/height/.initial=.328}%.23/.7
	\ctikzset{bipoles/varistor/width/.initial=.6}
	\ctikzset{bipoles/vresistor/height/.initial=.45}
	\ctikzset{bipoles/vresistor/width/.initial=.6}
	\ctikzset{bipoles/cuteinductor/height/.initial=.23}
	\ctikzset{bipoles/cuteinductor/width/.initial=.6}
	\ctikzset{bipoles/cuteinductor/coils/.initial=6}
	\ctikzset{bipoles/americaninductor/height/.initial=.23}
	\ctikzset{bipoles/americaninductor/height 2/.initial=.1}
	\ctikzset{bipoles/americaninductor/width/.initial=.6}
	\ctikzset{bipoles/americaninductor/coils/.initial=4}
	\ctikzset{bipoles/vcuteinductor/height/.initial=.6}
	\ctikzset{bipoles/vcuteinductor/coil height/.initial=.23}
	\ctikzset{bipoles/vcuteinductor/width/.initial=.6}
	\ctikzset{bipoles/vcuteinductor/coils/.initial=6}
	\ctikzset{bipoles/vamericaninductor/height/.initial=.45}
	\ctikzset{bipoles/vamericaninductor/height 2/.initial=.2}
	\ctikzset{bipoles/vamericaninductor/width/.initial=.6}
	\ctikzset{bipoles/vamericaninductor/coils/.initial=4}
	\ctikzset{bipoles/generic/height/.initial=.23}
	\ctikzset{bipoles/generic/width/.initial=.6}
	\ctikzset{bipoles/generic potentiometer/height/.initial=.6}
	\ctikzset{bipoles/generic potentiometer/height 2/.initial=.23}
	\ctikzset{bipoles/generic potentiometer/width/.initial=.6}
	\ctikzset{bipoles/ageneric/height/.initial=.23}
	\ctikzset{bipoles/ageneric/width/.initial=.6}
	\ctikzset{bipoles/memristor/height/.initial=.23}
	\ctikzset{bipoles/memristor/wave height/.initial=.375}
	\ctikzset{bipoles/memristor/width/.initial=.60}
	\ctikzset{bipoles/tgeneric/height/.initial=.525}
	\ctikzset{bipoles/tgeneric/width/.initial=.6}
	\ctikzset{bipoles/tfullgeneric/height/.initial=.525}
	\ctikzset{bipoles/tfullgeneric/width/.initial=.60}
	\ctikzset{bipoles/fullgeneric/height/.initial=.23}
	\ctikzset{bipoles/fullgeneric/width/.initial=.6}
	\ctikzset{bipoles/diode/height/.initial=.3}
	\ctikzset{bipoles/diode/width/.initial=.25}
	
	\ctikzset{tripoles/thyristor/height/.initial=.66}
	\ctikzset{tripoles/thyristor/height 2/.initial=.3}
	\ctikzset{tripoles/thyristor/width/.initial=.6}
	\ctikzset{tripoles/thyristor/diode height/.initial=.3}
	\ctikzset{tripoles/thyristor/diode width left/.initial=.4}
	\ctikzset{tripoles/thyristor/diode width right/.initial=.3}

	\ctikzset{tripoles/triac/height/.initial=.66}
	\ctikzset{tripoles/triac/width/.initial=.6}
	\ctikzset{tripoles/triac/diode width left/.initial=.3}
	\ctikzset{tripoles/triac/diode width right/.initial=.3}
}

%%%%%%%%%



%%%%%%%%%%% Springe nach circuitikz.code
%%%---------- open: circuitikz.code.tex

%% Options




%% Keys

\long\def\pgf@circ@comment#1{}

\def\circuitikzbasekey{/tikz/circuitikz}

\pgfkeys{\circuitikzbasekey/.is family}

\def\circuitikzset#1{\pgfkeys{\circuitikzbasekey,#1}}
\let\ctikzset\circuitikzset
\def\ctikzvalof#1{\pgfkeysvalueof{\circuitikzbasekey/#1}}
\def\ctikzsetvalof#1#2{\pgfkeyssetvalue{\circuitikzbasekey/#1}{#2}}

\newif\ifpgf@circuit@inputarrow
\ctikzset{inputarrow/.is choice}
\ctikzset{inputarrow/true/.code={\pgf@circuit@inputarrowtrue}}
\ctikzset{inputarrow/false/.code={\pgf@circuit@inputarrowfalse}}

\ctikzset{bipoles/.is family}
\ctikzset{bipoles/border margin/.initial=1.1}
\ctikzset{bipoles/thickness/.initial=2} 
\ctikzset{bipoles/length/.initial=1.4cm} 
\ctikzset{nodes width/.initial=.04}
\newdimen\pgf@circ@Rlen 
\ctikzset{bipoles/length/.code={\pgf@circ@Rlen = #1}} 


\ctikzset{monopoles/.is family}
\ctikzset{monopoles/ground/width/.initial=.25}
\ctikzset{monopoles/chassis/width/.initial=.25}
\ctikzset{monopoles/alternative chassis/width/.initial=.25}
\ctikzset{monopoles/equipotentiality/width/.initial=.25}
\ctikzset{monopoles/tlinestub/width/.initial=.25}          
\ctikzset{monopoles/antenna/width/.initial=.25}            
\ctikzset{monopoles/antenna/label/xanchor/.initial=.4}            
\ctikzset{monopoles/antenna/label/yanchor/.initial=.75}            
\ctikzset{monopoles/txantenna/label/xanchor/.initial=.4}            
\ctikzset{monopoles/txantenna/label/yanchor/.initial=.75}            
\ctikzset{monopoles/txantenna/width/.initial=.25}
\ctikzset{monopoles/rxantenna/label/xanchor/.initial=.4}            
\ctikzset{monopoles/rxantenna/label/yanchor/.initial=.75}            
\ctikzset{monopoles/rxantenna/width/.initial=.25}
\ctikzset{monopoles/tground/thickness/.initial=3}
\ctikzset{monopoles/vcc/width/.initial=.2}
\ctikzset{monopoles/match/width/.initial=.4}
\ctikzset{monopoles/oscillator/width/.initial=.7}

\ctikzset{bipoles/resistor/height/.initial=.3}
\ctikzset{bipoles/resistor/width/.initial=.8}
\ctikzset{bipoles/potentiometer/height/.initial=.8}
\ctikzset{bipoles/potentiometer/height 2/.initial=.3}
\ctikzset{bipoles/potentiometer/width/.initial=.8}
\ctikzset{bipoles/photoresistor/height/.initial=.6}
\ctikzset{bipoles/photoresistor/height 2/.initial=.3}
\ctikzset{bipoles/photoresistor/width/.initial=.8}
\ctikzset{bipoles/thermistor/main/.initial=.7}
\ctikzset{bipoles/thermistor/height/.initial=.428}%.3/.7
\ctikzset{bipoles/thermistorntc/width/.initial=.8}
\ctikzset{bipoles/thermistorntc/main/.initial=.7}
\ctikzset{bipoles/thermistorntc/height/.initial=.428}%.3/.7
\ctikzset{bipoles/thermistorntc/height 2/.initial=.75}%.3/.7
\ctikzset{bipoles/thermistorptc/width/.initial=.8}
\ctikzset{bipoles/thermistorptc/main/.initial=.7}
\ctikzset{bipoles/thermistorptc/height/.initial=.428}%.3/.7
\ctikzset{bipoles/thermistorptc/height 2/.initial=.75}%.3/.7
\ctikzset{bipoles/thermistor/width/.initial=.8}
\ctikzset{bipoles/varistor/main/.initial=.7}
\ctikzset{bipoles/varistor/height/.initial=.428}%.3/.7
\ctikzset{bipoles/varistor/width/.initial=.8}
\ctikzset{bipoles/vresistor/height/.initial=.6}
\ctikzset{bipoles/vresistor/width/.initial=.8}
\ctikzset{bipoles/cuteinductor/height/.initial=.3}
\ctikzset{bipoles/cuteinductor/width/.initial=.8}
\ctikzset{bipoles/cuteinductor/coils/.initial=6}
\ctikzset{bipoles/americaninductor/height/.initial=.3}
\ctikzset{bipoles/americaninductor/height 2/.initial=.1}
\ctikzset{bipoles/americaninductor/width/.initial=.8}
\ctikzset{bipoles/americaninductor/coils/.initial=4}
\ctikzset{bipoles/vcuteinductor/height/.initial=.6}
\ctikzset{bipoles/vcuteinductor/coil height/.initial=.3}
\ctikzset{bipoles/vcuteinductor/width/.initial=.8}
\ctikzset{bipoles/vcuteinductor/coils/.initial=6}
\ctikzset{bipoles/vamericaninductor/height/.initial=.6}
\ctikzset{bipoles/vamericaninductor/height 2/.initial=.2}
\ctikzset{bipoles/vamericaninductor/width/.initial=.8}
\ctikzset{bipoles/vamericaninductor/coils/.initial=4}
\ctikzset{bipoles/isource/height/.initial=.60}
\ctikzset{bipoles/isource/width/.initial=.60}
\ctikzset{bipoles/isourceam/height/.initial=.60}
\ctikzset{bipoles/isourceam/width/.initial=.60}
\ctikzset{bipoles/vsource/height/.initial=.60}
\ctikzset{bipoles/vsource/width/.initial=.60}
\ctikzset{bipoles/vsourceam/height/.initial=.60}
\ctikzset{bipoles/vsourceam/width/.initial=.60}
\ctikzset{bipoles/vsourceam/margin/.initial=.7}
\ctikzset{bipoles/isourcesin/height/.initial=.60}
\ctikzset{bipoles/isourcesin/width/.initial=.60}
\ctikzset{bipoles/vsourcesin/height/.initial=.60}
\ctikzset{bipoles/vsourcesin/width/.initial=.60}
\ctikzset{bipoles/vsourcesquare/height/.initial=.60}
\ctikzset{bipoles/vsourcesquare/width/.initial=.60}
\ctikzset{bipoles/cisource/height/.initial=.7}
\ctikzset{bipoles/cisource/width/.initial=.7}
\ctikzset{bipoles/cisourceam/height/.initial=.7}
\ctikzset{bipoles/cisourceam/width/.initial=.7}
\ctikzset{bipoles/cvsource/height/.initial=.7}
\ctikzset{bipoles/cvsource/width/.initial=.7}
\ctikzset{bipoles/cvsourceam/height/.initial=.7}
\ctikzset{bipoles/cvsourceam/width/.initial=.7}
\ctikzset{bipoles/cvsourceam/margin/.initial=.7}
\ctikzset{bipoles/cvsourceam/text scale/.initial=1}
\ctikzset{bipoles/cisourcesin/width/.initial=.7}
\ctikzset{bipoles/cvsourcesin/height/.initial=.7}
\ctikzset{bipoles/cvsourcesin/width/.initial=.7}
\ctikzset{bipoles/capacitor/height/.initial=.6}
\ctikzset{bipoles/capacitor/width/.initial=.2}
\ctikzset{bipoles/pcapacitor/height/.initial=.6}
\ctikzset{bipoles/pcapacitor/width/.initial=.2}
\ctikzset{bipoles/pcapacitor/bend width/.initial=1.1}
\ctikzset{bipoles/vcapacitor/height/.initial=.6}
\ctikzset{bipoles/vcapacitor/width/.initial=.5}
\ctikzset{bipoles/vcapacitor/capacitor width/.initial=.4}
\ctikzset{bipoles/battery/height/.initial=.6}
\ctikzset{bipoles/battery/width/.initial=.3}
\ctikzset{bipoles/battery1/height/.initial=.6}
\ctikzset{bipoles/battery1/width/.initial=.3}
\ctikzset{bipoles/diode/height/.initial=.50}
\ctikzset{bipoles/diode/width/.initial=.40}
\ctikzset{bipoles/varcap/height/.initial=.50}
\ctikzset{bipoles/varcap/width/.initial=.45}
\ctikzset{bipoles/interr/height/.initial=.35}
\ctikzset{bipoles/interr/width/.initial=.35}
\ctikzset{bipoles/interr/height 2/.initial=.1}
\ctikzset{bipoles/generic/height/.initial=.30}
\ctikzset{bipoles/generic/width/.initial=.80}
\ctikzset{bipoles/european gas filled surge arrester/height/.initial=.30}
\ctikzset{bipoles/european gas filled surge arrester/width/.initial=.80}
\ctikzset{bipoles/european gas filled surge arrester/inside/.initial=.30}
\ctikzset{bipoles/american gas filled surge arrester/height/.initial=.60}
\ctikzset{bipoles/american gas filled surge arrester/width/.initial=.60}
\ctikzset{bipoles/american gas filled surge arrester/inside/.initial=.15}
\ctikzset{bipoles/american gas filled surge arrester/dot x/.initial=.25}
\ctikzset{bipoles/american gas filled surge arrester/dot y/.initial=.45}
\ctikzset{bipoles/american gas filled surge arrester/size/.initial=.1}
\ctikzset{bipoles/fuse/height/.initial=.20}
\ctikzset{bipoles/fuse/width/.initial=.50}
\ctikzset{bipoles/afuse/height/.initial=.20}
\ctikzset{bipoles/afuse/width/.initial=.50}
\ctikzset{bipoles/generic potentiometer/height/.initial=.80}
\ctikzset{bipoles/generic potentiometer/height 2/.initial=.30}
\ctikzset{bipoles/generic potentiometer/width/.initial=.80}
\ctikzset{bipoles/ageneric/height/.initial=.30}
\ctikzset{bipoles/ageneric/width/.initial=.80}
\ctikzset{bipoles/memristor/height/.initial=.30}
\ctikzset{bipoles/memristor/wave height/.initial=.5}
\ctikzset{bipoles/memristor/width/.initial=.80}
\ctikzset{bipoles/tgeneric/height/.initial=.70}
\ctikzset{bipoles/tgeneric/width/.initial=.80}
\ctikzset{bipoles/tfullgeneric/height/.initial=.70}
\ctikzset{bipoles/tfullgeneric/width/.initial=.80}
\ctikzset{bipoles/fullgeneric/height/.initial=.30}
\ctikzset{bipoles/fullgeneric/width/.initial=.80}
\ctikzset{bipoles/open/height/.initial=.25}
\ctikzset{bipoles/open/width/.initial=.8}
\ctikzset{bipoles/ammeter/height/.initial=.60}
\ctikzset{bipoles/ammeter/width/.initial=.60}
\ctikzset{bipoles/voltmeter/height/.initial=.60}
\ctikzset{bipoles/voltmeter/width/.initial=.60}
\ctikzset{bipoles/buffer/height/.initial=1}
\ctikzset{bipoles/buffer/width/.initial=1}
\ctikzset{bipoles/not port/width/.initial=1}
\ctikzset{bipoles/not port/height/.initial=.8}
\ctikzset{bipoles/not port/circle width/.initial=.15}
\ctikzset{bipoles/lamp/height/.initial=.60}
\ctikzset{bipoles/lamp/width/.initial=.60}
\ctikzset{bipoles/tline/height/.initial=.3}
\ctikzset{bipoles/tline/width/.initial=.8}
\ctikzset{bipoles/squid/height/.initial=.60}
\ctikzset{bipoles/squid/width/.initial=.60}
\ctikzset{bipoles/barrier/height/.initial=.60}
\ctikzset{bipoles/barrier/width/.initial=.60}
\ctikzset{bipoles/thermocouple/height/.initial=.250}
\ctikzset{bipoles/thermocouple/height 2/.initial=.60}
\ctikzset{bipoles/thermocouple/width/.initial=.140}
\ctikzset{bipoles/pushbutton/height/.initial=.5}
\ctikzset{bipoles/pushbutton/height 2/.initial=.0}
\ctikzset{bipoles/pushbutton/width/.initial=.50}
\ctikzset{bipoles/twoport/width/.initial=.7}
\ctikzset{bipoles/twoport/height/.initial=.7}
\ctikzset{bipoles/twoport/text/.initial=}
\ctikzset{bipoles/vco/width/.initial=.7}
\ctikzset{bipoles/bandpass/width/.initial=.7}
\ctikzset{bipoles/highpass/width/.initial=.7}
\ctikzset{bipoles/lowpass/width/.initial=.7}
\ctikzset{bipoles/adc/width/.initial=.7}
\ctikzset{bipoles/dac/width/.initial=.7}
\ctikzset{bipoles/dsp/width/.initial=.7}
\ctikzset{bipoles/fft/width/.initial=.7}
\ctikzset{bipoles/amp/width/.initial=.7}
\ctikzset{bipoles/vamp/width/.initial=.7}
\ctikzset{bipoles/piattenuator/width/.initial=.7}
\ctikzset{bipoles/vpiattenuator/width/.initial=.7}
\ctikzset{bipoles/tattenuator/width/.initial=.7}
\ctikzset{bipoles/vtattenuator/width/.initial=.7}
\ctikzset{bipoles/phaseshifter/width/.initial=.7}
\ctikzset{bipoles/vphaseshifter/width/.initial=.7}
\ctikzset{bipoles/detector/width/.initial=.7}

\newif\ifpgf@circuit@mos@arrows
\ctikzset{tripoles/mos style/.is choice}
\ctikzset{tripoles/mos style/no arrows/.code={\pgf@circuit@mos@arrowsfalse}}
\ctikzset{tripoles/mos style/arrows/.code={\pgf@circuit@mos@arrowstrue}}
\ctikzset{tripoles/nmos/width/.initial=.7}
\ctikzset{tripoles/nmos/gate height/.initial=.35}
\ctikzset{tripoles/nmos/base height/.initial=.5}
\ctikzset{tripoles/nmos/height/.initial=1.1}
\ctikzset{tripoles/nmos/base width/.initial=.5}
\ctikzset{tripoles/nmos/gate width/.initial=.62}
\ctikzset{tripoles/pmos/width/.initial=.7}
\ctikzset{tripoles/pmos/gate height/.initial=.35}
\ctikzset{tripoles/pmos/base height/.initial=.5}
\ctikzset{tripoles/pmos/height/.initial=1.1}
\ctikzset{tripoles/pmos/base width/.initial=.5}
\ctikzset{tripoles/pmos/gate width/.initial=.62}

\ctikzset{tripoles/nfet/width/.initial=.7}
\ctikzset{tripoles/nfet/gate height/.initial=.35}
\ctikzset{tripoles/nfet/base height/.initial=.5}
\ctikzset{tripoles/nfet/height/.initial=1.1}
\ctikzset{tripoles/nfet/base width/.initial=.5}
\ctikzset{tripoles/nfet/gate width/.initial=.62}

\ctikzset{tripoles/pfet/width/.initial=.7}
\ctikzset{tripoles/pfet/gate height/.initial=.35}
\ctikzset{tripoles/pfet/base height/.initial=.5}
\ctikzset{tripoles/pfet/height/.initial=1.1}
\ctikzset{tripoles/pfet/base width/.initial=.5}
\ctikzset{tripoles/pfet/gate width/.initial=.62}

\ctikzset{tripoles/nigfete/width/.initial=.7}
\ctikzset{tripoles/nigfete/gate height/.initial=.35}
\ctikzset{tripoles/nigfete/base height/.initial=.5}
\ctikzset{tripoles/nigfete/height/.initial=1.1}
\ctikzset{tripoles/nigfete/base width/.initial=.5}
\ctikzset{tripoles/nigfete/gate width/.initial=.62}

\ctikzset{tripoles/nigfetd/width/.initial=.7}
\ctikzset{tripoles/nigfetd/gate height/.initial=.35}
\ctikzset{tripoles/nigfetd/base height/.initial=.5}
\ctikzset{tripoles/nigfetd/height/.initial=1.1}
\ctikzset{tripoles/nigfetd/base width/.initial=.5}
\ctikzset{tripoles/nigfetd/gate width/.initial=.62}

\ctikzset{tripoles/pigfete/width/.initial=.7}
\ctikzset{tripoles/pigfete/gate height/.initial=.35}
\ctikzset{tripoles/pigfete/base height/.initial=.5}
\ctikzset{tripoles/pigfete/height/.initial=1.1}
\ctikzset{tripoles/pigfete/base width/.initial=.5}
\ctikzset{tripoles/pigfete/gate width/.initial=.62}

\ctikzset{tripoles/pigfetd/width/.initial=.7}
\ctikzset{tripoles/pigfetd/gate height/.initial=.35}
\ctikzset{tripoles/pigfetd/base height/.initial=.5}
\ctikzset{tripoles/pigfetd/height/.initial=1.1}
\ctikzset{tripoles/pigfetd/base width/.initial=.5}
\ctikzset{tripoles/pigfetd/gate width/.initial=.62}

\ctikzset{tripoles/npn/width/.initial=.6}
\ctikzset{tripoles/npn/gate height/.initial=.45}
\ctikzset{tripoles/npn/gate height 2/.initial=.15}
\ctikzset{tripoles/npn/base height/.initial=.4}
\ctikzset{tripoles/npn/height/.initial=1.1}
\ctikzset{tripoles/npn/gate width/.initial=.5}



\ctikzset{tripoles/pnp/width/.initial=.6}
\ctikzset{tripoles/pnp/gate height/.initial=.45}
\ctikzset{tripoles/pnp/gate height 2/.initial=.15}
\ctikzset{tripoles/pnp/base height/.initial=.4}
\ctikzset{tripoles/pnp/height/.initial=1.1}
\ctikzset{tripoles/pnp/gate width/.initial=.5}

\ctikzset{tripoles/pigbt/width/.initial=.6}
\ctikzset{tripoles/pigbt/gate height/.initial=.45}
\ctikzset{tripoles/pigbt/gate height 2/.initial=.15}
\ctikzset{tripoles/pigbt/base height/.initial=.4}
\ctikzset{tripoles/pigbt/height/.initial=1.1}
\ctikzset{tripoles/pigbt/gate width/.initial=.62}
\ctikzset{tripoles/pigbt/base width/.initial=.5}
\ctikzset{tripoles/nigbt/width/.initial=.6}
\ctikzset{tripoles/nigbt/gate height/.initial=.45}
\ctikzset{tripoles/nigbt/gate height 2/.initial=.15}
\ctikzset{tripoles/nigbt/base height/.initial=.4}
\ctikzset{tripoles/nigbt/height/.initial=1.1}
\ctikzset{tripoles/nigbt/gate width/.initial=.62}
\ctikzset{tripoles/nigbt/base width/.initial=.5}

\ctikzset{tripoles/njfet/width/.initial=.7}
\ctikzset{tripoles/njfet/gate height/.initial=.5}
\ctikzset{tripoles/njfet/gate height 2/.initial=.35}
\ctikzset{tripoles/njfet/gate width/.initial=.5}
\ctikzset{tripoles/njfet/height/.initial=1.1}
\ctikzset{tripoles/pjfet/width/.initial=.7}
\ctikzset{tripoles/pjfet/gate height/.initial=.5}
\ctikzset{tripoles/pjfet/gate height 2/.initial=.35}
\ctikzset{tripoles/pjfet/gate width/.initial=.5}
\ctikzset{tripoles/pjfet/height/.initial=1.1}

\ctikzset{tripoles/isfet/width/.initial=1}
\ctikzset{tripoles/isfet/gate height/.initial=.35}
\ctikzset{tripoles/isfet/base height/.initial=.5}
\ctikzset{tripoles/isfet/height/.initial=1.1}
\ctikzset{tripoles/isfet/base width/.initial=.3}
\ctikzset{tripoles/isfet/gate width/.initial=.5}
\ctikzset{tripoles/isfet/wave width/.initial=.16}
\ctikzset{tripoles/isfet/wave amp/.initial=.06}
\ctikzset{tripoles/isfet/waves y sep/.initial=.22}
\ctikzset{tripoles/isfet/waves x sep/.initial=.8}

\newif\ifpgf@circuit@europeanlogicport
\ctikzset{logic ports/.is choice}
\ctikzset{logic ports/european/.code= {\pgf@circuit@europeanlogicporttrue } }
\ctikzset{logic ports/american/.code= {\pgf@circuit@europeanlogicportfalse } } 

\newif\ifpgf@circuit@bipole@voltage@backward
\ctikzset{bipole/voltage/direction/.is choice}
\ctikzset{bipole/voltage/direction/forward/.code={\pgf@circuit@bipole@voltage@backwardfalse}}
\ctikzset{bipole/voltage/direction/backward/.code={\pgf@circuit@bipole@voltage@backwardtrue}}

\ctikzset{tripoles/american and port/width/.initial=1.1}
\ctikzset{tripoles/american and port/height/.initial=.8}
\ctikzset{tripoles/american and port/port width/.initial=.7}
\ctikzset{tripoles/american and port/input height/.initial=.5}
\ctikzset{tripoles/american nand port/width/.initial=1.1}
\ctikzset{tripoles/american nand port/height/.initial=.8}
\ctikzset{tripoles/american nand port/port width/.initial=.7}
\ctikzset{tripoles/american nand port/circle width/.initial=.15}
\ctikzset{tripoles/american nand port/input height/.initial=.5}
\ctikzset{tripoles/american or port/width/.initial=1.1}
\ctikzset{tripoles/american or port/height/.initial=.8}
\ctikzset{tripoles/american or port/port width/.initial=.7}
\ctikzset{tripoles/american or port/input height/.initial=.5}
\ctikzset{tripoles/american or port/input skip/.initial=.25}
\ctikzset{tripoles/american or port/aaa/.initial=.6}
\ctikzset{tripoles/american or port/bbb/.initial=.4} 
\ctikzset{tripoles/american or port/ccc/.initial=.5} 
\ctikzset{tripoles/american or port/ddd/.initial=.0}
\ctikzset{tripoles/american nor port/width/.initial=1.1}
\ctikzset{tripoles/american nor port/height/.initial=.8}
\ctikzset{tripoles/american nor port/port width/.initial=.7}
\ctikzset{tripoles/american nor port/input height/.initial=.5}
\ctikzset{tripoles/american nor port/input skip/.initial=.25}
\ctikzset{tripoles/american nor port/circle width/.initial=.15}
\ctikzset{tripoles/american nor port/aaa/.initial=.6}
\ctikzset{tripoles/american nor port/bbb/.initial=.4} 
\ctikzset{tripoles/american nor port/ccc/.initial=.5} 
\ctikzset{tripoles/american nor port/ddd/.initial=.0}
\ctikzset{tripoles/american xor port/width/.initial=1.1}
\ctikzset{tripoles/american xor port/height/.initial=.8}
\ctikzset{tripoles/american xor port/port width/.initial=.7}
\ctikzset{tripoles/american xor port/input height/.initial=.5}
\ctikzset{tripoles/american xor port/input skip/.initial=.15}
\ctikzset{tripoles/american xor port/distance/.initial=.1} 
\ctikzset{tripoles/american xor port/aaa/.initial=.6}
\ctikzset{tripoles/american xor port/bbb/.initial=.4} 
\ctikzset{tripoles/american xor port/ccc/.initial=.5} 
\ctikzset{tripoles/american xor port/ddd/.initial=.0}
\ctikzset{tripoles/american xnor port/width/.initial=1.1}
\ctikzset{tripoles/american xnor port/height/.initial=.8}
\ctikzset{tripoles/american xnor port/port width/.initial=.7}
\ctikzset{tripoles/american xnor port/input height/.initial=.5}
\ctikzset{tripoles/american xnor port/input skip/.initial=.15}
\ctikzset{tripoles/american xnor port/distance/.initial=.1} 
\ctikzset{tripoles/american xnor port/aaa/.initial=.6}
\ctikzset{tripoles/american xnor port/bbb/.initial=.4} 
\ctikzset{tripoles/american xnor port/ccc/.initial=.5} 
\ctikzset{tripoles/american xnor port/ddd/.initial=.0}
\ctikzset{tripoles/american xnor port/circle width/.initial=.15}
\ctikzset{tripoles/european and port/width/.initial=1.4}
\ctikzset{tripoles/european and port/height/.initial=.65}
\ctikzset{tripoles/european and port/reserved/.initial=.6}
\ctikzset{tripoles/european and port/input height/.initial=.6}
\ctikzset{tripoles/european or port/width/.initial=1.4}
\ctikzset{tripoles/european or port/height/.initial=.65}
\ctikzset{tripoles/european or port/reserved/.initial=.6}
\ctikzset{tripoles/european or port/input height/.initial=.6}
\ctikzset{tripoles/european xor port/width/.initial=1.4}
\ctikzset{tripoles/european xor port/height/.initial=.65}
\ctikzset{tripoles/european xor port/reserved/.initial=.6}
\ctikzset{tripoles/european xor port/input height/.initial=.6}
\ctikzset{tripoles/european nand port/width/.initial=1.4}
\ctikzset{tripoles/european nand port/not height/.initial=.3}
\ctikzset{tripoles/european nand port/not width/.initial=.8}
\ctikzset{tripoles/european nand port/height/.initial=.65}
\ctikzset{tripoles/european nand port/reserved/.initial=.6}
\ctikzset{tripoles/european nand port/input height/.initial=.6}
\ctikzset{tripoles/european not port/width/.initial=1.4}
\ctikzset{tripoles/european not port/not height/.initial=.3}
\ctikzset{tripoles/european not port/not width/.initial=.8}
\ctikzset{tripoles/european not port/height/.initial=.65}
\ctikzset{tripoles/european not port/reserved/.initial=.6}
\ctikzset{tripoles/european not port/input height/.initial=0}
\ctikzset{tripoles/european xnor port/width/.initial=1.4}
\ctikzset{tripoles/european xnor port/not height/.initial=.3}
\ctikzset{tripoles/european xnor port/not width/.initial=.8}
\ctikzset{tripoles/european xnor port/height/.initial=.65}
\ctikzset{tripoles/european xnor port/reserved/.initial=.6}
\ctikzset{tripoles/european xnor port/input height/.initial=.6}
\ctikzset{tripoles/european nor port/width/.initial=1.4}
\ctikzset{tripoles/european nor port/not height/.initial=.3}
\ctikzset{tripoles/european nor port/not width/.initial=.8}
\ctikzset{tripoles/european nor port/height/.initial=.65}
\ctikzset{tripoles/european nor port/reserved/.initial=.6}
\ctikzset{tripoles/european nor port/input height/.initial=.6}
\ctikzset{tripoles/op amp/width/.initial=1.7}
\ctikzset{tripoles/op amp/port width/.initial=.7}
\ctikzset{tripoles/op amp/height/.initial=1.4}
\ctikzset{tripoles/op amp/input height/.initial=.5}
\ctikzset{tripoles/op amp/up pos/.initial=.45}
\ctikzset{tripoles/plain amp/width/.initial=1.7}
\ctikzset{tripoles/plain amp/port width/.initial=.7}
\ctikzset{tripoles/plain amp/height/.initial=1.4}
\ctikzset{tripoles/plain amp/input height/.initial=.5}
\ctikzset{tripoles/plain amp/up pos/.initial=.45}

\ctikzset{tripoles/thyristor/height/.initial=1.10}
\ctikzset{tripoles/thyristor/height 2/.initial=.5}
\ctikzset{tripoles/thyristor/width/.initial=1.0}
\ctikzset{tripoles/thyristor/diode height/.initial=.5}
\ctikzset{tripoles/thyristor/diode width left/.initial=.4}
\ctikzset{tripoles/thyristor/diode width right/.initial=.3}

\ctikzset{tripoles/triac/height/.initial=1.1}
\ctikzset{tripoles/triac/width/.initial=1}
\ctikzset{tripoles/triac/diode width left/.initial=.3}
\ctikzset{tripoles/triac/diode width right/.initial=.3}

\ctikzset{tripoles/spdt/width/.initial=.85}
\ctikzset{tripoles/spdt/height/.initial=.45}
\ctikzset{tripoles/spdt/margin/.initial=.45}

\ctikzset{tripoles/toggleswitch/height/.initial=.8}
\ctikzset{tripoles/toggleswitch/height 2/.initial=.0}
\ctikzset{tripoles/toggleswitch/width/.initial=.80}

\ctikzset{tripoles/mixer/width/.initial=0.7}
\ctikzset{tripoles/adder/width/.initial=0.7}
\ctikzset{tripoles/circulator/width/.initial=.7}

\ctikzset{tripoles/wilkinson/height/.initial=1.3}
\ctikzset{tripoles/wilkinson/width/.initial=1.3}

\ctikzset{quadpoles/transformer/width/.initial=1.5}
\ctikzset{quadpoles/transformer/width1/.initial=.4}
\ctikzset{quadpoles/transformer/height/.initial=1.5}
\ctikzset{quadpoles/transformer/height1/.initial=.8}
\ctikzset{quadpoles/transformer core/width/.initial=1.5}
\ctikzset{quadpoles/transformer core/height/.initial=1.5}
\ctikzset{quadpoles/transformer core/core height/.initial=.5}
\ctikzset{quadpoles/transformer core/core width/.initial=.05}
\ctikzset{quadpoles/gyrator/width/.initial=1.5}
\ctikzset{quadpoles/gyrator/height/.initial=1.5}
\ctikzset{quadpoles/coupler/width/.initial=1.3}
\ctikzset{quadpoles/coupler/height/.initial=1.3}

\ctikzset{bipole/.is family}
\ctikzset{bipole/kind/.initial = }
\ctikzset{bipole/name/.initial = }
\newif\ifpgf@circuit@bipole@reversed
\ctikzset{bipole/reversed/.is if=pgf@circuit@bipole@reversed}
\newif\ifpgf@circuit@bipole@isvoltage
\ctikzset{bipole/is voltage/.is if=pgf@circuit@bipole@isvoltage}
\newif\ifpgf@circuit@bipole@iscurrent
\ctikzset{bipole/is current/.is if=pgf@circuit@bipole@iscurrent}

\ctikzset{bipole/voltage/.is family}
\newif\ifpgf@circuit@bipole@voltage@backward
\ctikzset{bipole/voltage/direction/.is choice}
\ctikzset{bipole/voltage/direction/forward/.code={\pgf@circuit@bipole@voltage@backwardfalse}}
\ctikzset{bipole/voltage/direction/backward/.code={\pgf@circuit@bipole@voltage@backwardtrue}}
\newif\ifpgf@circuit@bipole@voltage@below
\ctikzset{bipole/voltage/position/.is choice}
\ctikzset{bipole/voltage/position/above/.code={\pgf@circuit@bipole@voltage@belowfalse}}
\ctikzset{bipole/voltage/position/below/.code={\pgf@circuit@bipole@voltage@belowtrue}}

\ctikzset{bipole/voltage/label/unit/.initial=}
\ctikzset{bipole/voltage/label/name/.initial=}

\ctikzset{bipole/current/.is family}
\newif\ifpgf@circuit@bipole@current@backward
\ctikzset{bipole/current/direction/.is choice}
\ctikzset{bipole/current/direction/forward/.code={\pgf@circuit@bipole@current@backwardfalse}}
\ctikzset{bipole/current/direction/backward/.code={\pgf@circuit@bipole@current@backwardtrue}}
\newif\ifpgf@circuit@bipole@current@before
\ctikzset{bipole/current/x position/.is choice}
\ctikzset{bipole/current/x position/after/.code={\pgf@circuit@bipole@current@beforefalse}}
\ctikzset{bipole/current/x position/before/.code={\pgf@circuit@bipole@current@beforetrue}}
\newif\ifpgf@circuit@bipole@current@below
\ctikzset{bipole/current/y position/.is choice}
\ctikzset{bipole/current/y position/above/.code={\pgf@circuit@bipole@current@belowfalse}}
\ctikzset{bipole/current/y position/below/.code={\pgf@circuit@bipole@current@belowtrue}}

\ctikzset{bipole/current/label/unit/.initial=}
\ctikzset{bipole/current/label/name/.initial=}

\ctikzset{bipole/label/.is family}
\ctikzset{bipole/label/position/.initial=90}
\ctikzset{bipole/label/unit/.initial=}
\ctikzset{bipole/label/name/.initial=}
\ctikzset{bipole/nodes/.is family}
\ctikzset{bipole/nodes/left/.is choice}
\ctikzset{bipole/nodes/left/none/.code={\ctikzsetvalof{bipole/nodes/left}{none}}}
\ctikzset{bipole/nodes/left/empty/.code={\ctikzsetvalof{bipole/nodes/left}{empty}}}
\ctikzset{bipole/nodes/left/full/.code={\ctikzsetvalof{bipole/nodes/left}{full}}}
\ctikzset{bipole/nodes/right/.is choice}
\ctikzset{bipole/nodes/right/none/.code={\ctikzsetvalof{bipole/nodes/right}{none}}}
\ctikzset{bipole/nodes/right/empty/.code={\ctikzsetvalof{bipole/nodes/right}{empty}}}
\ctikzset{bipole/nodes/right/full/.code={\ctikzsetvalof{bipole/nodes/right}{full}}}


\newif\ifpgf@circuit@europeanresistor
\ctikzset{resistor/.is choice}
\ctikzset{resistor/american/.code = \pgf@circuit@europeanresistorfalse }
\ctikzset{resistor/european/.code = \pgf@circuit@europeanresistortrue }

\ctikzset{inductor/.is choice}
\ctikzset{inductor/cute/.code={\ctikzsetvalof{inductor}{cute}}}
\ctikzset{inductor/european/.code={\ctikzsetvalof{inductor}{european}}}
\ctikzset{inductor/american/.code={\ctikzsetvalof{inductor}{american}}}

\newif\ifpgf@circuit@fulldiode
\ctikzset{diode/.is if=pgf@circuit@fulldiode}
\ctikzset{diode/.is choice}
\ctikzset{diode/empty/.code = \pgf@circuit@fulldiodefalse }
\ctikzset{diode/full/.code = \pgf@circuit@fulldiodetrue }
\ctikzset{thickness/.initial=2}
\ctikzset{color/.initial=black}
\pgfkeys{/tikz/color/.add code={}{\ctikzset{color=#1}}}


\newif\ifpgf@circ@siunitx
\newif\ifpgf@circ@siunitx@res

\ctikzset{voltage/.is family}
\ctikzset{voltage/distance from node/.initial=.5} %\pgf@circ@Rlen units
\ctikzset{voltage/distance from line/.initial=.08} % pos, tra 0 e 1
\ctikzset{voltage/bump a/.initial=1.2}
\ctikzset{voltage/bump b/.initial=1.5}
\ctikzset{voltage/european label distance/.initial=1.4}
\ctikzset{voltage/american label distance/.initial=1.1}
% special cases
\ctikzset{bipoles/generic/voltage/distance from node/.initial=.4}
\ctikzset{bipoles/generic/voltage/bump b/.initial=2}
\ctikzset{bipoles/generic/voltage/european label distance/.initial=1.8}
%\ctikzset{bipoles/thermocouple/voltage/distance from node/.initial=.3}
\ctikzset{bipoles/thermocouple/voltage/bump b/.initial=2.2}
\ctikzset{bipoles/thermocouple/voltage/european label distance/.initial=1.5}
\ctikzset{bipoles/ageneric/voltage/distance from node/.initial=.4}
\ctikzset{bipoles/ageneric/voltage/bump b/.initial=2}
\ctikzset{bipoles/ageneric/voltage/european label distance/.initial=1.8}
\ctikzset{bipoles/fullgeneric/voltage/distance from node/.initial=.4}
\ctikzset{bipoles/fullgeneric/voltage/bump b/.initial=2}
\ctikzset{bipoles/fullgeneric/voltage/european label distance/.initial=1.8}
\ctikzset{bipoles/memristor/voltage/distance from node/.initial=.4}
\ctikzset{bipoles/memristor/voltage/bump b/.initial=2}
\ctikzset{bipoles/memristor/voltage/european label distance/.initial=1.8}
%\ctikzset{bipoles/tline/voltage/distance from node/.initial=.2}
\ctikzset{bipoles/tline/voltage/bump b/.initial=2.4}
\ctikzset{bipoles/tline/voltage/european label distance/.initial=2.1}
%\ctikzset{bipoles/varistor/voltage/distance from node/.initial=.2}
\ctikzset{bipoles/varistor/voltage/bump b/.initial=2.4}
\ctikzset{bipoles/varistor/voltage/european label distance/.initial=2}
%\ctikzset{bipoles/photoresistor/voltage/distance from node/.initial=.2}
\ctikzset{bipoles/photoresistor/voltage/bump b/.initial=2}
\ctikzset{bipoles/photoresistor/voltage/european label distance/.initial=1.8}
%\ctikzset{bipoles/thermistor/voltage/distance from node/.initial=.2}
\ctikzset{bipoles/thermistor/voltage/bump b/.initial=2.4}
\ctikzset{bipoles/thermistor/voltage/european label distance/.initial=2}
%\ctikzset{bipoles/thermistorntc/voltage/distance from node/.initial=.2}
\ctikzset{bipoles/thermistorntc/voltage/bump b/.initial=1.6}
%\ctikzset{bipoles/thermistorptc/voltage/distance from node/.initial=.2}
\ctikzset{bipoles/thermistorptc/voltage/bump b/.initial=1.6}

\ctikzset{current/.is family}
\ctikzset{current/distance/.initial = .5}

\tikzset{american currents/.style = { \circuitikzbasekey/current = american } }
\tikzset{european currents/.style = { \circuitikzbasekey/current = european } }
\tikzset{american voltages/.style = { \circuitikzbasekey/voltage = american } }
\tikzset{european voltages/.style = { \circuitikzbasekey/voltage = european } }
\tikzset{american resistors/.style = { \circuitikzbasekey/resistor = american } }
\tikzset{european resistors/.style = { \circuitikzbasekey/resistor = european } }

\newif\ifpgf@circuit@europeangfsurgearrester
\ctikzset{gas filled surge arrester/.is choice}
\ctikzset{gas filled surge arrester/european/.code= {\pgf@circuit@europeangfsurgearrestertrue } }
\ctikzset{gas filled surge arrester/american/.code= {\pgf@circuit@europeangfsurgearresterfalse } } 

\tikzset{american gas filled surge arrester/.style = { \circuitikzbasekey/gas filled surge arrester = american } }
\tikzset{european gas filled surge arrester/.style = { \circuitikzbasekey/gas filled surge arrester = european } }
\tikzset{american inductors/.style = { \circuitikzbasekey/inductor = american } }
\tikzset{european inductors/.style = { \circuitikzbasekey/inductor = european } }
\tikzset{cute inductors/.style = { \circuitikzbasekey/inductor = cute } }
\tikzset{full diodes/.style = { \circuitikzbasekey/diode = full } }
\tikzset{empty diodes/.style = { \circuitikzbasekey/diode = empty } }
\tikzset{american ports/.style = { \circuitikzbasekey/logic ports = american } }
\tikzset{european ports/.style = { \circuitikzbasekey/logic ports = european } }
\tikzset{european/.style = { european currents, european voltages, european resistors, european inductors, european ports, european gas filled surge arrester } }
\tikzset{american/.style = { american currents, american voltages, american resistors, american inductors, american ports, american gas filled surge arrester } }
\tikzset{cute/.style = { european currents, european voltages, american resistors, cute inductors, american ports } }

% I should try to make the tree clearer (this voltaege conflicts with the options above)

\newif\ifpgf@circuit@europeanvoltage
\ctikzset{voltage/.is choice}
\ctikzset{voltage/american/.code = {\pgf@circuit@europeanvoltagefalse } }
\ctikzset{voltage/european/.code = {\pgf@circuit@europeanvoltagetrue } }

\newif\ifpgf@circuit@europeancurrent
\ctikzset{current/.is choice}
\ctikzset{current/american/.code = \pgf@circuit@europeancurrentfalse }
\ctikzset{current/european/.code = \pgf@circuit@europeancurrenttrue }

\ctikzset{label/align/.is choice}
\ctikzset{label/align/straight/.code={\ctikzsetvalof{label/align}{straight}}}
\ctikzset{label/align/rotate/.code={\ctikzsetvalof{label/align}{rotate}}}
\ctikzset{label/align/smart/.code={\ctikzsetvalof{label/align}{smart}}}
%% dependencies




%%%%%%%%%% new
\pgfkeys{\circuitikzbasekey/.search also={/tikz}}





%%%%%%%%%%% Springe nach pgfcircutils
%%%---------- open: pgfcircutils.tex
% Copyright 2007-2009 by Massimo Redaelli
%
% This file may be distributed and/or modified
%
% 1. under the LaTeX Project Public License and/or
% 2. under the GNU Public License.
%
% See the file doc/LICENSE for more details.

%\def\pgf@circ@handleSI#1{%
 % \pgf@circ@siunitx@resfalse
%  
 % \edef\len{\stringlength[e]{#1}}
  %\testmatchingchar[e]{#1}{\len}{>}%
  %\ifmatchingchar%
  %  \ifnum\findchars{#1}{<}=0
	%  \def\pgf@circ@handleSI@val{\substring{#1}{1}{\findchars{#1}{<}-1}}
	  %\def\pgf@circ@handleSI@unit{\substring{#1}{\findchars{#1}{<}-1}+1}{\stringlength{#1}}
	  %\pgf@circ@siunitx@restrue
%	\else
%	\fi
  %\else 
  %\fi
%}

\def\pgf@circ@handleSI#1{
	\noexpandarg
        	\def\pgf@temp{}
	\StrBetween{#1}{<}{>}[\pgf@circ@handleSI@unit]
	\StrLen{\pgf@circ@handleSI@unit}[\pgf@circ@handleSI@unit@len]

	\ifnum\pgf@circ@handleSI@unit@len=0  
	  \pgf@circ@siunitx@resfalse  
	\else  
	  \IfEndWith{#1}{>}{
	  	\pgf@circ@siunitx@restrue 
		\noexpandarg
	  	\StrBefore{#1}{<}[\pgf@circ@handleSI@val]		
                %\typeout{si |#1|}
	  }{
	  	\pgf@circ@siunitx@resfalse 
                %\typeout{no si |#1|}
	  }
	\fi
}

\def\pgf@circ@finallabel#1{%
		\edef\pgf@temp{}%
		\edef\pgf@circ@temp{\ctikzvalof{bipole/#1label/unit}}%
		\ifx\pgf@temp\pgf@circ@temp%
			\ctikzvalof{bipole/#1label/name}%
		\else%
			$\SI{\ctikzvalof{bipole/#1label/name}}{\ctikzvalof{bipole/#1label/unit}}$%
		\fi%
}

\def\pgf@circ@ifkeyempty#1{
	\pgfextra{
		\ctikzset{#1/.get=\pgf@circ@temp}
		\edef\pgf@temp{}
	}
	\ifx\pgf@circ@temp\pgf@temp
}


%%%---------- close: pgfcircutils
%%%%%%%%%%% Springe nach pgfcircmath
%%%---------- open: pgfcircmath.tex
% Copyright 2007-2009 by Massimo Redaelli
%
% This file may be distributed and/or modified
%
% 1. under the LaTeX Project Public License and/or
% 2. under the GNU Public License.
%
% See the file doc/LICENSE for more details.

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%%    Math routines

\def\pgf@circ@stripdecimals#1.#2\pgf@nil{#1}

% angle between 0 and 360
\def\pgf@circ@slope#1#2{%
 \pgf@process{#1}%
 \pgf@xa=\pgf@x%
 \pgf@ya=\pgf@y%
 \pgf@process{#2}%
 \advance\pgf@x by-\pgf@xa%
 \advance\pgf@y by-\pgf@ya%
 \ifdim\pgf@x<0.1pt 
 	\ifdim\pgf@x>-0.1pt % vertical
		\ifdim\pgf@y<0pt
			\def\pgfmathresult{-90.0}
		\else
			\def\pgfmathresult{+90.0}
		\fi 	
 	\else % oblique with dx < 0
		\pgfmathdivide{\pgf@y}{\pgf@x}
		\pgfmathatan{\pgfmathresult}
		\ifdim\pgf@x<0pt
			\pgfmathsubtract{\pgfmathresult}{+180}
		\fi
 	\fi
 \else % oblique with dx > 0
	\pgfmathdivide{\pgf@y}{\pgf@x}
	\pgfmathatan{\pgfmathresult}
	\ifdim\pgf@x<0pt
		\pgfmathsubtract{\pgfmathresult}{+180}
	\fi
 \fi
 \pgf@x=\pgfmathresult pt
 \ifdim\pgf@x<0pt
	\pgfmathadd{\pgfmathresult}{+360} 
 \fi
 }

  	
%%%---------- close: pgfcircmath

%%%%%%%%%%% Springe nach pgfcircshapes
%%%---------- open: pgfcircshapes.tex
% Copyright 2007-2009 by Massimo Redaelli
%
% This file may be distributed and/or modified
%
% 1. under the LaTeX Project Public License and/or
% 2. under the GNU Public License.
%
% See the file doc/LICENSE for more details.

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%%  Other shapes


%% Nothing

\pgfdeclareshape{emptyshape}{
	\savedanchor{\northeast}{%
		\pgf@x=.5\wd\pgfnodeparttextbox%
		\pgf@y=.5\ht\pgfnodeparttextbox%
   }
	\anchor{north}{
		\northeast
		\pgf@x=0cm
	}
	\anchor{east}{%
		\northeast
		\pgf@y=0cm
   }
	\anchor{south}{%
		\northeast
		\pgf@y=-\pgf@y
		\pgf@x=0cm
   }
	\anchor{west}{
		\northeast
		\pgf@y=0cm
		\pgf@x=-\pgf@x
	}
	\anchor{text}{%
		\pgfpointorigin
   }
	\anchor{center}{
		\pgfpointorigin
	}
}

%% Full terminal

\pgfdeclareshape{circ}{
	\anchor{center}{
		\pgfpointorigin
	}
	\anchorborder{
		\pgf@circ@res@left=\pgf@x
		\pgf@circ@res@up=\pgf@y
		\pgfpointborderellipse{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}
}{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/nodes width}*\pgfkeysvalueof{/tikz/circuitikz/bipoles/length}}{\pgfkeysvalueof{/tikz/circuitikz/nodes width}*\pgfkeysvalueof{/tikz/circuitikz/bipoles/length}}}		
	}
	\behindforegroundpath{		
		
		\pgfscope
			\pgfpathcircle{\pgfpointorigin}{\pgfkeysvalueof{/tikz/circuitikz/nodes width}*\pgfkeysvalueof{/tikz/circuitikz/bipoles/length}}
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}
			\pgfusepath{draw,fill}		
		\endpgfscope

		}
}

%% Empty terminal

\pgfdeclareshape{ocirc}{
	\anchor{center}{
		\pgfpointorigin
	}
	\anchorborder{
		\pgf@circ@res@left=\pgf@x
		\pgf@circ@res@up=\pgf@y
		\pgfpointborderellipse{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}
}{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/nodes width}*\pgfkeysvalueof{/tikz/circuitikz/bipoles/length}}{\pgfkeysvalueof{/tikz/circuitikz/nodes width}*\pgfkeysvalueof{/tikz/circuitikz/bipoles/length}}}		
	}

	\behindforegroundpath{		
		
		\pgfscope
			\pgfpathcircle{\pgfpointorigin}{\pgfkeysvalueof{/tikz/circuitikz/nodes width}*\pgfkeysvalueof{/tikz/circuitikz/bipoles/length}}
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}
			\pgfsetfillcolor{white}
			\pgfusepath{draw,fill}		
		\endpgfscope

		}
}

%% Current arrow

\pgfdeclareshape{currarrow}{
	\anchor{center}{
		\pgfpointorigin
	}
	\behindforegroundpath{		
		
		\pgfscope
			\pgf@circ@res@step = \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
			\divide \pgf@circ@res@step by 16

			\pgfpathmoveto{\pgfpoint{-.7\pgf@circ@res@step}{0pt}}
			\pgfpathlineto{\pgfpoint{-.7\pgf@circ@res@step}{-.8\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{1\pgf@circ@res@step}{0pt}}
			\pgfpathlineto{\pgfpoint{-.7\pgf@circ@res@step}{.8\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{-.7\pgf@circ@res@step}{0pt}}			
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}
			\pgfusepath{draw,fill}

		\endpgfscope
	}

}

%% Current arrow

\pgfdeclareshape{inputarrow}{
	\savedanchor{\tip}{
		\pgfpointorigin
	}
	\anchor{center}{
		\tip
	}
	\anchor{tip}{
		\tip
	}
	\behindforegroundpath{		
		
		\pgfscope
			\pgf@circ@res@step = \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
			\divide \pgf@circ@res@step by 16

			\pgfpathmoveto{\pgfpoint{-1.7\pgf@circ@res@step}{0pt}}
			\pgfpathlineto{\pgfpoint{-1.7\pgf@circ@res@step}{-.8\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{0pt}{0pt}}
			\pgfpathlineto{\pgfpoint{-1.7\pgf@circ@res@step}{.8\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{-1.7\pgf@circ@res@step}{0pt}}			
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}
			\pgfusepath{fill}

		\endpgfscope
	}

}

%%%---------- close: pgfcircshapes
%%%%%%%%%%% Springe nach pgfcircmonopoles
%%%---------- open: pgfcircmonopoles.tex
% Copyright 2007-2009 by Massimo Redaelli
%
% This file may be distributed and/or modified
%
% 1. under the LaTeX Project Public License and/or
% 2. under the GNU Public License.
%
% See the file doc/LICENSE for more details.

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%% Monopoles

%% Ground symbol

\pgfdeclareshape{ground}{
	\anchor{center}{
		\pgfpointorigin
	}
	\behindforegroundpath{		
		\pgf@circ@res@step=\ctikzvalof{monopoles/ground/width}\pgf@circ@Rlen
		
		\pgfscope		
			\pgfpathmoveto{\pgfpointorigin}
			\pgfpathlineto{\pgfpoint{0pt}{-\pgf@circ@res@step}}
			\pgfusepath{draw}

			\pgfstartlinewidth=\pgflinewidth
			%\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

			\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@step}{-\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{-\pgf@circ@res@step}}
			\pgfusepath{draw}
						
			\pgfsetlinewidth{\pgfstartlinewidth}
			\pgfpathmoveto{\pgfpoint{-.8\pgf@circ@res@step}{-1.2\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{.8\pgf@circ@res@step}{-1.2\pgf@circ@res@step}}
			\pgfpathmoveto{\pgfpoint{-.6\pgf@circ@res@step}{-1.4\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{.6\pgf@circ@res@step}{-1.4\pgf@circ@res@step}}
			\pgfpathmoveto{\pgfpoint{-.4\pgf@circ@res@step}{-1.6\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{.4\pgf@circ@res@step}{-1.6\pgf@circ@res@step}}
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}
			\pgfusepath{draw}
		
			
			\pgfsetlinewidth{\pgfstartlinewidth}
	
		\endpgfscope
	}

}



\pgfdeclareshape{rground}{
	\anchor{center}{
		\pgfpointorigin
	}
	\behindforegroundpath{		
		\pgf@circ@res@step=\ctikzvalof{monopoles/ground/width}\pgf@circ@Rlen
		
		\pgfscope		
			\pgfpathmoveto{\pgfpointorigin}
			\pgfpathlineto{\pgfpoint{0pt}{-\pgf@circ@res@step}}
			\pgfusepath{draw}

			\pgfstartlinewidth=\pgflinewidth
			\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

			\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@step}{-\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{-\pgf@circ@res@step}}
			\pgfusepath{draw}
						
						
			\pgfsetlinewidth{\pgfstartlinewidth}
	
		\endpgfscope
	}
}

\pgfdeclareshape{tground}{
	\anchor{center}{
		\pgfpointorigin
	}
	\behindforegroundpath{		
		\pgf@circ@res@step=\ctikzvalof{monopoles/ground/width}\pgf@circ@Rlen
		
		\pgfscope		
			\pgfpathmoveto{\pgfpointorigin}
			%\pgfpathlineto{\pgfpoint{0pt}{-\pgf@circ@res@step}}
			\pgfusepath{draw}

			\pgfstartlinewidth=\pgflinewidth
			\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/monopoles/tground/thickness}\pgfstartlinewidth}

			\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@step}{0pt}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{0pt}}
			\pgfusepath{draw}
						
						
			\pgfsetlinewidth{\pgfstartlinewidth}
	
		\endpgfscope
	}
}

\pgfdeclareshape{sground}{
	\anchor{center}{
		\pgfpointorigin
	}
	\behindforegroundpath{		
		\pgf@circ@res@step=\ctikzvalof{monopoles/ground/width}\pgf@circ@Rlen
		
		\pgfscope		
			\pgfpathmoveto{\pgfpointorigin}
			\pgfpathlineto{\pgfpoint{0pt}{-\pgf@circ@res@step}}
			\pgfusepath{draw}

			\pgfstartlinewidth=\pgflinewidth
			\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

			\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@step}{-\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{-\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{0}{-1.8\pgf@circ@res@step}}
			\pgfpathclose
			\pgfusepath{draw}
						
						
			\pgfsetlinewidth{\pgfstartlinewidth}
	
		\endpgfscope
	}

}

% noiseless ground
\pgfdeclareshape{nground}{
	\anchor{center}{
		\pgfpointorigin
	}
	\behindforegroundpath{		
		\pgf@circ@res@step=\ctikzvalof{monopoles/ground/width}\pgf@circ@Rlen
		
		\pgfscope		
			\pgfpathmoveto{\pgfpointorigin}
			\pgfpathlineto{\pgfpoint{0pt}{-\pgf@circ@res@step}}
			\pgfusepath{draw}

			\pgfstartlinewidth=\pgflinewidth
			%\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

			\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@step}{-\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{-\pgf@circ@res@step}}
			\pgfusepath{draw}
						
			\pgfsetlinewidth{\pgfstartlinewidth}
			\pgfpathmoveto{\pgfpoint{-.8\pgf@circ@res@step}{-1.2\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{.8\pgf@circ@res@step}{-1.2\pgf@circ@res@step}}
			\pgfpathmoveto{\pgfpoint{-.6\pgf@circ@res@step}{-1.4\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{.6\pgf@circ@res@step}{-1.4\pgf@circ@res@step}}
			\pgfpathmoveto{\pgfpoint{-.4\pgf@circ@res@step}{-1.6\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{.4\pgf@circ@res@step}{-1.6\pgf@circ@res@step}}
			\pgfusepath{draw}
			
			\pgfpathmoveto{\pgfpoint{1.3\pgf@circ@res@step}{-1.6\pgf@circ@res@step}}
			\pgfpatharc{0}{180}{1.3\pgf@circ@res@step}
			\pgfusepath{draw}
					
			\pgfsetlinewidth{\pgfstartlinewidth}
		\endpgfscope
	}
}

% protective ground
\pgfdeclareshape{pground}{
	\anchor{center}{
		\pgfpointorigin
	}
	\behindforegroundpath{		
		\pgf@circ@res@step=\ctikzvalof{monopoles/ground/width}\pgf@circ@Rlen
		
		\pgfscope		
			\pgfpathmoveto{\pgfpointorigin}
			\pgfpathlineto{\pgfpoint{0pt}{-\pgf@circ@res@step}}
			\pgfusepath{draw}

			\pgfstartlinewidth=\pgflinewidth
			%\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

			\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@step}{-\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{-\pgf@circ@res@step}}
			\pgfpathcircle{\pgfpoint{0pt}{-\pgf@circ@res@step}} {1.2\pgf@circ@res@step}
			\pgfusepath{draw}
						
			\pgfsetlinewidth{\pgfstartlinewidth}
			\pgfpathmoveto{\pgfpoint{-.8\pgf@circ@res@step}{-1.2\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{.8\pgf@circ@res@step}{-1.2\pgf@circ@res@step}}
			\pgfpathmoveto{\pgfpoint{-.6\pgf@circ@res@step}{-1.4\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{.6\pgf@circ@res@step}{-1.4\pgf@circ@res@step}}
			\pgfpathmoveto{\pgfpoint{-.4\pgf@circ@res@step}{-1.6\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{.4\pgf@circ@res@step}{-1.6\pgf@circ@res@step}}
			\pgfusepath{draw}
					
			\pgfsetlinewidth{\pgfstartlinewidth}
		\endpgfscope
	}
}

% chassis ground 
\pgfdeclareshape{cground}{ 
\anchor{center}{ 
    \pgfpointorigin 
} 
\behindforegroundpath{       
    \pgf@circ@res@step=\ctikzvalof{monopoles/chassis/width}\pgf@circ@Rlen 
 
    \pgfscope        
        \pgfpathmoveto{\pgfpointorigin} 
        \pgfpathlineto{\pgfpoint{0pt}{-\pgf@circ@res@step}} 
        \pgfusepath{draw}

        \pgfpathmoveto{\pgfpoint{-1.5\pgf@circ@res@step}{-2\pgf@circ@res@step}}
        \pgfpathlineto{\pgfpoint{-\pgf@circ@res@step}{-\pgf@circ@res@step}}
        \pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{-\pgf@circ@res@step}}
        \pgfpathlineto{\pgfpoint{0.5\pgf@circ@res@step}{-2\pgf@circ@res@step}}
        \pgfpathmoveto{\pgfpoint{0pt}{-\pgf@circ@res@step}}
        \pgfpathlineto{\pgfpoint{-0.5\pgf@circ@res@step}{-2\pgf@circ@res@step}}
        \pgfusepath{draw}                        
    \endpgfscope 
    } 
}

% Contributed by Leonardo Azzinnari
\pgfdeclareshape{tlinestub}{
	\anchor{center}{\pgfpointorigin}
	\behindforegroundpath{
		\pgfstartlinewidth=\pgflinewidth
		
		\pgf@circ@res@step=\ctikzvalof{bipoles/tline/width} \pgf@circ@Rlen
        \pgfpathmoveto{\pgfpoint{0.5\pgf@circ@res@step}{0.25\pgf@circ@res@step}}
        
            \pgfpathmoveto{\pgfpointorigin}
            \pgfpathlineto{\pgfpoint{0.5\pgf@circ@res@step}{0pt}}
            \pgfusepath{draw}
         \pgfscope
            \pgfpathellipse{\pgfpoint{0.5\pgf@circ@res@step}{0\pgf@circ@res@step}}{\pgfpoint{0.125\pgf@circ@res@step}{0\pgf@circ@res@step}}{\pgfpoint{0\pgf@circ@res@step}{0.25\pgf@circ@res@step}}
			\pgfpathmoveto{\pgfpoint{0.5\pgf@circ@res@step}{0.25\pgf@circ@res@step}}
            \pgfpathlineto{\pgfpoint{1.5\pgf@circ@res@step}{0.25\pgf@circ@res@step}}
            \pgfpatharc{90}{-90}{0.125\pgf@circ@res@step and 0.25\pgf@circ@res@step}
            \pgfpathlineto{\pgfpoint{0.5\pgf@circ@res@step}{-0.25\pgf@circ@res@step}}
            \pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
            \pgfusepath{draw}
         \endpgfscope
      }
}
                            



\pgfdeclareshape{antenna}{
\anchor{center}{\pgfpointorigin}
	\savedanchor{\northeast}{
		\pgf@circ@res@step=\ctikzvalof{monopoles/antenna/width}\pgf@circ@Rlen
		\pgf@x=5\pgf@circ@res@step%-0.5\pgflinewidth
		\pgf@y=6\pgf@circ@res@step
	}
	\anchor{text}{
		\northeast
		\pgf@x=\ctikzvalof{monopoles/antenna/label/xanchor}\pgf@x
		\pgf@y=\ctikzvalof{monopoles/antenna/label/yanchor}\pgf@y
	}
   \behindforegroundpath{
     \pgfstartlinewidth=\pgflinewidth
     \pgf@circ@res@step=\ctikzvalof{monopoles/antenna/width}\pgf@circ@Rlen
                           
        % \pgfpathmoveto{\pgfpointorigin}
        % \pgfpathlineto{\pgfpoint{4\pgf@circ@res@step}{0pt}}
        % \pgfpathmoveto{\pgfpoint{4\pgf@circ@res@step-0.5\pgflinewidth}{0pt}}
        %     \pgfpathlineto{\pgfpoint{4\pgf@circ@res@step-0.5\pgflinewidth}{6\pgf@circ@res@step}}
        
        \pgftransformxshift{ -4\pgf@circ@res@step }

        \pgfpathmoveto{\pgfpoint{4\pgf@circ@res@step-0.5\pgflinewidth}{0pt}}
        \pgfpathlineto{\pgfpoint{4\pgf@circ@res@step-0.5\pgflinewidth}{6\pgf@circ@res@step}}
             
         \pgfusepath{draw}
             
          \pgfscope   
          \pgfpathmoveto{\pgfpoint{4\pgf@circ@res@step-0.5\pgflinewidth}{6\pgf@circ@res@step}}
             \pgfpathlineto{\pgfpoint{5\pgf@circ@res@step-0.5\pgflinewidth}{6\pgf@circ@res@step}}
             \pgfpathlineto{\pgfpoint{4\pgf@circ@res@step-0.5\pgflinewidth}{4\pgf@circ@res@step}}
             \pgfpathlineto{\pgfpoint{3\pgf@circ@res@step-0.5\pgflinewidth}{6\pgf@circ@res@step}}
             \pgfpathlineto{\pgfpoint{4\pgf@circ@res@step-0.5\pgflinewidth}{6\pgf@circ@res@step}}
             \pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}
             \pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
             \pgfusepath{draw}
           \endpgfscope
                           \pgfsetlinewidth{\pgfstartlinewidth}
                        
                           }
     }


\pgfdeclareshape{txantenna}{
	\anchor{center}{\pgfpointorigin}
	\savedanchor{\northeast}{
		\pgf@circ@res@step=\ctikzvalof{monopoles/txantenna/width}\pgf@circ@Rlen
		\pgf@x=5\pgf@circ@res@step%-0.5\pgflinewidth
		\pgf@y=6\pgf@circ@res@step
	}
	\anchor{text}{
		\northeast
		\pgf@x=\ctikzvalof{monopoles/txantenna/label/xanchor}\pgf@x
		\pgf@y=\ctikzvalof{monopoles/txantenna/label/yanchor}\pgf@y
	}
       \behindforegroundpath{
       \pgfstartlinewidth=\pgflinewidth
       \pgf@circ@res@step=\ctikzvalof{monopoles/txantenna/width}\pgf@circ@Rlen
        
         \pgfpathmoveto{\pgfpointorigin}
         \pgfpathlineto{\pgfpoint{4\pgf@circ@res@step}{0pt}}
         \pgfpathmoveto{\pgfpoint{4\pgf@circ@res@step-0.5\pgflinewidth}{0pt}}
             \pgfpathlineto{\pgfpoint{4\pgf@circ@res@step-0.5\pgflinewidth}{6\pgf@circ@res@step}}
             
         \pgfusepath{draw}
             
          \pgfscope   
          \pgfpathmoveto{\pgfpoint{4\pgf@circ@res@step-0.5\pgflinewidth}{6\pgf@circ@res@step}}
             \pgfpathlineto{\pgfpoint{5\pgf@circ@res@step-0.5\pgflinewidth}{6\pgf@circ@res@step}}
             \pgfpathlineto{\pgfpoint{4\pgf@circ@res@step-0.5\pgflinewidth}{4\pgf@circ@res@step}}
             \pgfpathlineto{\pgfpoint{3\pgf@circ@res@step-0.5\pgflinewidth}{6\pgf@circ@res@step}}
             \pgfpathlineto{\pgfpoint{4\pgf@circ@res@step-0.5\pgflinewidth}{6\pgf@circ@res@step}}
             \pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}
             \pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
             \pgfusepath{draw}
           \endpgfscope
          \pgfpathmoveto{\pgfpoint{5.5\pgf@circ@res@step}{6\pgf@circ@res@step}}
%        \pgfpatharc{60}{-60}{\pgf@circ@res@step and \pgf@circ@res@step}
        \pgfpatharc{30}{-30}{2\pgf@circ@res@step}         \pgfpathmoveto{\pgfpoint{6\pgf@circ@res@step}{6.25\pgf@circ@res@step}}
        \pgfpatharc{30}{-30}{2.5\pgf@circ@res@step}
        \pgfpathmoveto{\pgfpoint{6.5\pgf@circ@res@step}{6.5\pgf@circ@res@step}}
        \pgfpatharc{30}{-30}{3\pgf@circ@res@step}
        \pgfpathmoveto{\pgfpoint{7\pgf@circ@res@step}{6.75\pgf@circ@res@step}}
        \pgfpatharc{30}{-30}{3.5\pgf@circ@res@step}
        \pgfpathmoveto{\pgfpoint{7.5\pgf@circ@res@step}{7\pgf@circ@res@step}}
        \pgfpatharc{30}{-30}{4\pgf@circ@res@step}
        \pgfusepath{draw}
        \pgfsetlinewidth{\pgfstartlinewidth}
        
        }
     }


\pgfdeclareshape{rxantenna}{
	\anchor{center}{\pgfpointorigin}
	\savedanchor{\northeast}{
		\pgf@circ@res@step=\ctikzvalof{monopoles/txantenna/width}\pgf@circ@Rlen
		\pgf@x=5\pgf@circ@res@step%-0.5\pgflinewidth
		\pgf@y=6\pgf@circ@res@step
	}
	\anchor{text}{
		\northeast
		\pgf@x=\ctikzvalof{monopoles/rxantenna/label/xanchor}\pgf@x
		\pgf@y=\ctikzvalof{monopoles/rxantenna/label/yanchor}\pgf@y
	}
    \behindforegroundpath{
        \pgfstartlinewidth=\pgflinewidth
        \pgf@circ@res@step=\ctikzvalof{monopoles/rxantenna/width}\pgf@circ@Rlen
             
         \pgfpathmoveto{\pgfpointorigin}
         \pgfpathlineto{\pgfpoint{4\pgf@circ@res@step}{0pt}}
         \pgfpathmoveto{\pgfpoint{4\pgf@circ@res@step-0.5\pgflinewidth}{0pt}}
             \pgfpathlineto{\pgfpoint{4\pgf@circ@res@step-0.5\pgflinewidth}{6\pgf@circ@res@step}}
             
         \pgfusepath{draw}
             
          \pgfscope   
          \pgfpathmoveto{\pgfpoint{4\pgf@circ@res@step-0.5\pgflinewidth}{6\pgf@circ@res@step}}
             \pgfpathlineto{\pgfpoint{5\pgf@circ@res@step-0.5\pgflinewidth}{6\pgf@circ@res@step}}
             \pgfpathlineto{\pgfpoint{4\pgf@circ@res@step-0.5\pgflinewidth}{4\pgf@circ@res@step}}
             \pgfpathlineto{\pgfpoint{3\pgf@circ@res@step-0.5\pgflinewidth}{6\pgf@circ@res@step}}
             \pgfpathlineto{\pgfpoint{4\pgf@circ@res@step-0.5\pgflinewidth}{6\pgf@circ@res@step}}
             \pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}
             \pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
             \pgfusepath{draw}
           \endpgfscope
           
           \pgfpathmoveto{\pgfpoint{6\pgf@circ@res@step}{7\pgf@circ@res@step}}
%             \pgfpatharc{60}{-60}{\pgf@circ@res@step and \pgf@circ@res@step}
             \pgfpatharc{150}{210}{4\pgf@circ@res@step}              \pgfpathmoveto{\pgfpoint{6.5\pgf@circ@res@step}{6.75\pgf@circ@res@step}}
             \pgfpatharc{150}{210}{3.5\pgf@circ@res@step}
             \pgfpathmoveto{\pgfpoint{7\pgf@circ@res@step}{6.5\pgf@circ@res@step}}
             \pgfpatharc{150}{210}{3\pgf@circ@res@step}
             \pgfpathmoveto{\pgfpoint{7.5\pgf@circ@res@step}{6.25\pgf@circ@res@step}}
             \pgfpatharc{150}{210}{2.5\pgf@circ@res@step}
             \pgfpathmoveto{\pgfpoint{8\pgf@circ@res@step}{6\pgf@circ@res@step}}
             \pgfpatharc{150}{210}{2\pgf@circ@res@step}
             \pgfusepath{draw}
             \pgfsetlinewidth{\pgfstartlinewidth}
             
             }
}

% Vcc
\pgfdeclareshape{vcc}{
	\anchor{center}{
		\pgfpointorigin
	}
	\anchor{text}{
		\pgf@x=0pt
		\pgf@y=\ctikzvalof{monopoles/vcc/width}\pgf@circ@Rlen
		\pgf@y=2\pgf@y
		\advance \pgf@y by 0.5\ht\pgfnodeparttextbox
		\pgf@x=-.5\wd\pgfnodeparttextbox
	}
	\behindforegroundpath{		
		\pgf@circ@res@step=\ctikzvalof{monopoles/vcc/width}\pgf@circ@Rlen
		
		\pgfscope		
			\pgfpathmoveto{\pgfpointorigin}
			\pgfpathlineto{\pgfpoint{0pt}{1.5\pgf@circ@res@step}}
			\pgfusepath{draw}

			\pgfstartlinewidth=\pgflinewidth
			\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

			\pgfpathmoveto{\pgfpoint{-0.5\pgf@circ@res@step}{.8\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{0}{1.5\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{0.5\pgf@circ@res@step}{.8\pgf@circ@res@step}}
			\pgfusepath{draw}
									
			\pgfsetlinewidth{\pgfstartlinewidth}
	
		\endpgfscope
	}

}

% match
\pgfdeclareshape{match}{
	\anchor{center}{
		\pgfpointorigin
	}
	\anchor{text}{
		\pgf@x=\ctikzvalof{monopoles/match/width}\pgf@circ@Rlen
		\pgf@x=1.5\pgf@x
		\advance \pgf@x by -.5\wd\pgfnodeparttextbox
		\pgf@y=-1.5\ht\pgfnodeparttextbox
	}
	\behindforegroundpath{		
		\pgf@circ@res@step=\ctikzvalof{monopoles/match/width}\pgf@circ@Rlen
		
		\pgfscope		
			\pgfpathmoveto{\pgfpointorigin}
			\pgfpathlineto{\pgfpoint{2\pgf@circ@res@step}{0pt}}
			\pgfusepath{draw}

			\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step}{0pt}}
			\pgfpathlineto{\pgfpoint{2\pgf@circ@res@step}{0.5\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpoint{2\pgf@circ@res@step}{0}}
			\pgfusepath{fill}
									
			\pgfsetlinewidth{\pgfstartlinewidth}
	
		\endpgfscope
	}

}

% oscillator
\pgfdeclareshape{oscillator}{
	\anchor{center}{
		\pgfpointorigin
	}
	\anchor{north}{
		\pgf@x=\ctikzvalof{monopoles/oscillator/width}\pgf@circ@Rlen
		\pgf@x=-0.5\pgf@x
		\pgf@y=\ctikzvalof{monopoles/oscillator/width}\pgf@circ@Rlen
		\pgf@y=0.5\pgf@y
	}
	\anchor{south}{
		\pgf@x=\ctikzvalof{monopoles/oscillator/width}\pgf@circ@Rlen
		\pgf@x=-0.5\pgf@x
		\pgf@y=\ctikzvalof{monopoles/oscillator/width}\pgf@circ@Rlen
		\pgf@y=-0.5\pgf@y
	}
	\anchor{east}{
		\pgfpointorigin
		\pgf@x=-\ctikzvalof{monopoles/oscillator/width}\pgf@circ@Rlen
	}
	\anchor{west}{
		\pgfpointorigin
	}
	\anchor{text}{
		\pgf@x=\ctikzvalof{monopoles/oscillator/width}\pgf@circ@Rlen
		\pgf@x=-2\pgf@x
		\advance \pgf@x by -.5\wd\pgfnodeparttextbox
		\pgf@y=-\ctikzvalof{monopoles/oscillator/width}\pgf@circ@Rlen
		\advance \pgf@y by -1.5\ht\pgfnodeparttextbox
	}
	\behindforegroundpath{		
		\pgf@circ@res@step=\ctikzvalof{monopoles/oscillator/width}\pgf@circ@Rlen
		\pgf@circ@res@step=.5\pgf@circ@res@step
		
		\pgfscope		
			\pgfpathmoveto{\pgfpointorigin}
			\pgfstartlinewidth=\pgflinewidth
			
			% draw circle
			\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
			\pgfpathcircle{\pgfpoint{-\pgf@circ@res@step}{0}} {\pgf@circ@res@step}
			\pgfusepath{draw}

			% draw inner sine waves
			\pgfsetdash{}{0pt}	% always draw solid line for inner symbol
			\pgfsetlinewidth{\pgfstartlinewidth}

			\pgfpathmoveto{\pgfpoint{-1.5\pgf@circ@res@step}{0\pgf@circ@res@step}}
			\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
			\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
			\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
			\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
			\pgfusepath{draw}
					
			\pgfsetlinewidth{\pgfstartlinewidth}

		\endpgfscope
	}
}

%%%---------- close: pgfcircmonopoles
%%%%%%%%%%% Springe nach pgfcircbipoles
%%%---------- open: pgfcircbipoles.tex
% Copyright 2007-2009 by Massimo Redaelli
%
% This file may be distributed and/or modified
%
% 1. under the LaTeX Project Public License and/or
% 2. under the GNU Public License.
%
% See the file doc/LICENSE for more details.

%% Generic macro for defining a bipole shape
% #1 - additional anchors
% #2 - lower y-size of the bipole (from the center).
% #3 - #shape is the name of the shape
% #4 - upper y-size of the bipole (from the center)
% #5 - width of the bipole
% #6 - macros drawing the bipole


\long\def\pgfcircdeclarebipole#1#2#3#4#5#6{
	\pgfdeclareshape{#3shape}{
	
	\savedanchor{\northeast}{
		\pgf@y=#4\pgf@circ@Rlen
		\pgf@y=.5\pgf@y
		\pgf@x=#5\pgf@circ@Rlen
		\pgf@x=.5\pgf@x
	}
	\savedanchor{\northeastborder}{
		\pgf@y=#4\pgf@circ@Rlen
		\pgf@y=.5\pgf@y
		\pgf@y=\ctikzvalof{bipoles/border margin}\pgf@y
		\pgf@x=#5\pgf@circ@Rlen
		\pgf@x=.5\pgf@x
		\pgf@x=\ctikzvalof{bipoles/border margin}\pgf@x
	}
	\savedanchor{\southwestborder}{
		\pgf@y=-#2\pgf@circ@Rlen
		\pgf@y=.5\pgf@y
		\pgf@y=\ctikzvalof{bipoles/border margin}\pgf@y
		\pgf@x=-#5\pgf@circ@Rlen
		\pgf@x=.5\pgf@x
		\pgf@x=\ctikzvalof{bipoles/border margin}\pgf@x
	}
	\savedanchor{\southwest}{
		\pgf@y=-#2\pgf@circ@Rlen
		\pgf@y=.5\pgf@y
		\pgf@x=-#5\pgf@circ@Rlen
		\pgf@x=.5\pgf@x
	}
	\savedanchor{\centerpoint}{
		\pgf@circ@res@down=-#2\pgf@circ@Rlen
		\pgf@circ@res@up=#4\pgf@circ@Rlen
		\pgfpointorigin
		\pgf@y=\pgf@circ@res@up
		\advance\pgf@y by\pgf@circ@res@down
		\pgf@y=.5\pgf@y
	}
	\anchor{center}{\pgfpointorigin}
	\anchor{n}{
		\ifpgf@circuit@bipole@reversed\southwest\else\northeast\fi
		\pgf@x=0cm
	}
	\anchor{ne}{
		\ifpgf@circuit@bipole@reversed\southwest\else\northeast\fi
	}
	\anchor{nw}{
		\ifpgf@circuit@bipole@reversed\southwest\else\northeast\fi
		\pgf@x=-\pgf@x
	}
	\anchor{e}{%
		\ifpgf@circuit@bipole@reversed\else\southwest\northeast\fi
		\pgf@y=0cm
   }
	\anchor{s}{%
		\ifpgf@circuit@bipole@reversed\northeast\else\southwest\fi
		\pgf@x=0cm
   }
	\anchor{se}{%
		\ifpgf@circuit@bipole@reversed\northeast\else\southwest\fi
		\pgf@x=-\pgf@x
   }
	\anchor{sw}{%
		\ifpgf@circuit@bipole@reversed\northeast\else\southwest\fi
   }
	\anchor{w}{
		\ifpgf@circuit@bipole@reversed\northeast\else\southwest\fi
		\pgf@y=0cm
	}
	\anchor{north}{
		\ifpgf@circuit@bipole@reversed\southwest\else\northeast\fi
		\pgf@x=0cm
	}
	\anchor{east}{%
		\ifpgf@circuit@bipole@reversed\southwest\else\northeast\fi
		\pgf@y=0cm
   }
	\anchor{south}{%
		\ifpgf@circuit@bipole@reversed\northeast\else\southwest\fi
		\pgf@x=0cm
   }
	\anchor{west}{
		\ifpgf@circuit@bipole@reversed\northeast\else\southwest\fi
		\pgf@y=0cm
	}
	\anchor{right}{
		\ifpgf@circuit@bipole@reversed\southwest\else\northeast\fi
		\pgf@y=0cm
	}
	\anchor{above}{
		\ifpgf@circuit@bipole@reversed\southwest\else\northeast\fi
		\pgf@x=0cm
	}
	\anchor{left}{%
		\ifpgf@circuit@bipole@reversed\northeast\else\southwest\fi
		\pgf@y=0cm
   }
	\anchor{below}{%
		\ifpgf@circuit@bipole@reversed\northeast\else\southwest\fi
		\pgf@x=0cm                    
   }
	\anchor{a}{%
		\ifpgf@circuit@bipole@reversed\southwest\else\northeast\fi
		\pgf@y=0cm
   }
	\anchor{b} {
		\ifpgf@circuit@bipole@reversed\northeast\else\southwest\fi
		\pgf@y=0cm
	}
	\savedanchor{\textanchor}{%
		\pgf@y=\ht\pgfnodeparttextbox
		\pgf@x=-.5\wd\pgfnodeparttextbox
   }
	\anchor{text}{%
		\textanchor
   }
	\anchorborder{%
		\def\pgf@temp{false}
		\ifpgf@circuit@bipole@reversed\pgf@temp
			\pgf@circ@res@left=-\pgf@x
			\pgf@circ@res@right=-\pgf@y
		\else
			\pgf@circ@res@left=\pgf@x
			\pgf@circ@res@right=\pgf@y
		\fi
		\ifdim\pgf@circ@res@right>0cm
			\pgfpointborderrectangle{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@right}}{\northeastborder}
		\else
	  		\southwestborder	
	  	\pgfpointborderrectangle{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@right}}{\pgfpoint{-\pgf@x}{-\pgf@y}}
		\fi
	}
	
	#1
	
	\backgroundpath{	
		\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}	
		
		\northeast
		\pgf@circ@res@up = \pgf@y 
		\pgf@circ@res@zero = 0cm
		\pgf@circ@res@left = -\pgf@x
		\pgf@circ@res@right = \pgf@x
		\southwest
		\pgf@circ@res@down = \pgf@y

 		\pgfstartlinewidth=\pgflinewidth
		
		#6
			
		\pgfsetlinewidth{\pgfstartlinewidth}
	}
	}
}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%% Standard bipole shapes declarations

%% Resistor
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/resistor/height}}{resistor}{\ctikzvalof{bipoles/resistor/height}}{\ctikzvalof{bipoles/resistor/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/resistor/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 12

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgf@circ@res@other = \pgf@circ@res@left
		\advance\pgf@circ@res@other by \pgf@circ@res@step 

		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\pgf@circ@res@up}}
		\advance\pgf@circ@res@other by 2\pgf@circ@res@step 
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\pgf@circ@res@down}}
		\advance\pgf@circ@res@other by 2\pgf@circ@res@step
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\pgf@circ@res@up}}
		\advance\pgf@circ@res@other by 2\pgf@circ@res@step
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\pgf@circ@res@down}}
		\advance\pgf@circ@res@other by 2\pgf@circ@res@step
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\pgf@circ@res@up}}
		\advance\pgf@circ@res@other by 2\pgf@circ@res@step
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\pgf@circ@res@down}}
		\advance\pgf@circ@res@other by \pgf@circ@res@step
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\pgf@circ@res@zero}}
		\pgfusepath{draw} 
}



%% Variable resistor
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/vresistor/height}}{vresistor}{\ctikzvalof{bipoles/vresistor/height}}{\ctikzvalof{bipoles/vresistor/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/vresistor/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 12
		\def\myfrac{.5}

		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgf@circ@res@other = \pgf@circ@res@left
		\advance\pgf@circ@res@other by \pgf@circ@res@step 
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\myfrac\pgf@circ@res@up}}
		\advance\pgf@circ@res@other by 2\pgf@circ@res@step 
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\myfrac\pgf@circ@res@down}}
		\advance\pgf@circ@res@other by 2\pgf@circ@res@step
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\myfrac\pgf@circ@res@up}}
		\advance\pgf@circ@res@other by 2\pgf@circ@res@step
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\myfrac\pgf@circ@res@down}}
		\advance\pgf@circ@res@other by 2\pgf@circ@res@step
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\myfrac\pgf@circ@res@up}}
		\advance\pgf@circ@res@other by 2\pgf@circ@res@step
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\myfrac\pgf@circ@res@down}}
		\advance\pgf@circ@res@other by \pgf@circ@res@step
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@zero}}
		\pgfusepath{draw}
		
		\pgfscope
		\pgfsetarrowsend{latex'}
		\pgfpathmoveto{\pgfpoint{.4\pgf@circ@res@other}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{-.4\pgf@circ@res@other}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		\endpgfscope
}



%% Capacitor

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/capacitor/height}}{capacitor}{\ctikzvalof{bipoles/capacitor/height}}{\ctikzvalof{bipoles/capacitor/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/capacitor/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 5

		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@down}}

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}
}


%% Polar Capacitor

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/pcapacitor/height}}{polarcapacitor}{\ctikzvalof{bipoles/pcapacitor/height}}{\ctikzvalof{bipoles/pcapacitor/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/pcapacitor/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 5

		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
				
		\pgfscope
			\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left+ \ctikzvalof{bipoles/pcapacitor/bend width}\pgf@circ@res@left}{\pgf@circ@res@up}}
			\pgftransformrotate{-90}
			\pgfpathsine{\pgfpoint{\pgf@circ@res@up}{-\ctikzvalof{bipoles/pcapacitor/bend width}\pgf@circ@res@left}}
			\pgfpathcosine{\pgfpoint{\pgf@circ@res@up}{\ctikzvalof{bipoles/pcapacitor/bend width}\pgf@circ@res@left}}
			\pgfusepath{draw}
		\endpgfscope
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		
}

%% Battery

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/battery/height}}{battery}{\ctikzvalof{bipoles/battery/height}}{\ctikzvalof{bipoles/battery/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/battery/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 6

		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{.5\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{.5\pgf@circ@res@down}}

		\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@step}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{-\pgf@circ@res@step}{\pgf@circ@res@down}}

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step}{.5\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{.5\pgf@circ@res@down}}

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}

		\pgfusepath{draw}
}


%% Battery 1

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/battery1/height}}{battery1}{\ctikzvalof{bipoles/battery1/height}}{\ctikzvalof{bipoles/battery1/width}}{
		\pgfpathmoveto{\pgfpoint{.33\pgf@circ@res@right}{0}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{0}}
		\pgfpathmoveto{\pgfpoint{.33\pgf@circ@res@left}{0}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{0}}
		\pgfusepath{draw}

		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathmoveto{\pgfpoint{.33\pgf@circ@res@left}{.5\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{.33\pgf@circ@res@left}{.5\pgf@circ@res@down}}

		\pgfpathmoveto{\pgfpoint{.33\pgf@circ@res@right}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{.33\pgf@circ@res@right}{\pgf@circ@res@down}}
		



		\pgfusepath{draw}
}



%% cute inductor

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/cuteinductor/height}}{cuteinductor}{\ctikzvalof{bipoles/cuteinductor/height}}{\ctikzvalof{bipoles/cuteinductor/width}}{
	\pgf@circ@res@step=\ctikzvalof{bipoles/cuteinductor/width}\pgf@circ@Rlen
	\divide \pgf@circ@res@step by \ctikzvalof{bipoles/cuteinductor/coils}

	\pgfdecorationsegmentamplitude=\ctikzvalof{bipoles/cuteinductor/height}\pgf@circ@Rlen
	\pgfdecorationsegmentamplitude=.5\pgfdecorationsegmentamplitude
	\pgfdecorationsegmentlength = \pgf@circ@res@step
	\pgfdecorationsegmentaspect=.6
	
	\pgfdecoration{{coil}{\pgfdecoratedremainingdistance}}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@zero}}
	\endpgfdecoration
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfusepath{stroke}	
}



%% american inductor

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/americaninductor/height 2}}{americaninductor}{\ctikzvalof{bipoles/americaninductor/height}}{\ctikzvalof{bipoles/americaninductor/width}}{
	\pgf@circ@res@step=\ctikzvalof{bipoles/americaninductor/width}\pgf@circ@Rlen
	\divide \pgf@circ@res@step by \ctikzvalof{bipoles/americaninductor/coils}

	\pgfdecorationsegmentamplitude=\ctikzvalof{bipoles/americaninductor/height}\pgf@circ@Rlen
	\pgfdecorationsegmentamplitude=.45\pgfdecorationsegmentamplitude
	\pgfdecorationsegmentlength = 1.99\pgf@circ@res@step
	
	\pgfdecoration{{bumps}{\pgfdecoratedremainingdistance}}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@zero}}
	\endpgfdecoration
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfusepath{stroke}	
}





%% Independent voltage source

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/vsource/height}}{vsource}{\ctikzvalof{bipoles/vsource/height}}{\ctikzvalof{bipoles/vsource/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

	\pgfpathellipse{\pgfpointorigin}{\pgfpoint{0}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@left}{0}}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@zero}}
	\pgfusepath{draw}
}


%% Independent voltage source - American style

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/vsourceam/height}}{vsourceAM}{\ctikzvalof{bipoles/vsourceam/height}}{\ctikzvalof{bipoles/vsourceam/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

	\pgfpathellipse{\pgfpointorigin}{\pgfpoint{0}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@left}{0}}

	
	\pgftext[bottom,rotate=90,y=\ctikzvalof{bipoles/vsourceam/margin}\pgf@circ@res@down]{$+$}
	\pgftext[top,rotate=90,y=\ctikzvalof{bipoles/vsourceam/margin}\pgf@circ@res@up]{$-$}

	\pgfusepath{draw}
}



%% Independent sinusoidal voltage source

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/vsourcesin/height}}{vsourcesin}{\ctikzvalof{bipoles/vsourcesin/height}}{\ctikzvalof{bipoles/vsourcesin/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfpathellipse{\pgfpointorigin}{\pgfpoint{0}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@left}{0}}
	\pgfusepath{draw}		
		
		\pgf@circ@res@up = .5\pgf@circ@res@up
		\pgfscope
			\pgftransformrotate{90}
			\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@up}{0cm}}
			\pgfpathsine{\pgfpoint{.5\pgf@circ@res@up}{.5\pgf@circ@res@up}}
			\pgfpathcosine{\pgfpoint{.5\pgf@circ@res@up}{-.5\pgf@circ@res@up}}
			\pgfpathsine{\pgfpoint{.5\pgf@circ@res@up}{-.5\pgf@circ@res@up}}
			\pgfpathcosine{\pgfpoint{.5\pgf@circ@res@up}{.5\pgf@circ@res@up}}
			\pgfusepath{draw}
		\endpgfscope
}




% contributed by Alistair Kwan
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/vsourcesquare/height}}{vsourcesquare}{\ctikzvalof{bipoles/vsourcesquare/height}}{\ctikzvalof{bipoles/vsourcesquare/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfpathellipse{\pgfpointorigin}{\pgfpoint{0}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@left}{0}}
	\pgfusepath{draw}		
		
		\pgf@circ@res@up = .5\pgf@circ@res@up
		\pgfscope
			\pgftransformrotate{90}
			\pgfpathmoveto{\pgfpoint{-1\pgf@circ@res@up}{0cm}}
			\pgfpathlineto{\pgfpoint{-1\pgf@circ@res@up}{1\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{0\pgf@circ@res@up}{1\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{0\pgf@circ@res@up}{-1\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{1\pgf@circ@res@up}{-1\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{1\pgf@circ@res@up}{0\pgf@circ@res@up}}
			\pgfusepath{draw}
		\endpgfscope
}


%% Independent current source

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/isource/height}}{isource}{\ctikzvalof{bipoles/isource/height}}{\ctikzvalof{bipoles/isource/width}}{
	\pgfpointorigin
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfpathellipse{\pgfpointorigin}{\pgfpoint{0}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@left}{0}}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step}{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{\pgf@circ@res@down}}
	\pgfusepath{draw}
}




%% Independent current source - American

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/isourceam/height}}{isourceAM}{\ctikzvalof{bipoles/isourceam/height}}{\ctikzvalof{bipoles/isourceam/width}}{
	\pgfpointorigin
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfpathellipse{\pgfpointorigin}{\pgfpoint{0}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@left}{0}}
	\pgfusepath{draw}

	\pgfpathmoveto{\pgfpoint{.7\pgf@circ@res@left}{\pgf@circ@res@zero}}
	\pgfpathlineto{\pgfpoint{.7\pgf@circ@res@right}{\pgf@circ@res@zero}}
	\pgfusepath{draw}
	\pgfscope
		\pgftransformshift{\pgfpoint{.5\pgf@circ@res@right}{\pgf@circ@res@zero}}
		\pgfnode{currarrow}{center}{}{}{\pgfusepath{stroke}}
	\endpgfscope
}




%% Independent sinusoidal current source

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/isource/height}}{isourcesin}{\ctikzvalof{bipoles/isource/height}}{\ctikzvalof{bipoles/isource/width}}{
	\pgfpointorigin
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfpathellipse{\pgfpointorigin}{\pgfpoint{0}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@left}{0}}
	\pgfusepath{draw}
	
		\pgf@circ@res@up = .5\pgf@circ@res@up
		\pgfscope
			\pgftransformrotate{90}
			\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@up}{0cm}}
			\pgfpathsine{\pgfpoint{.5\pgf@circ@res@up}{.5\pgf@circ@res@up}}
			\pgfpathcosine{\pgfpoint{.5\pgf@circ@res@up}{-.5\pgf@circ@res@up}}
			\pgfpathsine{\pgfpoint{.5\pgf@circ@res@up}{-.5\pgf@circ@res@up}}
			\pgfpathcosine{\pgfpoint{.5\pgf@circ@res@up}{.5\pgf@circ@res@up}}
			\pgfusepath{draw}
		\endpgfscope

}


%% Controlled voltage source

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/cvsource/height}}{cvsource}{\ctikzvalof{bipoles/cvsource/height}}{\ctikzvalof{bipoles/cvsource/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

			\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@zero}{\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@zero}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@zero}{\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@zero}}
			\pgfusepath{draw}		
}




%% Controlled voltage source - American

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/cvsourceam/height}}{cvsourceAM}{\ctikzvalof{bipoles/cvsourceam/height}}{\ctikzvalof{bipoles/cvsourceam/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

			\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@zero}{\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@zero}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@zero}{\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
			\pgftext[bottom,rotate=90,y=\ctikzvalof{bipoles/cvsourceam/margin}\pgf@circ@res@left]{$+$}
			\pgftext[top,rotate=90,y=\ctikzvalof{bipoles/cvsourceam/margin}\pgf@circ@res@right]{$-$}
			\pgfusepath{draw}		
}


%% Controlled sinusoidal voltage source

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/cvsourcesin/height}}{cvsourcesin}{\ctikzvalof{bipoles/cvsourcesin/height}}{\ctikzvalof{bipoles/cvsourcesin/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

		\pgfscope
			\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@zero}{\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@zero}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@zero}{\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
			\pgfusepath{draw}		
		\endpgfscope	

		\pgf@circ@res@up = .5\pgf@circ@res@up
		\pgfscope
			\pgftransformrotate{90}
			\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@up}{0cm}}
			\pgfpathsine{\pgfpoint{.5\pgf@circ@res@up}{.5\pgf@circ@res@up}}
			\pgfpathcosine{\pgfpoint{.5\pgf@circ@res@up}{-.5\pgf@circ@res@up}}
			\pgfpathsine{\pgfpoint{.5\pgf@circ@res@up}{-.5\pgf@circ@res@up}}
			\pgfpathcosine{\pgfpoint{.5\pgf@circ@res@up}{.5\pgf@circ@res@up}}
			\pgfusepath{draw}
		\endpgfscope
}



%% Controlled sinusoidal current source

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/cvsourcesin/height}}{cisourcesin}{\ctikzvalof{bipoles/cvsourcesin/height}}{\ctikzvalof{bipoles/cvsourcesin/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

		\pgfscope
			\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@zero}{\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@zero}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@zero}{\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
			\pgfusepath{draw}		
		\endpgfscope	

		\pgf@circ@res@up = .5\pgf@circ@res@up
		\pgfscope
			\pgftransformrotate{90}
			\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@up}{0cm}}
			\pgfpathsine{\pgfpoint{.5\pgf@circ@res@up}{.5\pgf@circ@res@up}}
			\pgfpathcosine{\pgfpoint{.5\pgf@circ@res@up}{-.5\pgf@circ@res@up}}
			\pgfpathsine{\pgfpoint{.5\pgf@circ@res@up}{-.5\pgf@circ@res@up}}
			\pgfpathcosine{\pgfpoint{.5\pgf@circ@res@up}{.5\pgf@circ@res@up}}
			\pgfusepath{draw}
		\endpgfscope
}




%% Controlled current source

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/cisource/height}}{cisource}{\ctikzvalof{bipoles/cisource/height}}{\ctikzvalof{bipoles/cisource/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	
			\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@zero}{\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@zero}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@zero}{\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
			\pgfpathmoveto{\pgfpoint{\pgf@circ@res@zero}{\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@zero}{\pgf@circ@res@down}}
			\pgfusepath{draw}		
}




%% Controlled current source - American

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/cisourceam/height}}{cisourceAM}{\ctikzvalof{bipoles/cisourceam/height}}{\ctikzvalof{bipoles/cisourceam/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	
			\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@zero}{\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@zero}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@zero}{\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
			\pgfusepath{draw}		

	\pgfpathmoveto{\pgfpoint{.7\pgf@circ@res@left}{\pgf@circ@res@zero}}
	\pgfpathlineto{\pgfpoint{.7\pgf@circ@res@right}{\pgf@circ@res@zero}}
	\pgfusepath{draw}
	\pgfscope
		\pgftransformshift{\pgfpoint{.5\pgf@circ@res@right}{\pgf@circ@res@zero}}
		\pgfnode{currarrow}{center}{}{}{\pgfusepath{draw}}
	\endpgfscope
}

%% Black generic diode

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/diode/height}}{fulldiode}{\ctikzvalof{bipoles/diode/height}}{\ctikzvalof{bipoles/diode/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

	\pgfscope
		\pgftransformxshift{\pgf@circ@res@left}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfusepath{draw,fill}
	\endpgfscope
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
		\pgfusepath{draw}
}

%% Black Zener diode

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/diode/height}}{fullzdiode}{\ctikzvalof{bipoles/diode/height}}{\ctikzvalof{bipoles/diode/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

	\pgfscope
		\pgftransformxshift{\pgf@circ@res@left}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfusepath{draw,fill}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-1.2\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfusepath{draw}
	\endpgfscope
}

%% Black Schottky diode

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/diode/height}}{fullsdiode}{\ctikzvalof{bipoles/diode/height}}{\ctikzvalof{bipoles/diode/width}}{
		
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfscope
		\pgftransformxshift{\pgf@circ@res@left}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfusepath{draw,fill}
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-.8\pgf@circ@res@left}{.8\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-.8\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-1.2\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-1.2\pgf@circ@res@left}{.8\pgf@circ@res@up}}
		\pgfusepath{draw}
	\endpgfscope

}

%% Black tunnel diode

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/diode/height}}{fulltdiode}{\ctikzvalof{bipoles/diode/height}}{\ctikzvalof{bipoles/diode/width}}{
		
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfscope
		\pgftransformxshift{\pgf@circ@res@left}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfusepath{draw,fill}

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-.8\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-.8\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfusepath{draw}
	\endpgfscope
}

%% Black light emitting diode

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/diode/height}}{fulllediode}{\ctikzvalof{bipoles/diode/height}}{\ctikzvalof{bipoles/diode/width}}{
		
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfscope
		\pgftransformxshift{\pgf@circ@res@left}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfusepath{draw,fill}
	\endpgfscope
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
		\pgfusepath{draw}

			\pgfsetlinewidth{\pgfstartlinewidth}
			\pgfsetarrowsend{latex'}
			\pgfpathmoveto{\pgfpoint{-0.4\pgf@circ@res@right}{\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{0.6\pgf@circ@res@right}{2\pgf@circ@res@up}}
			\pgfusepath{draw}
			\pgfpathmoveto{\pgfpoint{0.2\pgf@circ@res@right}{0.8\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{1.2\pgf@circ@res@right}{1.8\pgf@circ@res@up}}
			\pgfusepath{draw}

}

%% Black photodiode

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/diode/height}}{fullpdiode}{\ctikzvalof{bipoles/diode/height}}{\ctikzvalof{bipoles/diode/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfscope
		\pgftransformxshift{\pgf@circ@res@left}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfusepath{draw,fill}
	\endpgfscope
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
		\pgfusepath{draw}

			\pgfsetlinewidth{\pgfstartlinewidth}
			\pgfsetarrowsstart{latex'}
			\pgfpathmoveto{\pgfpoint{-0.4\pgf@circ@res@right}{\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{0.6\pgf@circ@res@right}{2\pgf@circ@res@up}}
			\pgfusepath{draw}
			\pgfpathmoveto{\pgfpoint{0.2\pgf@circ@res@right}{0.8\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{1.2\pgf@circ@res@right}{1.8\pgf@circ@res@up}}
			\pgfusepath{draw}
}

%% Black varcap

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/varcap/height}}{fullvarcap}{\ctikzvalof{bipoles/varcap/height}}{\ctikzvalof{bipoles/varcap/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfscope
		\pgftransformxshift{\pgf@circ@res@left}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-.8\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-.8\pgf@circ@res@left}{0pt}}
		\pgfusepath{draw,fill}
	
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-.8\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-.8\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfusepath{draw}
		
	\endpgfscope
}

%% Empty generic diode

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/diode/height}}{emptydiode}{\ctikzvalof{bipoles/diode/height}}{\ctikzvalof{bipoles/diode/width}}{


	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

	\pgfscope
		\pgftransformxshift{\pgf@circ@res@left}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfusepath{draw}
	\endpgfscope
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
		\pgfusepath{draw}
}

%% Empty Zener diode

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/diode/height}}{emptyzdiode}{\ctikzvalof{bipoles/diode/height}}{\ctikzvalof{bipoles/diode/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

	\pgfscope
		\pgftransformxshift{\pgf@circ@res@left}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfusepath{draw}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-1.2\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfusepath{draw}
	\endpgfscope
}

%% Empty Schottky diode

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/diode/height}}{emptysdiode}{\ctikzvalof{bipoles/diode/height}}{\ctikzvalof{bipoles/diode/width}}{
		
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfscope
		\pgftransformxshift{\pgf@circ@res@left}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfusepath{draw}
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-.8\pgf@circ@res@left}{.8\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-.8\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-1.2\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-1.2\pgf@circ@res@left}{.8\pgf@circ@res@up}}
		\pgfusepath{draw}
	\endpgfscope

}

%% Empty tunnel diode

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/diode/height}}{emptytdiode}{\ctikzvalof{bipoles/diode/height}}{\ctikzvalof{bipoles/diode/width}}{
		
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfscope
		\pgftransformxshift{\pgf@circ@res@left}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfusepath{draw}

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-.8\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-.8\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfusepath{draw}
	\endpgfscope
}

%% Empty light emitting diode

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/diode/height}}{emptylediode}{\ctikzvalof{bipoles/diode/height}}{\ctikzvalof{bipoles/diode/width}}{
		
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfscope
		\pgftransformxshift{\pgf@circ@res@left}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfusepath{draw}
	\endpgfscope
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
		\pgfusepath{draw}

			\pgfsetlinewidth{\pgfstartlinewidth}
			\pgfsetarrowsend{latex'}
			\pgfpathmoveto{\pgfpoint{-0.4\pgf@circ@res@right}{\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{0.6\pgf@circ@res@right}{2\pgf@circ@res@up}}
			\pgfusepath{draw}
			\pgfpathmoveto{\pgfpoint{0.2\pgf@circ@res@right}{0.8\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{1.2\pgf@circ@res@right}{1.8\pgf@circ@res@up}}
			\pgfusepath{draw}
}

%% Empty photodiode

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/diode/height}}{emptypdiode}{\ctikzvalof{bipoles/diode/height}}{\ctikzvalof{bipoles/diode/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfscope
		\pgftransformxshift{\pgf@circ@res@left}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{0pt}}
		\pgfusepath{draw}
	\endpgfscope
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
		\pgfusepath{draw}

			\pgfsetlinewidth{\pgfstartlinewidth}
			\pgfsetarrowsstart{latex'}
			\pgfpathmoveto{\pgfpoint{-0.4\pgf@circ@res@right}{\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{0.6\pgf@circ@res@right}{2\pgf@circ@res@up}}
			\pgfusepath{draw}
			\pgfpathmoveto{\pgfpoint{0.2\pgf@circ@res@right}{0.8\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{1.2\pgf@circ@res@right}{1.8\pgf@circ@res@up}}
			\pgfusepath{draw}
}

%% Empty varcap

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/varcap/height}}{emptyvarcap}{\ctikzvalof{bipoles/varcap/height}}{\ctikzvalof{bipoles/varcap/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfscope
		\pgftransformxshift{\pgf@circ@res@left}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-.8\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-.8\pgf@circ@res@left}{0pt}}
		\pgfusepath{draw}
	
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-.8\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-.8\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfusepath{draw}
		
	\endpgfscope
}

%% Closing SPST

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/interr/height 2}}{cspst}{\ctikzvalof{bipoles/interr/height}}{\ctikzvalof{bipoles/interr/width}}{

			\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		
			\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0pt}}
			\pgfpathlineto{\pgfpoint{.6\pgf@circ@res@right}{\pgf@circ@res@up}}
			\pgfpathmoveto{\pgfpoint{.9\pgf@circ@res@left}{.9\pgf@circ@res@up}}
            \pgfpatharc{65}{25}{\pgfkeysvalueof{/tikz/circuitikz/bipoles/interr/width}\pgf@circ@Rlen}
			%\pgfsetarrowsend{latex'}
			\pgfusepath{draw}
			
			\pgfpathmoveto{\pgfpoint{.1\pgf@circ@res@right}{-.25\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{.14\pgf@circ@res@right}{-.35\pgf@circ@res@up}}
            \pgfsetarrowsend{latex'}
			\pgfusepath{draw}	

}

%% Opening SPST

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/interr/height 2}}{ospst}{\ctikzvalof{bipoles/interr/height}}{\ctikzvalof{bipoles/interr/width}}{

			\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		
			\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0pt}}
			\pgfpathlineto{\pgfpoint{.6\pgf@circ@res@right}{\pgf@circ@res@up}}
			\pgfpathmoveto{\pgfpoint{.3\pgf@circ@res@right}{.1\pgf@circ@res@down}}
            \pgfpatharc{15}{50}{\pgfkeysvalueof{/tikz/circuitikz/bipoles/interr/width}\pgf@circ@Rlen}
            %\pgfpathlineto{\pgfpoint{.6\pgf@circ@res@right}{\pgf@circ@res@up}}
			\pgfusepath{draw}
			
			\pgfpathmoveto{\pgfpoint{.85\pgf@circ@res@left}{1.25\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{.87\pgf@circ@res@left}{1.26\pgf@circ@res@up}}
            \pgfsetarrowsend{latex'}
			\pgfusepath{draw}
            

}


%% Push Button

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/pushbutton/height 2}}{pushbutton}{\ctikzvalof{bipoles/pushbutton/height}}{\ctikzvalof{bipoles/pushbutton/width}}{

			%\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
			\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{.5\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{.5\pgf@circ@res@up}}
			\pgfpathmoveto{\pgfpoint{0}{.5\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{0}{\pgf@circ@res@up}}
			\pgfusepath{draw}
			
			\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
			\pgfnode{ocirc}{center}{}{}{\pgfusepath{draw}}
			\pgftransformshift{\pgfpoint{2\pgf@circ@res@right}{0pt}}
			\pgfnode{ocirc}{center}{}{}{\pgfusepath{draw}}
}


%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%

%% Ammeter

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/ammeter/height}}{ammeter}{\ctikzvalof{bipoles/ammeter/height}}{\ctikzvalof{bipoles/ammeter/width}}{
	\def\pgf@circ@temp{right}
	\ifx\tikz@res@label@pos\pgf@circ@temp
		\pgf@circ@res@step=-1.2\pgf@circ@res@up
	\else
		\def\pgf@circ@temp{below}
		\ifx\tikz@res@label@pos\pgf@circ@temp
			\pgf@circ@res@step=-1.2\pgf@circ@res@up
		\else
			\pgf@circ@res@step=1.2\pgf@circ@res@up
		\fi
	\fi

	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}		
	\pgfpointorigin	\pgf@circ@res@other =  \pgf@x  \advance \pgf@circ@res@other by -\pgf@circ@res@up
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\pgf@circ@res@zero}}
	\pgfusepath{draw}

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

		\pgfscope
			\pgfpathcircle{\pgfpointorigin}{.9\pgf@circ@res@up}
			\pgfusepath{draw}		
		\endpgfscope	

	\pgfsetlinewidth{\pgfstartlinewidth}

	\pgfsetarrowsend{latex}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@other}{\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@up}}
	\pgfusepath{draw}
	\pgfsetarrowsend{}

	
	\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@zero}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@zero}}
	\pgfusepath{draw}

	\pgfnode{circle}{center}{\textbf{A}}{}{}
}

%% Voltmeter

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/voltmeter/height}}{voltmeter}{\ctikzvalof{bipoles/voltmeter/height}}{\ctikzvalof{bipoles/voltmeter/width}}{
	\def\pgf@circ@temp{right}
	\ifx\tikz@res@label@pos\pgf@circ@temp
		\pgf@circ@res@step=-1.2\pgf@circ@res@up
	\else
		\def\pgf@circ@temp{below}
		\ifx\tikz@res@label@pos\pgf@circ@temp
			\pgf@circ@res@step=-1.2\pgf@circ@res@up
		\else
			\pgf@circ@res@step=1.2\pgf@circ@res@up
		\fi
	\fi

	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}		
	\pgfpointorigin	\pgf@circ@res@other =  \pgf@x  \advance \pgf@circ@res@other by -\pgf@circ@res@up
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\pgf@circ@res@zero}}
	\pgfusepath{draw}

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

		\pgfscope
			\pgfpathcircle{\pgfpointorigin}{.9\pgf@circ@res@up}
			\pgfusepath{draw}		
		\endpgfscope	

	\pgfsetlinewidth{\pgfstartlinewidth}

	\pgfsetarrowsend{latex}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@other}{\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@up}}
	\pgfusepath{draw}
	\pgfsetarrowsend{}

	
	\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@zero}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@zero}}
	\pgfusepath{draw}

	\pgfnode{circle}{center}{\textbf{V}}{}{}
		
}

%% Short circuit

\pgfcircdeclarebipole{}{0}{short}{0}{0}{ }

%% Open circuit

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/open/height}}{open}{\ctikzvalof{bipoles/open/height}}{\ctikzvalof{bipoles/open/width}}{

}

%% Generic bipole - used as resistor by some (bleah)

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/generic/height}}{generic}{\ctikzvalof{bipoles/generic/height}}{\ctikzvalof{bipoles/generic/width}}{

		%\pgf@circ@res@step = \ctikzvalof{bipoles/resistor/width}\pgf@circ@Rlen
		%\divide \pgf@circ@res@step by 14

		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
					
		\pgfusepath{draw} 
}


%% fuse

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/fuse/height}}{fuse}{\ctikzvalof{bipoles/fuse/height}}{\ctikzvalof{bipoles/fuse/width}}{

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{0}}
		\pgfusepath{draw}
		
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
					
		\pgfusepath{draw} 
}



%% Generic bipole, filled - used as inductor by some (bleah)

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/fullgeneric/height}}{fullgeneric}{\ctikzvalof{bipoles/fullgeneric/height}}{\ctikzvalof{bipoles/fullgeneric/width}}{

		%\pgf@circ@res@step = \ctikzvalof{bipoles/resistor/width}\pgf@circ@Rlen
		%\divide \pgf@circ@res@step by 14

		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
					
		\pgfusepath{draw,fill} 
}


%% Generic asymmetric bipole 

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/ageneric/height}}{ageneric}{\ctikzvalof{bipoles/ageneric/height}}{\ctikzvalof{bipoles/ageneric/width}}{
		%\pgf@circ@res@step = \ctikzvalof{bipoles/resistor/width}\pgf@circ@Rlen
		%\divide \pgf@circ@res@step by 14

		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
					
		\pgfusepath{draw} 

			\pgfpathrectanglecorners{\pgfpoint{.7\pgf@circ@res@right}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
			\pgfusepath{stroke,fill}		
}


%% asymmetric fuse

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/afuse/height}}{afuse}{\ctikzvalof{bipoles/afuse/height}}{\ctikzvalof{bipoles/afuse/width}}{

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{0}}
		\pgfusepath{draw}
		
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
					
		\pgfusepath{draw}
		
		\pgfpathrectanglecorners{\pgfpoint{.7\pgf@circ@res@right}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
			\pgfusepath{stroke,fill}		 
}




%% Memristor

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/memristor/height}}{memristor}{\ctikzvalof{bipoles/memristor/height}}{\ctikzvalof{bipoles/memristor/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/resistor/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 14

		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{.72*\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{.72*\pgf@circ@res@left}{\ctikzvalof{bipoles/memristor/wave height}\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{.35*\pgf@circ@res@left}{\ctikzvalof{bipoles/memristor/wave height}\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{.35*\pgf@circ@res@left}{-\ctikzvalof{bipoles/memristor/wave height}\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{-.05*\pgf@circ@res@left}{-\ctikzvalof{bipoles/memristor/wave height}\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{-.05*\pgf@circ@res@left}{\ctikzvalof{bipoles/memristor/wave height}\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{.42*\pgf@circ@res@right}{\ctikzvalof{bipoles/memristor/wave height}\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{.42*\pgf@circ@res@right}{0pt}}
		\pgfpathlineto{\pgfpoint{.8*\pgf@circ@res@right}{0pt}}
					
		\pgfusepath{draw} 

			\pgfpathrectanglecorners{\pgfpoint{.7\pgf@circ@res@right}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
			\pgfusepath{stroke,fill}		
}




%% Generic empty tunable

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/tgeneric/height}}{tgeneric}{\ctikzvalof{bipoles/tgeneric/height}}{\ctikzvalof{bipoles/tgeneric/width}}{
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{.4\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{.4\pgf@circ@res@down}}
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfusepath{draw}
		
		\pgfscope
		\pgfsetarrowsend{latex'}
		\pgfpathmoveto{\pgfpoint{.5\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{-.5\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		\endpgfscope
}

%% Photoresistor

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/photoresistor/height 2}}{photoresistor}{\ctikzvalof{bipoles/photoresistor/height}}{\ctikzvalof{bipoles/photoresistor/width}}{
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@down}}{\pgfpoint{\pgf@circ@res@right}{-\pgf@circ@res@down}}
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfusepath{draw}
		
		\pgfscope
		\pgfsetarrowsend{latex'}
		\pgfpathmoveto{\pgfpoint{.7\pgf@circ@res@right}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{.3\pgf@circ@res@right}{-1.2\pgf@circ@res@down}}
		\pgfusepath{draw}
		\pgfpathmoveto{\pgfpoint{.45\pgf@circ@res@right}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{.05\pgf@circ@res@right}{-1.2\pgf@circ@res@down}}
		\pgfusepath{draw}
		\endpgfscope
}




%% Thermistor
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/thermistor/height}}{thermistor}{\ctikzvalof{bipoles/thermistor/height}}{\ctikzvalof{bipoles/thermistor/width}}{
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thermistor/main}\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{-\pgfkeysvalueof{/tikz/circuitikz/bipoles/thermistor/main}\pgf@circ@res@up}}
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfusepath{draw}
		
		%\pgfscope
		\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@left}{-\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{.4\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		%\endpgfscope
}


%% Thermistor PTC
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/thermistorptc/height 2}}{thermistorptc}{\ctikzvalof{bipoles/thermistorptc/height}}{\ctikzvalof{bipoles/thermistorptc/width}}{
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thermistorptc/main}\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{-\pgfkeysvalueof{/tikz/circuitikz/bipoles/thermistorptc/main}\pgf@circ@res@up}}
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfusepath{draw}
		
		\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{.4\pgf@circ@res@left}{-\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{-\pgf@circ@res@up}}
		\pgfusepath{draw}
		
		\pgfsetlinewidth{\pgfstartlinewidth}
		\pgftext[top,x=.85\pgf@circ@res@left,y=.75\pgf@circ@res@down]{\tiny$\vartheta$}
		\pgfsetarrowsend{latex'}
		\pgfpathmoveto{\pgfpoint{.62\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{.62\pgf@circ@res@left}{.7\pgf@circ@res@down}}
		\pgfusepath{draw}
		\pgfpathmoveto{\pgfpoint{.45\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{.45\pgf@circ@res@left}{.7\pgf@circ@res@down}}
		\pgfusepath{draw}
}

%% Thermistor NTC
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/thermistorntc/height 2}}{thermistorntc}{\ctikzvalof{bipoles/thermistorntc/height}}{\ctikzvalof{bipoles/thermistorntc/width}}{
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thermistorntc/main}\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{-\pgfkeysvalueof{/tikz/circuitikz/bipoles/thermistorntc/main}\pgf@circ@res@up}}
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfusepath{draw}
		
		\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{.4\pgf@circ@res@left}{-\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{-\pgf@circ@res@up}}
		\pgfusepath{draw}
		
		\pgfsetlinewidth{\pgfstartlinewidth}
		\pgftext[top,x=.85\pgf@circ@res@left,y=.75\pgf@circ@res@down]{\tiny$\vartheta$}
		\pgfsetarrowsend{latex'}
		\pgfpathmoveto{\pgfpoint{.62\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{.62\pgf@circ@res@left}{.7\pgf@circ@res@down}}
		\pgfusepath{draw}
		\pgfpathmoveto{\pgfpoint{.45\pgf@circ@res@left}{.7\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{.45\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfusepath{draw}
}

%% thermocouple
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/thermocouple/height 2}}{thermocouple}{\ctikzvalof{bipoles/thermocouple/height}}{\ctikzvalof{bipoles/thermocouple/width}}{
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{.5\pgf@circ@res@down}}
		\pgfusepath{draw}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{.5\pgf@circ@res@down}}
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathlineto{\pgfpoint{0}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		\pgfsetlinewidth{\pgfstartlinewidth}
		\pgfpathmoveto{\pgfpoint{0}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{.5\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{0}}
		\pgfusepath{draw}
}

%% Varistor
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/varistor/height}}{varistor}{\ctikzvalof{bipoles/varistor/height}}{\ctikzvalof{bipoles/varistor/width}}{
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/bipoles/varistor/main}\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{-\pgfkeysvalueof{/tikz/circuitikz/bipoles/varistor/main}\pgf@circ@res@up}}
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfusepath{draw}
		
		\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@left}{-\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{.4\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		
		\pgftext[top,x=.65\pgf@circ@res@left,y=1.2\pgf@circ@res@down]{{\tiny\textsf{U}}}
}



%% Generic full tunable

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/tfullgeneric/height}}{tfullgeneric}{\ctikzvalof{bipoles/tfullgeneric/height}}{\ctikzvalof{bipoles/tfullgeneric/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/resistor/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 14

		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{.4\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{.4\pgf@circ@res@down}}
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfusepath{draw,fill}
		
		\pgfscope
		\pgfsetarrowsend{latex'}
		\pgfpathmoveto{\pgfpoint{.5\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{-.5\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		\endpgfscope
}


%% Variable Cute Inductor

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/vcuteinductor/height}}{vcuteinductor}{\ctikzvalof{bipoles/vcuteinductor/height}}{\ctikzvalof{bipoles/vcuteinductor/width}}{
	\pgf@circ@res@step=\ctikzvalof{bipoles/vcuteinductor/width}\pgf@circ@Rlen
	\divide \pgf@circ@res@step by \ctikzvalof{bipoles/vcuteinductor/coils}

	\pgfdecorationsegmentamplitude=\ctikzvalof{bipoles/vcuteinductor/coil height}\pgf@circ@Rlen
	\pgfdecorationsegmentamplitude=.5\pgfdecorationsegmentamplitude
	\pgfdecorationsegmentlength = \pgf@circ@res@step
	\pgfdecorationsegmentaspect=.6
	
	\pgfdecoration{{coil}{\pgfdecoratedremainingdistance}}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@zero}}
	\endpgfdecoration
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfusepath{stroke}	
	
		\pgfscope
		\pgfsetarrowsend{latex'}
		\pgfpathmoveto{\pgfpoint{.4\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{-.4\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		\endpgfscope
}


%% variable american inductor

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/vamericaninductor/height 2}}{vamericaninductor}{\ctikzvalof{bipoles/vamericaninductor/height}}{\ctikzvalof{bipoles/vamericaninductor/width}}{
	\pgf@circ@res@step=\ctikzvalof{bipoles/vamericaninductor/width}\pgf@circ@Rlen
	\divide \pgf@circ@res@step by \ctikzvalof{bipoles/vamericaninductor/coils}

	\pgfdecorationsegmentamplitude=\ctikzvalof{bipoles/vamericaninductor/height}\pgf@circ@Rlen
	\pgfdecorationsegmentamplitude=.45\pgfdecorationsegmentamplitude
	\pgfdecorationsegmentamplitude=.45\pgfdecorationsegmentamplitude % per freccia
	\pgfdecorationsegmentlength = 1.99\pgf@circ@res@step
	
	\pgfdecoration{{bumps}{\pgfdecoratedremainingdistance}}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@zero}}
	\endpgfdecoration
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfusepath{stroke}	
	
		\pgfscope
		\pgfsetarrowsend{latex'}
		\pgfpathmoveto{\pgfpoint{.4\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{-.4\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfusepath{draw}
		\endpgfscope
}




%% Variable Capacitor

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/vcapacitor/height}}{vcapacitor}{\ctikzvalof{bipoles/vcapacitor/height}}{\ctikzvalof{bipoles/vcapacitor/width}}{
		%\pgf@circ@res@step = \ctikzvalof{bipoles/vcapacitor/width}\pgf@circ@Rlen
		\pgf@circ@res@step = \ctikzvalof{bipoles/vcapacitor/capacitor width} \pgf@circ@res@right

		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@step}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{-\pgf@circ@res@step}{\pgf@circ@res@down}}

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		
		\pgfscope
		\pgfsetarrowsend{latex'}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		\endpgfscope
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{-\pgf@circ@res@step}{0pt}}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{0pt}}
		\pgfsetlinewidth{\pgfstartlinewidth}
		\pgfusepath{draw}
}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%% Handling of terminals


%% Easily usable styles

\ctikzset{*-/.style =  {\circuitikzbasekey/bipole/nodes/left=full, \circuitikzbasekey/bipole/nodes/right=none}}
\ctikzset{*-o/.style = {\circuitikzbasekey/bipole/nodes/left=full, \circuitikzbasekey/bipole/nodes/right=empty}}
\ctikzset{*-*/.style = {\circuitikzbasekey/bipole/nodes/left=full, \circuitikzbasekey/bipole/nodes/right=full}}
\ctikzset{o-/.style = {\circuitikzbasekey/bipole/nodes/left=empty, \circuitikzbasekey/bipole/nodes/right=none}}
\ctikzset{o-o/.style = {\circuitikzbasekey/bipole/nodes/left=empty, \circuitikzbasekey/bipole/nodes/right=empty}}
\ctikzset{o-*/.style = {\circuitikzbasekey/bipole/nodes/left=empty, \circuitikzbasekey/bipole/nodes/right=full}}
\ctikzset{-o/.style = {\circuitikzbasekey/bipole/nodes/left=none, \circuitikzbasekey/bipole/nodes/right=empty}}
\ctikzset{-*/.style = {\circuitikzbasekey/bipole/nodes/left=none, \circuitikzbasekey/bipole/nodes/right=full}}

\tikzset{reversed/.style = {\circuitikzbasekey/bipole/reversed=true}}


%% The output routine

\def\drawpoles{
	\pgfextra{ \edef\pgf@circ@temp{\ctikzvalof{bipole/nodes/left}} \def\pgf@temp{empty}  }
	\ifx\pgf@temp\pgf@circ@temp 
		{ (\tikztostart) node[ocirc] {} }
	\else 
		\pgfextra{ \def\pgf@temp{full}  }
		\ifx\pgf@temp\pgf@circ@temp
			{ (\tikztostart) node[circ] {} }
		\fi
	\fi
	\pgfextra{ \edef\pgf@circ@temp{\ctikzvalof{bipole/nodes/right}} \def\pgf@temp{empty}  }
	\ifx\pgf@temp\pgf@circ@temp
		{ (\tikztotarget) node[ocirc] {} }
	\else
		\pgfextra{ \def\pgf@temp{full}  }
		\ifx\pgf@temp\pgf@circ@temp
			{ (\tikztotarget) node[circ] {} }
		\fi
	\fi 
}




















%% Lamp

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/lamp/height}}{lamp}{\ctikzvalof{bipoles/lamp/height}}{\ctikzvalof{bipoles/lamp/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

	\pgfpathellipse{\pgfpointorigin}{\pgfpoint{0}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@left}{0}}
	\pgfpathmoveto{\pgfpoint{.7071*\pgf@circ@res@left}{.7071*\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{.7071*\pgf@circ@res@right}{.7071*\pgf@circ@res@down}}
	\pgfpathmoveto{\pgfpoint{.7071*\pgf@circ@res@left}{.7071*\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{.7071*\pgf@circ@res@right}{.7071*\pgf@circ@res@up}}
	\pgfusepath{draw}
}


\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/tline/height}
                        }{tline}{\ctikzvalof{bipoles/tline/height}
                                 }{\ctikzvalof{bipoles/tline/width}
                                   }    
          {
          \pgf@circ@res@step=.2\pgf@circ@res@right % half x axis
          \pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
          \pgfpathellipse{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@step}{0}}
                         {\pgfpoint{\pgf@circ@res@step}{0}}
                         {\pgfpoint{0}{-\pgf@circ@res@up}}
          \pgfpathmoveto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@step}{\pgf@circ@res@up}}
          \pgfpathlineto{\pgfpoint{\pgf@circ@res@left+\pgf@circ@res@step}{\pgf@circ@res@up}}
          \pgfpatharc{-90}{90}{-\pgf@circ@res@step and -\pgf@circ@res@up}
          \pgfpathlineto{\pgfpoint{\pgf@circ@res@right-\pgf@circ@res@step}{\pgf@circ@res@down}}
          \pgfusepath{draw}
}




%% SQUID added by Cor Molenaar 5 March 2010

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/squid/height}}{squid}{\ctikzvalof{bipoles/squid/height}}{\ctikzvalof{bipoles/squid/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

	\pgfpathellipse{\pgfpointorigin}{\pgfpoint{0}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@left}{0}}
	\pgfpathmoveto{\pgfpoint{0.35*\pgf@circ@res@left}{1.35*\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{0.35*\pgf@circ@res@right}{0.65*\pgf@circ@res@up}}
	\pgfpathmoveto{\pgfpoint{0.35*\pgf@circ@res@left}{0.65*\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{0.35*\pgf@circ@res@right}{1.35*\pgf@circ@res@up}}
	\pgfpathmoveto{\pgfpoint{0.35*\pgf@circ@res@left}{1.35*\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{0.35*\pgf@circ@res@right}{0.65*\pgf@circ@res@down}}
	\pgfpathmoveto{\pgfpoint{0.35*\pgf@circ@res@left}{0.65*\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{0.35*\pgf@circ@res@right}{1.35*\pgf@circ@res@down}}

	\pgfusepath{draw}
}



% Generic barrier added by Cor Molenaar 5 March 2010

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/barrier/height}}{barrier}{\ctikzvalof{bipoles/barrier/height}}{\ctikzvalof{bipoles/barrier/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@step}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@step}}
	\pgfpathmoveto{\pgfpoint{0.35*\pgf@circ@res@left}{0.35*\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{0.35*\pgf@circ@res@right}{0.35*\pgf@circ@res@down}}
	\pgfpathmoveto{\pgfpoint{0.35*\pgf@circ@res@left}{0.35*\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{0.35*\pgf@circ@res@right}{0.35*\pgf@circ@res@up}}

	\pgfusepath{draw}
}


% Contributed by Danilo Piazzalunga
 
\pgfdeclareshape{buffer}
	{
	  \anchor{center}{\pgfpointorigin}
	  \savedanchor\northwest{%
		\pgf@y= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/bipoles/buffer/height}\pgf@y
		\pgf@y=.5\pgf@y
		\pgf@x= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/bipoles/buffer/width}\pgf@x
		\pgf@x=.5\pgf@x
	  }
	  \anchor{south}{
		\northwest
		\pgf@y=-\pgf@y
	  }
	  \savedanchor\left{%
	  	\pgf@y=0pt
	  }
	  \anchor{in}{
		\northwest
		\pgf@y=0pt
	  }
	  \anchor{out}{
		\northwest
		\pgf@y=0pt
		\pgf@x=-\pgf@x
	  }
	  
	  \backgroundpath{			
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}	
			
			
			\northwest
			\pgf@circ@res@up = \pgf@y 
			\pgf@circ@res@down = -\pgf@y
			\pgf@circ@res@right = -\pgf@x
			\pgf@circ@res@left = \pgf@x
			
	\pgfscope
		\pgfsetlinewidth{2\pgflinewidth}
		\pgftransformxshift{.7\pgf@circ@res@left}
		\pgf@circ@res@step=\pgf@circ@res@right
		\advance\pgf@circ@res@step by -\pgf@circ@res@left
		\pgf@circ@res@step=.7\pgf@circ@res@step
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step}{0pt}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{0pt}}
		\pgfusepath{draw}
	\endpgfscope
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{.7\pgf@circ@res@left}{0pt}}
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
		\pgfpathlineto{\pgfpoint{.7\pgf@circ@res@right}{0pt}}
	
		\pgfusepath{draw}
	  
	  }
	}





\pgfdeclareshape{plain amp}
	{
	  \anchor{center}{\pgfpointorigin}
	  \savedanchor\northwest{%
		\pgf@y= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/plain amp/height}\pgf@y
		\pgf@y=.5\pgf@y
		\pgf@x= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/plain amp/width}\pgf@x
		\pgf@x=.5\pgf@x
	  }
	  \anchor{south}{
		\northwest
		\pgf@y=-\pgf@y
	  }
	  \savedanchor\left{%
	  	\pgf@y=0pt
	  }
	  \savedanchor\inOne{%
		\pgf@y= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/plain amp/height}\pgf@y
		\pgf@y=.5\pgf@y
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/plain amp/input height}\pgf@y
		\pgf@x= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/plain amp/width}\pgf@x
		\pgf@x=.5\pgf@x
	  }	  
	  \anchor{-}{
		\inOne
	  }
	  \anchor{+}{
		\inOne
		\pgf@y=-\pgf@y
	  }
	  \savedanchor\up{%
		\pgf@y= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/plain amp/height}\pgf@y
		\pgf@y=.5\pgf@y
		\pgf@x= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/plain amp/width}\pgf@x
		\pgf@x=.5\pgf@x
			\pgf@circ@res@up = \pgf@y 
			\pgf@circ@res@right = -\pgf@x
			\pgf@circ@res@left = \pgf@x
	    \pgfpointlineattime{
			\pgfkeysvalueof{/tikz/circuitikz/tripoles/plain amp/up pos}}{
			\pgfpoint{
				\pgfkeysvalueof{/tikz/circuitikz/tripoles/plain amp/port width}\pgf@circ@res@left}
				{\pgf@circ@res@up}}
			{\pgfpoint{.7\pgf@circ@res@right}{0pt}}
	  }
	  \anchor{up}{
		\up
	  }
	  \anchor{down}{
		\up
		\pgf@y=-\pgf@y
	  }
	  \anchor{out}{
		\northwest
		\pgf@y=0pt
		\pgf@x=-\pgf@x
	  }
	  
	  \backgroundpath{			
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}	
			
			
			\northwest
			\pgf@circ@res@up = \pgf@y 
			\pgf@circ@res@down = -\pgf@y
			\pgf@circ@res@right = -\pgf@x
			\pgf@circ@res@left = \pgf@x
			
	\pgfpathmoveto{\pgfpoint
		{\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/plain amp/input height}\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/plain amp/port width}\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/plain amp/input height}\pgf@circ@res@up}}
	

	\pgfpathmoveto{\pgfpoint
		{\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/plain amp/input height}\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/plain amp/port width}\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/plain amp/input height}\pgf@circ@res@down}}
		
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
	\pgfpathlineto{\pgfpoint{.7\pgf@circ@res@right}{0pt}}
	
	\pgfusepath{draw}

						
	\pgfscope
		\pgfsetlinewidth{2\pgflinewidth}
		\pgftransformxshift{.7\pgf@circ@res@left}
		\pgf@circ@res@step=\pgf@circ@res@right
		\advance\pgf@circ@res@step by -\pgf@circ@res@left
		\pgf@circ@res@step=.7\pgf@circ@res@step
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step}{0pt}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{0pt}}
		\pgfusepath{draw}
	\endpgfscope
		
		
	  
	  }
	}
	
%% Generic two port box
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/twoport/height}}{twoport}{\ctikzvalof{bipoles/twoport/height}}{\ctikzvalof{bipoles/twoport/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/twoport/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 2

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgf@circ@res@other = \pgf@circ@res@left
		\advance\pgf@circ@res@other by \pgf@circ@res@step 

		% draw outer box
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		
		\ifpgf@circuit@inputarrow
			{
				\advance \pgf@circ@res@left by -.5\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
				\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfnode{inputarrow}{tip}{}{pgf@inputarrow}{\pgfusepath{fill}}
			}
		\fi
		
		% rotate inner symbol
		\def\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgf@circ@direction\pgf@nil}
		\ifnum \pgfcircmathresult > 45 \ifnum \pgfcircmathresult < 135
			\pgftransformrotate{270}
		\fi\fi
		\ifnum \pgfcircmathresult > 135 \ifnum \pgfcircmathresult < 225
			\pgftransformrotate{180}
		\fi\fi
		\ifnum \pgfcircmathresult > 225 \ifnum \pgfcircmathresult < 315
			\pgftransformrotate{90}
		\fi\fi
		
		% draw inner symbol
		\pgftext[center,x=0,y=0]{\ctikzvalof{bipoles/twoport/text}}
		
}

%% voltage controled oscillator
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/vco/width}}{vco}{\ctikzvalof{bipoles/twoport/width}}{\ctikzvalof{bipoles/vco/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/vco/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 2

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgf@circ@res@other = \pgf@circ@res@left
		\advance\pgf@circ@res@other by \pgf@circ@res@step 
		
		% draw circle
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathcircle{\pgfpoint{0}{0}} {\pgf@circ@res@step}
		\pgfusepath{draw}
		
		\ifpgf@circuit@inputarrow
			{
				\advance \pgf@circ@res@left by -.5\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
				\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfnode{inputarrow}{tip}{}{pgf@inputarrow}{\pgfusepath{fill}}
			}
		\fi

		% rotate inner symbol
		\def\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgf@circ@direction\pgf@nil}
		\ifnum \pgfcircmathresult > 45 \ifnum \pgfcircmathresult < 135
			\pgftransformrotate{270}
		\fi\fi
		\ifnum \pgfcircmathresult > 134 \ifnum \pgfcircmathresult < 225  % 134 degree, because >= 135 is not possible
			\pgftransformrotate{180}
		\fi\fi
		\ifnum \pgfcircmathresult > 224 \ifnum \pgfcircmathresult < 315
			\pgftransformrotate{90}
		\fi\fi
		
		% draw inner sine waves
		\pgfsetdash{}{0pt}	% always draw solid line for inner symbol
		\pgfsetlinewidth{\pgfstartlinewidth}
		\pgfpathmoveto{\pgfpoint{-.5\pgf@circ@res@step}{0\pgf@circ@res@step}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfusepath{draw}
		
}

%% bandpass filter
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/bandpass/width}}{bandpass}{\ctikzvalof{bipoles/bandpass/width}}{\ctikzvalof{bipoles/bandpass/width}}{
		
		\pgf@circ@res@step = \ctikzvalof{bipoles/bandpass/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 2

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgf@circ@res@other = \pgf@circ@res@left
		\advance\pgf@circ@res@other by \pgf@circ@res@step
		
		% draw outer box
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		
		\ifpgf@circuit@inputarrow
			{
				\advance \pgf@circ@res@left by -.5\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
				\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfnode{inputarrow}{tip}{}{pgf@inputarrow}{\pgfusepath{fill}}
			}
		\fi
		
		% rotate inner symbol
		\def\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgf@circ@direction\pgf@nil}
		\ifnum \pgfcircmathresult > 45 \ifnum \pgfcircmathresult < 135
			\pgftransformrotate{270}
		\fi\fi
		\ifnum \pgfcircmathresult > 134 \ifnum \pgfcircmathresult < 225  % 134 degree, because >= 135 is not possible
			\pgftransformrotate{180}
		\fi\fi
		\ifnum \pgfcircmathresult > 224 \ifnum \pgfcircmathresult < 315
			\pgftransformrotate{90}
		\fi\fi
		
		% draw inner symbol
		\pgfsetdash{}{0pt}	% always draw solid line for inner symbol
		\pgfsetlinewidth{\pgfstartlinewidth}
		\pgfpathmoveto{\pgfpoint{-0.5\pgf@circ@res@step}{0.5\pgf@circ@res@step}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfusepath{draw}
		\pgfpathmoveto{\pgfpoint{-0.15\pgf@circ@res@step}{0.35\pgf@circ@res@step}}
		\pgfpathlineto{\pgfpoint{0.15\pgf@circ@res@step}{0.65\pgf@circ@res@step}}
		\pgfusepath{draw}

		\pgfpathmoveto{\pgfpoint{-0.5\pgf@circ@res@step}{0}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfusepath{draw}

		\pgfpathmoveto{\pgfpoint{-0.5\pgf@circ@res@step}{-0.5\pgf@circ@res@step}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfusepath{draw}
		\pgfpathmoveto{\pgfpoint{-0.15\pgf@circ@res@step}{-0.65\pgf@circ@res@step}}
		\pgfpathlineto{\pgfpoint{0.15\pgf@circ@res@step}{-0.35\pgf@circ@res@step}}
		\pgfusepath{draw}
}

%% highpass filter
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/highpass/width}}{highpass}{\ctikzvalof{bipoles/highpass/width}}{\ctikzvalof{bipoles/highpass/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/highpass/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 2

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgf@circ@res@other = \pgf@circ@res@left
		\advance\pgf@circ@res@other by \pgf@circ@res@step 

		% draw outer box
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		
		\ifpgf@circuit@inputarrow
			{
				\advance \pgf@circ@res@left by -.5\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
				\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfnode{inputarrow}{tip}{}{pgf@inputarrow}{\pgfusepath{fill}}
			}
		\fi
		
		% rotate inner symbol
		\def\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgf@circ@direction\pgf@nil}
		\ifnum \pgfcircmathresult > 45 \ifnum \pgfcircmathresult < 135
			\pgftransformrotate{270}
		\fi\fi
		\ifnum \pgfcircmathresult > 134 \ifnum \pgfcircmathresult < 225  % 134 degree, because >= 135 is not possible
			\pgftransformrotate{180}
		\fi\fi
		\ifnum \pgfcircmathresult > 224 \ifnum \pgfcircmathresult < 315
			\pgftransformrotate{90}
		\fi\fi

		% draw inner symbol
		\pgfsetdash{}{0pt}	% always draw solid line for inner symbol
		\pgfsetlinewidth{\pgfstartlinewidth}
		\pgfpathmoveto{\pgfpoint{-0.5\pgf@circ@res@step}{0.5\pgf@circ@res@step}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfusepath{draw}

		\pgfpathmoveto{\pgfpoint{-0.5\pgf@circ@res@step}{0}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfusepath{draw}
		\pgfpathmoveto{\pgfpoint{-0.15\pgf@circ@res@step}{-0.15\pgf@circ@res@step}}
		\pgfpathlineto{\pgfpoint{0.15\pgf@circ@res@step}{0.15\pgf@circ@res@step}}
		\pgfusepath{draw}

		\pgfpathmoveto{\pgfpoint{-0.5\pgf@circ@res@step}{-0.5\pgf@circ@res@step}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfusepath{draw}
		\pgfpathmoveto{\pgfpoint{-0.15\pgf@circ@res@step}{-0.65\pgf@circ@res@step}}
		\pgfpathlineto{\pgfpoint{0.15\pgf@circ@res@step}{-0.35\pgf@circ@res@step}}
		\pgfusepath{draw}
}

%% lowpass filter
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/lowpass/width}}{lowpass}{\ctikzvalof{bipoles/lowpass/width}}{\ctikzvalof{bipoles/lowpass/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/lowpass/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 2

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgf@circ@res@other = \pgf@circ@res@left
		\advance\pgf@circ@res@other by \pgf@circ@res@step 

		% draw outer box
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		
		\ifpgf@circuit@inputarrow
			{
				\advance \pgf@circ@res@left by -.5\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
				\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfnode{inputarrow}{tip}{}{pgf@inputarrow}{\pgfusepath{fill}}
			}
		\fi
		
		% rotate inner symbol
		\def\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgf@circ@direction\pgf@nil}
		\ifnum \pgfcircmathresult > 45 \ifnum \pgfcircmathresult < 135
			\pgftransformrotate{270}
		\fi\fi
		\ifnum \pgfcircmathresult > 134 \ifnum \pgfcircmathresult < 225  % 134 degree, because >= 135 is not possible
			\pgftransformrotate{180}
		\fi\fi
		\ifnum \pgfcircmathresult > 224 \ifnum \pgfcircmathresult < 315
			\pgftransformrotate{90}
		\fi\fi

		% draw inner symbol
		\pgfsetdash{}{0pt}	% always draw solid line for inner symbol
		\pgfsetlinewidth{\pgfstartlinewidth}
		\pgfpathmoveto{\pgfpoint{-0.5\pgf@circ@res@step}{0.5\pgf@circ@res@step}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfusepath{draw}
		\pgfpathmoveto{\pgfpoint{-0.15\pgf@circ@res@step}{0.35\pgf@circ@res@step}}
		\pgfpathlineto{\pgfpoint{0.15\pgf@circ@res@step}{0.65\pgf@circ@res@step}}
		\pgfusepath{draw}

		\pgfpathmoveto{\pgfpoint{-0.5\pgf@circ@res@step}{0}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfusepath{draw}
		\pgfpathmoveto{\pgfpoint{-0.15\pgf@circ@res@step}{-0.15\pgf@circ@res@step}}
		\pgfpathlineto{\pgfpoint{0.15\pgf@circ@res@step}{0.15\pgf@circ@res@step}}
		\pgfusepath{draw}

		\pgfpathmoveto{\pgfpoint{-0.5\pgf@circ@res@step}{-0.5\pgf@circ@res@step}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathsine{\pgfpoint{.25\pgf@circ@res@step}{-.25\pgf@circ@res@step}}
		\pgfpathcosine{\pgfpoint{.25\pgf@circ@res@step}{.25\pgf@circ@res@step}}
		\pgfusepath{draw}
}

%% ADC
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/adc/width}}{adc}{\ctikzvalof{bipoles/adc/width}}{\ctikzvalof{bipoles/adc/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/adc/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 2

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgf@circ@res@other = \pgf@circ@res@left
		\advance\pgf@circ@res@other by \pgf@circ@res@step 

		% draw outer box
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		
		\ifpgf@circuit@inputarrow
			{
				\advance \pgf@circ@res@left by -.5\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
				\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfnode{inputarrow}{tip}{}{pgf@inputarrow}{\pgfusepath{fill}}
			}
		\fi
		
		% rotate inner symbol
		\def\texti{A}
		\def\textii{D}
		\def\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgf@circ@direction\pgf@nil}
		\ifnum \pgfcircmathresult > 45 \ifnum \pgfcircmathresult < 135
			\def\texti{D}
			\def\textii{A}
			\pgftransformrotate{270}
		\fi\fi
		\ifnum \pgfcircmathresult > 134 \ifnum \pgfcircmathresult < 225  % 134 degree, because >= 135 is not possible
			\def\texti{D}
			\def\textii{A}
			\pgftransformrotate{180}
		\fi\fi
		\ifnum \pgfcircmathresult > 225 \ifnum \pgfcircmathresult < 315
			\pgftransformrotate{90}
			\def\texti{A}
			\def\textii{D}
		\fi\fi

		% draw inner symbol					
		\pgfsetlinewidth{\pgfstartlinewidth}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
		\pgfusepath{draw}
		
		\pgftext[center,x=0.45\pgf@circ@res@left,y=0.45\pgf@circ@res@up]{\textsf{\texti}}
		\pgftext[center,x=0.45\pgf@circ@res@right,y=0.45\pgf@circ@res@down]{\textsf{\textii}}
}

%% DAC
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/dac/width}}{dac}{\ctikzvalof{bipoles/dac/width}}{\ctikzvalof{bipoles/dac/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/dac/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 2

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgf@circ@res@other = \pgf@circ@res@left
		\advance\pgf@circ@res@other by \pgf@circ@res@step 

		% draw outer box
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		
		\ifpgf@circuit@inputarrow
			{
				\advance \pgf@circ@res@left by -.5\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
				\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfnode{inputarrow}{tip}{}{pgf@inputarrow}{\pgfusepath{fill}}
			}
		\fi
		
		% rotate inner symbol
		\def\texti{D}
		\def\textii{A}
		\def\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgf@circ@direction\pgf@nil}
		\ifnum \pgfcircmathresult > 45 \ifnum \pgfcircmathresult < 135
			\def\texti{A}
			\def\textii{D}
			\pgftransformrotate{270}
		\fi\fi
		\ifnum \pgfcircmathresult > 134 \ifnum \pgfcircmathresult < 225  % 134 degree, because >= 135 is not possible
			\def\texti{A}
			\def\textii{D}
			\pgftransformrotate{180}
		\fi\fi
		\ifnum \pgfcircmathresult > 225 \ifnum \pgfcircmathresult < 315
			\pgftransformrotate{90}
			\def\texti{D}
			\def\textii{A}
		\fi\fi

		% draw inner symbol					
		\pgfsetlinewidth{\pgfstartlinewidth}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
		\pgfusepath{draw}
		
		\pgftext[center,x=0.45\pgf@circ@res@left,y=0.45\pgf@circ@res@up]{\textsf{\texti}}
		\pgftext[center,x=0.45\pgf@circ@res@right,y=0.45\pgf@circ@res@down]{\textsf{\textii}}
}

%% DSP
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/dsp/width}}{dsp}{\ctikzvalof{bipoles/dsp/width}}{\ctikzvalof{bipoles/dsp/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/dsp/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 2

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgf@circ@res@other = \pgf@circ@res@left
		\advance\pgf@circ@res@other by \pgf@circ@res@step
		
		% draw outer box
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		
		\ifpgf@circuit@inputarrow
			{
				\advance \pgf@circ@res@left by -.5\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
				\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfnode{inputarrow}{tip}{}{pgf@inputarrow}{\pgfusepath{fill}}
			}
		\fi
		
		% rotate inner symbol
		\def\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgf@circ@direction\pgf@nil}
		\ifnum \pgfcircmathresult > 45 \ifnum \pgfcircmathresult < 135
			\pgftransformrotate{270}
		\fi\fi
		\ifnum \pgfcircmathresult > 135 \ifnum \pgfcircmathresult < 225
			\pgftransformrotate{180}
		\fi\fi
		\ifnum \pgfcircmathresult > 225 \ifnum \pgfcircmathresult < 315
			\pgftransformrotate{90}
		\fi\fi

		% draw inner symbol
		\pgftext[center,x=0,y=0]{\textsf{DSP}}
}

%% FFT
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/fft/width}}{fft}{\ctikzvalof{bipoles/fft/width}}{\ctikzvalof{bipoles/fft/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/fft/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 2

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgf@circ@res@other = \pgf@circ@res@left
		\advance\pgf@circ@res@other by \pgf@circ@res@step
		
		% draw outer box
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		
		\ifpgf@circuit@inputarrow
			{
				\advance \pgf@circ@res@left by -.5\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
				\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfnode{inputarrow}{tip}{}{pgf@inputarrow}{\pgfusepath{fill}}
			}
		\fi
		
		% rotate inner symbol
		\def\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgf@circ@direction\pgf@nil}
		\ifnum \pgfcircmathresult > 45 \ifnum \pgfcircmathresult < 135
			\pgftransformrotate{270}
		\fi\fi
		\ifnum \pgfcircmathresult > 135 \ifnum \pgfcircmathresult < 225
			\pgftransformrotate{180}
		\fi\fi
		\ifnum \pgfcircmathresult > 225 \ifnum \pgfcircmathresult < 315
			\pgftransformrotate{90}
		\fi\fi

		% draw inner symbol
		\pgftext[center,x=0,y=0]{\textsf{FFT}}
}

%% Amplifier
\pgfcircdeclarebipole{}{
		%\ifpgf@circuit@box
			\ctikzvalof{bipoles/twoport/width}
		%\else
		%	\ctikzvalof{bipoles/amp/width}
		%\fi
	}{amp}{
		%\ifpgf@circuit@box
			\ctikzvalof{bipoles/twoport/width}
		%\else
		%	\ctikzvalof{bipoles/amp/width}
	%	\fi
	}{
	%	\ifpgf@circuit@box
			\ctikzvalof{bipoles/twoport/width}
	%	\else
	%		\ctikzvalof{bipoles/amp/width}
	%	\fi
	}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/amp/width}\pgf@circ@Rlen


		% draw outer box
		%\ifpgf@circuit@box
		%	\pgfnode{box}{center}{}{pgf@box}{\pgfusepath{draw}}
		%\fi
		% draw outer box
		% draw outer box
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		
		% draw input arrow
		\ifpgf@circuit@inputarrow
			{
				\advance \pgf@circ@res@left by -.5\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
				\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfnode{inputarrow}{tip}{}{pgf@inputarrow}{\pgfusepath{fill}}
			}
		\fi
		
		\pgfsetdash{}{0pt}	% always draw solid line for inner symbol
		\pgfsetlinewidth{\pgfstartlinewidth}
		\pgfpathmoveto{\pgfpoint{0.5\pgf@circ@res@left}{0.75\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0.63\pgf@circ@res@right}{0}}
		\pgfpathlineto{\pgfpoint{0.5\pgf@circ@res@left}{0.75\pgf@circ@res@down}}
		\pgfpathclose
		\pgfusepath{draw}
}


%% variable amplifier
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/vamp/width}}{vamp}{\ctikzvalof{bipoles/vamp/width}}{\ctikzvalof{bipoles/vamp/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/vamp/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 2

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgf@circ@res@other = \pgf@circ@res@left
		\advance\pgf@circ@res@other by \pgf@circ@res@step 

		% draw outer box
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		
		\ifpgf@circuit@inputarrow
			{
				\advance \pgf@circ@res@left by -.5\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
				\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfnode{inputarrow}{tip}{}{pgf@inputarrow}{\pgfusepath{fill}}
			}
		\fi
		
		\pgfsetdash{}{0pt}	% always draw solid line for inner symbol
		\pgfsetlinewidth{\pgfstartlinewidth}
		\pgfpathmoveto{\pgfpoint{0.5\pgf@circ@res@left}{0.75\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0.63\pgf@circ@res@right}{0}}
		\pgfpathlineto{\pgfpoint{0.5\pgf@circ@res@left}{0.75\pgf@circ@res@down}}
		\pgfpathclose
		\pgfusepath{draw}
		
		\pgfsetarrowsend{latex}
		\pgfpathmoveto{\pgfpoint{0.75\pgf@circ@res@left}{0.5\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{0.7\pgf@circ@res@right}{0.7\pgf@circ@res@up}}
		\pgfusepath{draw}
}

%% pi attenuator
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/piattenuator/width}}{piattenuator}{\ctikzvalof{bipoles/piattenuator/width}}{\ctikzvalof{bipoles/piattenuator/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/piattenuator/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 2

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgf@circ@res@other = \pgf@circ@res@left
		\advance\pgf@circ@res@other by \pgf@circ@res@step 

		% draw outer box
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		
		\ifpgf@circuit@inputarrow
			{
				\advance \pgf@circ@res@left by -.5\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
				\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfnode{inputarrow}{tip}{}{pgf@inputarrow}{\pgfusepath{fill}}
			}
		\fi
		
		% rotate inner symbol
		\def\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgf@circ@direction\pgf@nil}
		\ifnum \pgfcircmathresult > 45 \ifnum \pgfcircmathresult < 135
			\pgftransformrotate{270}
		\fi\fi
		\ifnum \pgfcircmathresult > 225 \ifnum \pgfcircmathresult < 315
			\pgftransformrotate{90}
		\fi\fi

		% draw inner symbol
		\pgfsetdash{}{0pt}	% always draw solid line for inner symbol
		\pgfsetlinewidth{\pgfstartlinewidth}
		\pgfpathmoveto{\pgfpoint{0.4\pgf@circ@res@left}{0.4\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{0.4\pgf@circ@res@left}{0.4\pgf@circ@res@up}}
		\pgfusepath{draw}
		\pgfpathmoveto{\pgfpoint{0.4\pgf@circ@res@right}{0.4\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{0.4\pgf@circ@res@right}{0.4\pgf@circ@res@up}}
		\pgfusepath{draw}
		\pgfpathmoveto{\pgfpoint{0.6\pgf@circ@res@left}{0.4\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0.6\pgf@circ@res@right}{0.4\pgf@circ@res@up}}
		\pgfusepath{draw}
}

%% variable pi attenuator
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/vpiattenuator/width}}{vpiattenuator}{\ctikzvalof{bipoles/vpiattenuator/width}}{\ctikzvalof{bipoles/vpiattenuator/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/vpiattenuator/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 2

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgf@circ@res@other = \pgf@circ@res@left
		\advance\pgf@circ@res@other by \pgf@circ@res@step 

		% draw outer box
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		
		\ifpgf@circuit@inputarrow
			{
				\advance \pgf@circ@res@left by -.5\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
				\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfnode{inputarrow}{tip}{}{pgf@inputarrow}{\pgfusepath{fill}}
			}
		\fi
		
		% rotate inner symbol
		\def\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgf@circ@direction\pgf@nil}
		\ifnum \pgfcircmathresult > 45 \ifnum \pgfcircmathresult < 135
			\pgftransformrotate{270}
		\fi\fi
		\ifnum \pgfcircmathresult > 225 \ifnum \pgfcircmathresult < 315
			\pgftransformrotate{90}
		\fi\fi

		% draw inner symbol
		\pgfsetdash{}{0pt}	% always draw solid line for inner symbol
		\pgfsetlinewidth{\pgfstartlinewidth}
		\pgfpathmoveto{\pgfpoint{0.4\pgf@circ@res@left}{0.4\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{0.4\pgf@circ@res@left}{0.4\pgf@circ@res@up}}
		\pgfusepath{draw}
		\pgfpathmoveto{\pgfpoint{0.4\pgf@circ@res@right}{0.4\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{0.4\pgf@circ@res@right}{0.4\pgf@circ@res@up}}
		\pgfusepath{draw}
		\pgfpathmoveto{\pgfpoint{0.6\pgf@circ@res@left}{0.4\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0.6\pgf@circ@res@right}{0.4\pgf@circ@res@up}}
		\pgfusepath{draw}

		\pgfsetarrowsend{latex}
		\pgfpathmoveto{\pgfpoint{0.7\pgf@circ@res@left}{0.5\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{0.7\pgf@circ@res@right}{0.8\pgf@circ@res@up}}
		\pgfusepath{draw}
}

%% T attenuator
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/tattenuator/width}}{tattenuator}{\ctikzvalof{bipoles/tattenuator/width}}{\ctikzvalof{bipoles/tattenuator/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/tattenuator/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 2

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgf@circ@res@other = \pgf@circ@res@left
		\advance\pgf@circ@res@other by \pgf@circ@res@step 

		% draw outer box
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		
		\ifpgf@circuit@inputarrow
			{
				\advance \pgf@circ@res@left by -.5\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
				\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfnode{inputarrow}{tip}{}{pgf@inputarrow}{\pgfusepath{fill}}
			}
		\fi
		
		% rotate inner symbol
		\def\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgf@circ@direction\pgf@nil}
		\ifnum \pgfcircmathresult > 45 \ifnum \pgfcircmathresult < 135
			\pgftransformrotate{270}
		\fi\fi
		\ifnum \pgfcircmathresult > 225 \ifnum \pgfcircmathresult < 315
			\pgftransformrotate{90}
		\fi\fi

		% draw inner symbol
		\pgfsetdash{}{0pt}	% always draw solid line for inner symbol
		\pgfsetlinewidth{\pgfstartlinewidth}
		\pgfpathmoveto{\pgfpoint{0pt}{0.4\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{0pt}{0.4\pgf@circ@res@up}}
		\pgfusepath{draw}
		\pgfpathmoveto{\pgfpoint{0.6\pgf@circ@res@left}{0.4\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0.6\pgf@circ@res@right}{0.4\pgf@circ@res@up}}
		\pgfusepath{draw}
}

%% variable T attenuator
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/vtattenuator/width}}{vtattenuator}{\ctikzvalof{bipoles/vtattenuator/width}}{\ctikzvalof{bipoles/vtattenuator/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/vtattenuator/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 2

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgf@circ@res@other = \pgf@circ@res@left
		\advance\pgf@circ@res@other by \pgf@circ@res@step 

		% draw outer box
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		
		\ifpgf@circuit@inputarrow
			{
				\advance \pgf@circ@res@left by -.5\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
				\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfnode{inputarrow}{tip}{}{pgf@inputarrow}{\pgfusepath{fill}}
			}
		\fi
		
		% rotate inner symbol
		\def\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgf@circ@direction\pgf@nil}
		\ifnum \pgfcircmathresult > 45 \ifnum \pgfcircmathresult < 135
			\pgftransformrotate{270}
		\fi\fi
		\ifnum \pgfcircmathresult > 225 \ifnum \pgfcircmathresult < 315
			\pgftransformrotate{90}
		\fi\fi

		% draw inner symbol
		\pgfsetdash{}{0pt}	% always draw solid line for inner symbol
		\pgfsetlinewidth{\pgfstartlinewidth}
		\pgfpathmoveto{\pgfpoint{0pt}{0.4\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{0pt}{0.4\pgf@circ@res@up}}
		\pgfusepath{draw}
		\pgfpathmoveto{\pgfpoint{0.6\pgf@circ@res@left}{0.4\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0.6\pgf@circ@res@right}{0.4\pgf@circ@res@up}}
		\pgfusepath{draw}
		
		\pgfsetarrowsend{latex}
		\pgfpathmoveto{\pgfpoint{0.7\pgf@circ@res@left}{0.5\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{0.7\pgf@circ@res@right}{0.8\pgf@circ@res@up}}
		\pgfusepath{draw}
}

%% phase shifter
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/phaseshifter/width}}{phaseshifter}{\ctikzvalof{bipoles/phaseshifter/width}}{\ctikzvalof{bipoles/phaseshifter/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/phaseshifter/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 2

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgf@circ@res@other = \pgf@circ@res@left
		\advance\pgf@circ@res@other by \pgf@circ@res@step 

		% draw outer box
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		
		\ifpgf@circuit@inputarrow
			{
				\advance \pgf@circ@res@left by -.5\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
				\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfnode{inputarrow}{tip}{}{pgf@inputarrow}{\pgfusepath{fill}}
			}
		\fi
		
		% rotate inner symbol
		\def\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgf@circ@direction\pgf@nil}
		\ifnum \pgfcircmathresult > 45 \ifnum \pgfcircmathresult < 135
			\pgftransformrotate{270}
		\fi\fi
		\ifnum \pgfcircmathresult > 135 \ifnum \pgfcircmathresult < 225
			\pgftransformrotate{180}
		\fi\fi
		\ifnum \pgfcircmathresult > 225 \ifnum \pgfcircmathresult < 315
			\pgftransformrotate{90}
		\fi\fi
		
		% inner symbol
		\pgftext[center,x=0,y=0]{\Large$\varphi$}
}

%% variable phase shifter
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/phaseshifter/width}}{vphaseshifter}{\ctikzvalof{bipoles/vphaseshifter/width}}{\ctikzvalof{bipoles/vphaseshifter/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/vphaseshifter/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 2

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgf@circ@res@other = \pgf@circ@res@left
		\advance\pgf@circ@res@other by \pgf@circ@res@step 

		% draw outer box
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		
		\ifpgf@circuit@inputarrow
			{
				\advance \pgf@circ@res@left by -.5\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
				\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfnode{inputarrow}{tip}{}{pgf@inputarrow}{\pgfusepath{fill}}
			}
		\fi
		
		% rotate inner symbol
		\def\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgf@circ@direction\pgf@nil}
		\ifnum \pgfcircmathresult > 45 \ifnum \pgfcircmathresult < 135
			\pgftransformrotate{270}
		\fi\fi
		\ifnum \pgfcircmathresult > 135 \ifnum \pgfcircmathresult < 225
			\pgftransformrotate{180}
		\fi\fi
		\ifnum \pgfcircmathresult > 225 \ifnum \pgfcircmathresult < 315
			\pgftransformrotate{90}
		\fi\fi
		
		% inner symbol
		\pgftext[center,x=0,y=0]{\Large$\varphi$}
		
		\pgfsetdash{}{0pt}	% always draw solid line for inner symbol
		\pgfsetlinewidth{\pgfstartlinewidth}
		\pgfsetarrowsend{latex}
		\pgfpathmoveto{\pgfpoint{0.75\pgf@circ@res@left}{0.65\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{0.7\pgf@circ@res@right}{0.65\pgf@circ@res@up}}
		\pgfusepath{draw}
}

%% detector
\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/detector/width}}{detector}{\ctikzvalof{bipoles/detector/width}}{\ctikzvalof{bipoles/detector/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/detector/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 2

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgf@circ@res@other = \pgf@circ@res@left
		\advance\pgf@circ@res@other by \pgf@circ@res@step 

		% draw outer box
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfusepath{draw}
		
		\ifpgf@circuit@inputarrow
			{
				\advance \pgf@circ@res@left by -.5\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth
				\pgftransformshift{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfnode{inputarrow}{tip}{}{pgf@inputarrow}{\pgfusepath{fill}}
			}
		\fi
		
		% draw inner stuff
		\pgfsetlinewidth{0.8\pgfstartlinewidth}
		\pgfpathmoveto{\pgfpoint{0.75\pgf@circ@res@left}{0}}
		\pgfpathlineto{\pgfpoint{0.75\pgf@circ@res@right}{0}}
		\pgfusepath{draw}
		
		\ifpgf@circuit@fulldiode
			\pgfmathparse{2\pgf@circ@res@up / \pgf@circ@Rlen / \ctikzvalof{bipoles/generic/width}}
			\pgftransformscale{\pgfmathresult}
			\pgfnode{fulldiodeshape}{center}{}{pgf@fulldiode}{\pgfusepath{fill}}
		\else
			\pgfmathparse{2\pgf@circ@res@up / \pgf@circ@Rlen / \ctikzvalof{bipoles/resistor/width}}
			\pgftransformscale{\pgfmathresult}
			\pgfnode{emptydiodeshape}{center}{}{pgf@emptydiode}{\pgfusepath{fill}}
		\fi
		
}




%% european gas filled surge arrester

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/european gas filled surge arrester/height}}{european gas filled surge arrester}{\ctikzvalof{bipoles/european gas filled surge arrester/height}}{\ctikzvalof{bipoles/european gas filled surge arrester/width}}{

		%\pgf@circ@res@step = \ctikzvalof{bipoles/resistor/width}\pgf@circ@Rlen
		%\divide \pgf@circ@res@step by 14

		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
					
		\pgfusepath{draw} 
		
		\pgfscope
		\pgfsetarrowsend{latex'}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/bipoles/european gas filled surge arrester/inside}\pgf@circ@res@left}{0pt}}
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}	
				\pgfusepath{draw} 
	
		\endpgfscope
}




%% american gas filled surge arrester

\pgfcircdeclarebipole{}{\ctikzvalof{bipoles/american gas filled surge arrester/height}}{american gas filled surge arrester}{\ctikzvalof{bipoles/american gas filled surge arrester/height}}{\ctikzvalof{bipoles/american gas filled surge arrester/width}}{
	%\def\pgf@circ@temp{right}
	%\ifx\tikz@res@label@pos\pgf@circ@temp
	%	\pgf@circ@res@step=-1.2\pgf@circ@res@up
	%\else
%		\def\pgf@circ@temp{below}
%		\ifx\tikz@res@label@pos\pgf@circ@temp
%			\pgf@circ@res@step=-1.2\pgf@circ@res@up
%		\else
%			\pgf@circ@res@step=1.2\pgf@circ@res@up
%		\fi
%	\fi

	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}		
	\pgfpointorigin	\pgf@circ@res@other =  \pgf@x  \advance \pgf@circ@res@other by -\pgf@circ@res@up
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\pgf@circ@res@zero}}
	\pgfusepath{draw}

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

		\pgfscope
			\pgfpathcircle{\pgfpointorigin}{.9\pgf@circ@res@up}
			\pgfusepath{draw}		
		\endpgfscope	

	\pgfsetlinewidth{\pgfstartlinewidth}


	\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@zero}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@zero}}
	\pgfusepath{draw}

	\pgfnode{circle}{center}{}{}{}
	
	\pgfscope
		\pgfsetarrowsend{latex}
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@zero}}
		\pgfpathlineto{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/bipoles/american gas filled surge arrester/inside}\pgf@circ@res@right}{\pgf@circ@res@zero}}
		\pgfusepath{draw}	
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgfpathlineto{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/bipoles/american gas filled surge arrester/inside}\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgfusepath{draw}	
	\endpgfscope{}
	
	%\pgftransformshift{\pgfpoint{.25\pgf@circ@res@left}{.45\pgf@circ@res@down}}
	%\pgfnode{circ}{center}{}{}{}
	%\pgftransformshift{}
	\pgfcircle{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/bipoles/american gas filled surge arrester/dot x}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/bipoles/american gas filled surge arrester/dot y}\pgf@circ@res@down}}{\pgfkeysvalueof{/tikz/circuitikz/bipoles/american gas filled surge arrester/size}\pgf@circ@res@down}
	\pgfusepath{fill}
}






%%%---------- close: pgfcircbipoles
%%%%%%%%%%% Springe nach pgfcirctripoles
%%%---------- open: pgfcirctripoles.tex
% Copyright 2007-2009 by Massimo Redaelli
%
% This file may be distributed and/or modified
%
% 1. under the LaTeX Project Public License and/or
% 2. under the GNU Public License.
%
% See the file doc/LICENSE for more details.

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%% Tripoles


\pgfdeclareshape{mixer}
{
	\savedanchor\northwest{
		\pgf@y= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/mixer/width}\pgf@y
		\pgf@y=.5\pgf@y
		\pgf@x= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/mixer/width}\pgf@x
		\pgf@x=.5\pgf@x
	}
	\anchor{center}{
		\pgfpointorigin
	}
	\anchor{left}{%
		\northwest
		\pgf@y=0pt
	}
	\anchor{in 1}{
		\northwest
		\pgf@y=0pt
	}
	\anchor{in1}{
		\northwest
		\pgf@y=0pt
	}
	\anchor{in}{
		\northwest
		\pgf@y=0pt
	}	  
	\anchor{in 2}{
		\northwest
		\pgf@y=-\pgf@y
		\pgf@x=0pt
	}
	\anchor{in2}{
		\northwest
		\pgf@y=-\pgf@y
		\pgf@x=0pt
	}
	\anchor{out}{
		\northwest
		\pgf@y=0pt
		\pgf@x=-\pgf@x
	}
	\anchor{center}{
		\pgf@y=0pt
		\pgf@x=0pt
	}
	\anchor{east}{
		\northwest
		\pgf@y=0pt
		\pgf@x=-\pgf@x  
	}
	\anchor{west}{
		\northwest
		\pgf@y=0pt
	}
	\anchor{south}{
		\northwest
		\pgf@x=0pt
		\pgf@y=-\pgf@y
	}
	\anchor{north}{
		\northwest
		\pgf@x=0pt
	}
	\anchor{south west}{
		\northwest
		\pgf@y=-\pgf@y
	}
	\anchor{north east}{
		\northwest
		\pgf@x=-\pgf@x
	}
	\anchor{north west}{
		\northwest
	}
	\anchor{south east}{
		\northwest
		\pgf@x=-\pgf@x
		\pgf@y=-\pgf@y
	}
	\backgroundpath{
		\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}	
			
		\pgf@circ@res@step=\ctikzvalof{tripoles/mixer/width}\pgf@circ@Rlen
			
		\pgfscope
			\pgfstartlinewidth=\pgflinewidth
			
			% draw outer circle
			\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
			\pgfpathcircle{\pgfpoint{0}{0}} {0.5\pgf@circ@res@step}
			\pgfusepath{draw}
			
			% draw inner stuff
			\pgfsetlinewidth{\pgfstartlinewidth}
			\pgfpathmoveto{\pgfpointorigin}
			\pgfpathmoveto{\pgfpointpolar{135}{0.5\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpointpolar{-45}{0.5\pgf@circ@res@step}}
			\pgfpathmoveto{\pgfpointorigin}
			\pgfpathmoveto{\pgfpointpolar{45}{0.5\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpointpolar{-135}{0.5\pgf@circ@res@step}}
			\pgfsetlinewidth{2\pgflinewidth}
			\pgfusepath{draw}
		\endpgfscope				  
	}
}

\pgfdeclareshape{adder}
{
	\savedanchor\northwest{
		\pgf@y= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/adder/width}\pgf@y
		\pgf@y=.5\pgf@y
		\pgf@x= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/adder/width}\pgf@x
		\pgf@x=.5\pgf@x
	}
	\anchor{center}{
		\pgfpointorigin
	}
	\anchor{left}{%
		\northwest
		\pgf@y=0pt
	}
	\anchor{in 1}{
		\northwest
		\pgf@y=0pt
	}
	\anchor{in1}{
		\northwest
		\pgf@y=0pt
	}
	\anchor{in}{
		\northwest
		\pgf@y=0pt
	}	  
	\anchor{in 2}{
		\northwest
		\pgf@y=-\pgf@y
		\pgf@x=0pt
	}
	\anchor{in2}{
		\northwest
		\pgf@y=-\pgf@y
		\pgf@x=0pt
	}
	\anchor{out}{
		\northwest
		\pgf@y=0pt
		\pgf@x=-\pgf@x
	}
	\anchor{center}{
		\pgf@y=0pt
		\pgf@x=0pt
	}
	\anchor{east}{
		\northwest
		\pgf@y=0pt
		\pgf@x=-\pgf@x  
	}
	\anchor{west}{
		\northwest
		\pgf@y=0pt
	}
	\anchor{south}{
		\northwest
		\pgf@x=0pt
		\pgf@y=-\pgf@y
	}
	\anchor{north}{
		\northwest
		\pgf@x=0pt
	}
	\anchor{south west}{
		\northwest
		\pgf@y=-\pgf@y
	}
	\anchor{north east}{
		\northwest
		\pgf@x=-\pgf@x
	}
	\anchor{north west}{
		\northwest
	}
	\anchor{south east}{
		\northwest
		\pgf@x=-\pgf@x
		\pgf@y=-\pgf@y
	}
	\backgroundpath{
		\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}	
			
		\pgf@circ@res@step=\ctikzvalof{tripoles/adder/width}\pgf@circ@Rlen
			
		\pgfscope
			\pgfstartlinewidth=\pgflinewidth
			
			% draw outer circle
			\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
			\pgfpathcircle{\pgfpoint{0}{0}} {0.5\pgf@circ@res@step}
			\pgfusepath{draw}
			
			% draw inner stuff
			\pgfsetlinewidth{\pgfstartlinewidth}
			\pgfpathmoveto{\pgfpointorigin}
			\pgfpathmoveto{\pgfpointpolar{0}{0.3\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpointpolar{180}{0.3\pgf@circ@res@step}}
			\pgfpathmoveto{\pgfpointorigin}
			\pgfpathmoveto{\pgfpointpolar{90}{0.3\pgf@circ@res@step}}
			\pgfpathlineto{\pgfpointpolar{270}{0.3\pgf@circ@res@step}}
			\pgfsetlinewidth{2\pgflinewidth}
			\pgfusepath{draw}
		\endpgfscope				  
	}
}



	\pgfdeclareshape{spdt}
	{
	  \savedanchor\northwest{%
		\pgf@y= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/spdt/height}\pgf@y
		\pgf@y=.5\pgf@y
		\pgf@x= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/spdt/width}\pgf@x
		\pgf@x=.5\pgf@x
	  }
	  \anchor{left}{%
	  	\northwest
	  	\pgf@y=0pt
	  }
	  \anchor{in}{
	  	\northwest
	  	\pgf@y=0pt
	  }	  
	  \anchor{out 1}{
		\northwest
		\pgf@x=-\pgf@x
	  }
	  \anchor{out 2}{
		\northwest
		\pgf@x=-\pgf@x
		\pgf@y=-\pgf@y
	  }
  	  \anchor{center}{
		\pgf@y=0pt
		\pgf@x=0pt
	  }
	  \anchor{east}{
	  	\northwest
		\pgf@y=0pt
	  	\pgf@x=-\pgf@x  
	  }
	  \anchor{west}{
	  	\northwest
		\pgf@y=0pt
	  }
	  \anchor{south}{
		\northwest
		\pgf@x=0pt
		\pgf@y=-\pgf@y
	  }
	  \anchor{north}{
		\northwest
		\pgf@x=0pt
	  }
	  \anchor{south west}{
		\northwest
		\pgf@y=-\pgf@y
	  }
	  \anchor{north east}{
		\northwest
		\pgf@x=-\pgf@x
	  }
	  \anchor{north west}{
		\northwest
	  }
	  \anchor{south east}{
		\northwest
		\pgf@x=-\pgf@x
		\pgf@y=-\pgf@y
	  }	  
	  \backgroundpath{			
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}	
			
			
			\northwest
			\pgf@circ@res@up = \pgf@y 
			\pgf@circ@res@down = -\pgf@y
			\pgf@circ@res@right = -\pgf@x  
			\pgf@circ@res@left = \pgf@x  
			\pgf@circ@res@other = \pgfkeysvalueof{/tikz/circuitikz/tripoles/spdt/margin}\pgf@circ@res@left
			
		
	  	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@up}}
	  	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@down}}
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{0pt}}
		
		\pgfusepath{draw}
		
		\pgfscope
			\pgftransformshift{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@up}}
			\pgfnode{ocirc}{center}{}{spdt1}{\pgfusepath{stroke}}
		\endpgfscope
		\pgfscope
			\pgftransformshift{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@down}}
			\pgfnode{ocirc}{center}{}{}{\pgfusepath{stroke}}
		\endpgfscope
		\pgfscope
			\pgftransformshift{\pgfpoint{\pgf@circ@res@other}{0pt}}
			\pgfnode{ocirc}{center}{}{spdt2}{\pgfusepath{stroke}}
		\endpgfscope
		
		
		\pgfscope
			\pgfpathmoveto{\pgfpointshapeborder{spdt2}{\pgfpointorigin}}
			\pgfpathlineto{
				\pgfpointadd{\pgfpointshapeborder{spdt1}{\pgfpoint{-\pgf@circ@res@other}{-100pt}}}
				{\pgfpoint{-.05\pgf@circ@res@up}{-.05\pgf@circ@res@up}}
			}
			\pgfsetlinewidth{2\pgflinewidth}
			\pgfusepath{draw}
		\endpgfscope
	  }
	}
	
	
	
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%%
%%       Logic ports
%%






\long\def\pgfcircdeclarelogicport#1#2{
	\pgfdeclareshape{american #1 port}
	{
	  \savedanchor\northwest{%
		\pgf@y= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/american #1 port/height}\pgf@y
		\pgf@y=.5\pgf@y
		\pgf@x= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/american #1 port/width}\pgf@x
		\pgf@x=.5\pgf@x
	  }
	  \savedanchor\left{%
	  	\pgf@y=0pt
	  }
	  \savedanchor\inOne{%
		\pgf@y= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/american #1 port/height}\pgf@y
		\pgf@y=.5\pgf@y
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/american #1 port/input height}\pgf@y
		\pgf@x= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/american #1 port/width}\pgf@x
		\pgf@x=.5\pgf@x
	  }	  
	  \anchor{in 1}{
		\inOne
	  }
	  \anchor{in}{
		\inOne
	  }	  
	  \anchor{in 2}{
		\inOne
		\pgf@y=-\pgf@y
	  }
	  \anchor{out}{
		\northwest
		\pgf@y=0pt
		\pgf@x=-\pgf@x
	  }
  	  \anchor{center}{
		\northwest
		\pgf@y=0pt
		\pgf@x=-.8\pgf@x  
	  }
	  \anchor{east}{
	  	\left
	  	\pgf@x=-.8\pgf@x  
	  }
	  \anchor{west}{
	  	\left
	  }
	  \anchor{south}{
		\northwest
		\pgf@x=0pt
		\pgf@y=-\pgf@y
	  }
	  \anchor{north}{
		\northwest
		\pgf@x=0pt
	  }
	  \anchor{south west}{
		\northwest
		\pgf@y=-\pgf@y
	  }
	  \anchor{north east}{
		\northwest
		\pgf@x=-\pgf@x
	  }
	  \anchor{north west}{
		\northwest
	  }
	  \anchor{south east}{
		\northwest
		\pgf@x=-\pgf@x
		\pgf@y=-\pgf@y
	  }	  
	  \backgroundpath{			
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}	
			
			
			\northwest
			\pgf@circ@res@up = \pgf@y 
			\pgf@circ@res@down = -\pgf@y
			\pgf@circ@res@right = -\pgf@x
			\pgf@circ@res@left = \pgf@x
			
			#2
	  
	  }
	}
}


\pgfcircdeclarelogicport{and}{
	\pgfpathmoveto{\pgfpoint
		{\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american and port/input height}\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american and port/port width}\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american and port/input height}\pgf@circ@res@up}}
	
	\pgfpathmoveto{\pgfpoint
		{\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american and port/input height}\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american and port/port width}\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american and port/input height}\pgf@circ@res@down}}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
	\pgfpathlineto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american and port/port width}\pgf@circ@res@right}
		{0pt}}
	
	\pgfusepath{draw}
	
	\pgfsetlinewidth{2\pgflinewidth}
	\pgfpathmoveto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american and port/port width}\pgf@circ@res@left}
		{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american and port/port width}\pgf@circ@res@left}
		{\pgf@circ@res@down}}
	\pgfpathcurveto
		{\pgfpoint{.0\pgf@circ@res@left}{\pgf@circ@res@down}}
		{\pgfpoint
			{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american and port/port width}\pgf@circ@res@right}
			{.5\pgf@circ@res@down}}
		{\pgfpoint
			{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american and port/port width}\pgf@circ@res@right}
			{0pt}}
	\pgfpathcurveto
		{\pgfpoint
			{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american and port/port width}\pgf@circ@res@right}
			{.5\pgf@circ@res@up}}
		{\pgfpoint{.0\pgf@circ@res@left}{\pgf@circ@res@up}}
		{\pgfpoint
			{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american and port/port width}\pgf@circ@res@left}
			{\pgf@circ@res@up}}	
	\pgfusepath{draw}
}



\pgfcircdeclarelogicport{nand}{
	\pgfpathmoveto{\pgfpoint
		{\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nand port/input height}\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nand port/port width}\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nand port/input height}\pgf@circ@res@up}}
	
	\pgfpathmoveto{\pgfpoint
		{\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nand port/input height}\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nand port/port width}\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nand port/input height}\pgf@circ@res@down}}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
	\pgfpathlineto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nand port/port width}\pgf@circ@res@right}
		{0pt}}
	
	\pgfusepath{draw}
	
	\pgfsetlinewidth{2\pgflinewidth}

	\pgf@circ@res@step = \pgfkeysvalueof{/tikz/circuitikz/tripoles/american nand port/circle width}\pgf@circ@res@right
	\pgf@circ@res@other = \pgfkeysvalueof{/tikz/circuitikz/tripoles/american nand port/port width}\pgf@circ@res@right
	
	\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@down}}
	\pgfpathcurveto
		{\pgfpoint{.0\pgf@circ@res@left}{\pgf@circ@res@down}}
		{\pgfpoint{\pgf@circ@res@other-\pgf@circ@res@step}{.5\pgf@circ@res@down}}
		{\pgfpoint{\pgf@circ@res@other-\pgf@circ@res@step}{0pt}}
	\pgfpathcurveto
		{\pgfpoint{\pgf@circ@res@other-\pgf@circ@res@step}{.5\pgf@circ@res@up}}
		{\pgfpoint{.0\pgf@circ@res@left}{\pgf@circ@res@up}}
		{\pgfpoint
			{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nand port/port width}\pgf@circ@res@left}
			{\pgf@circ@res@up}}	
	\pgfpathellipse
		{\pgfpoint{\pgf@circ@res@other-.5\pgf@circ@res@step}{0pt}}
		{\pgfpoint{.5\pgf@circ@res@step}{0pt}}
		{\pgfpoint{0pt}{.5\pgf@circ@res@step}}

	\pgfusepath{draw}
}


\pgfcircdeclarelogicport{nor}{
	\pgfpathmoveto{\pgfpoint
		{\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/input height}\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint
		{(\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/port width}-\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/input skip})*\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/input height}\pgf@circ@res@up}}
	
	\pgfpathmoveto{\pgfpoint
		{\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/input height}\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint
		{(\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/port width}-\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/input skip})*\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/input height}\pgf@circ@res@down}}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
	\pgfpathlineto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/port width}\pgf@circ@res@right}
		{0pt}}	
	
	\pgfusepath{draw}
	
	\pgf@circ@res@other=\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/port width}\pgf@circ@res@right
	\pgf@circ@res@step = \pgfkeysvalueof{/tikz/circuitikz/tripoles/american nand port/circle width}\pgf@circ@res@right
		
	\pgfsetlinewidth{2\pgflinewidth}
	\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@up}}
	\pgfpathcurveto
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/aaa}\pgf@circ@res@left}{\pgf@circ@res@up}}
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/bbb}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/ccc}\pgf@circ@res@up}}
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/bbb}\pgf@circ@res@left}{0pt}}
	\pgfpathcurveto
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/bbb}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/ccc}\pgf@circ@res@down}}
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/aaa}\pgf@circ@res@left}{\pgf@circ@res@down}}
		{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@down}}	

	\pgfpathcurveto
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/ddd}\pgf@circ@res@left}{\pgf@circ@res@down}}
		{\pgfpoint{\pgf@circ@res@other-\pgf@circ@res@step}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/ccc}\pgf@circ@res@down}}
		{\pgfpoint{\pgf@circ@res@other-\pgf@circ@res@step}{0pt}}
	\pgfpathcurveto
		{\pgfpoint{\pgf@circ@res@other-\pgf@circ@res@step}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/ccc}\pgf@circ@res@up}}
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american nor port/ddd}\pgf@circ@res@left}{\pgf@circ@res@up}}
		{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@up}}	
		
	\pgfpathellipse
		{\pgfpoint{\pgf@circ@res@other-.5\pgf@circ@res@step}{0pt}}
		{\pgfpoint{.5\pgf@circ@res@step}{0pt}}
		{\pgfpoint{0pt}{.5\pgf@circ@res@step}}
		
	\pgfusepath{draw}
}




\pgfcircdeclarelogicport{or}{

	
	\pgfpathmoveto{\pgfpoint
		{\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/input height}\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint
		{(\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/port width}-\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/input skip})*\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/input height}\pgf@circ@res@up}}
	
	\pgfpathmoveto{\pgfpoint
		{\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/input height}\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint
		{(\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/port width}-\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/input skip})*\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/input height}\pgf@circ@res@down}}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
	\pgfpathlineto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/port width}\pgf@circ@res@right}
		{0pt}}	
	
	\pgfusepath{draw}
	\pgf@circ@res@other=\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/port width}\pgf@circ@res@right
	\pgfsetlinewidth{2\pgflinewidth}
	\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@up}}
	\pgfpathcurveto
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/aaa}\pgf@circ@res@left}{\pgf@circ@res@up}}
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/bbb}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/ccc}\pgf@circ@res@up}}
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/bbb}\pgf@circ@res@left}{0pt}}
	\pgfpathcurveto
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/bbb}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/ccc}\pgf@circ@res@down}}
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/aaa}\pgf@circ@res@left}{\pgf@circ@res@down}}
		{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@down}}	

	\pgfpathcurveto
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/ddd}\pgf@circ@res@left}{\pgf@circ@res@down}}
		{\pgfpoint{\pgf@circ@res@other}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/ccc}\pgf@circ@res@down}}
		{\pgfpoint{\pgf@circ@res@other}{0pt}}
	\pgfpathcurveto
		{\pgfpoint{\pgf@circ@res@other}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/ccc}\pgf@circ@res@up}}
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american or port/ddd}\pgf@circ@res@left}{\pgf@circ@res@up}}
		{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@up}}	
	\pgfusepath{draw}
}


\pgfcircdeclarelogicport{xor}{

	\pgfpathmoveto{\pgfpoint
		{\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/input height}\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint
		{(\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/port width}-\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/input skip})*\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/input height}\pgf@circ@res@up}}
	
	\pgfpathmoveto{\pgfpoint
		{\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/input height}\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint
		{(\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/port width}-\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/input skip})*\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/input height}\pgf@circ@res@down}}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
	\pgfpathlineto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/port width}\pgf@circ@res@right}
		{0pt}}	
	
	\pgfusepath{draw}
	\pgf@circ@res@other=\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/port width}\pgf@circ@res@right
	\pgfsetlinewidth{2\pgflinewidth}
	\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@up}}
	\pgfpathcurveto
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/aaa}\pgf@circ@res@left}{\pgf@circ@res@up}}
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/bbb}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/ccc}\pgf@circ@res@up}}
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/bbb}\pgf@circ@res@left}{0pt}}
	\pgfpathcurveto
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/bbb}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/ccc}\pgf@circ@res@down}}
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/aaa}\pgf@circ@res@left}{\pgf@circ@res@down}}
		{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@down}}	

	\pgfpathcurveto
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/ddd}\pgf@circ@res@left}{\pgf@circ@res@down}}
		{\pgfpoint{\pgf@circ@res@other}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/ccc}\pgf@circ@res@down}}
		{\pgfpoint{\pgf@circ@res@other}{0pt}}
	\pgfpathcurveto
		{\pgfpoint{\pgf@circ@res@other}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/ccc}\pgf@circ@res@up}}
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/ddd}\pgf@circ@res@left}{\pgf@circ@res@up}}
		{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@up}}	
		
	\def\pgf@circ@temp{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/distance}\pgf@circ@res@right+}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@temp-\pgf@circ@res@other}{\pgf@circ@res@up}}
	
	\pgfpathcurveto
		{\pgfpoint{\pgf@circ@temp\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/aaa}\pgf@circ@res@left}{.95*\pgf@circ@res@up}}
		{\pgfpoint{\pgf@circ@temp\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/bbb}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/ccc}\pgf@circ@res@up}}
		{\pgfpoint{\pgf@circ@temp\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/bbb}\pgf@circ@res@left}{0pt}}
	\pgfpathcurveto
		{\pgfpoint{\pgf@circ@temp\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/bbb}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/ccc}\pgf@circ@res@down}}
		{\pgfpoint{\pgf@circ@temp\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xor port/aaa}\pgf@circ@res@left}{.95*\pgf@circ@res@down}}
		{\pgfpoint{\pgf@circ@temp-\pgf@circ@res@other}{.95*\pgf@circ@res@down}}	
				
	\pgfusepath{draw}
}



\pgfcircdeclarelogicport{xnor}{

	\pgfpathmoveto{\pgfpoint
		{\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/input height}\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint
		{(\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/port width}-\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/input skip})*\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/input height}\pgf@circ@res@up}}
	
	\pgfpathmoveto{\pgfpoint
		{\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/input height}\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint
		{(\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/port width}-\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/input skip})*\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/input height}\pgf@circ@res@down}}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
	\pgfpathlineto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/port width}\pgf@circ@res@right}
		{0pt}}	
	
	\pgfusepath{draw}
	\pgf@circ@res@other=\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/port width}\pgf@circ@res@right
	\pgf@circ@res@step = \pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/circle width}\pgf@circ@res@right

	\pgfsetlinewidth{2\pgflinewidth}
	\pgfpathmoveto{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@up}}
	\pgfpathcurveto
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/aaa}\pgf@circ@res@left}{\pgf@circ@res@up}}
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/bbb}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/ccc}\pgf@circ@res@up}}
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/bbb}\pgf@circ@res@left}{0pt}}
	\pgfpathcurveto
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/bbb}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/ccc}\pgf@circ@res@down}}
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/aaa}\pgf@circ@res@left}{\pgf@circ@res@down}}
		{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@down}}	

	\pgfpathcurveto
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/ddd}\pgf@circ@res@left}{\pgf@circ@res@down}}
		{\pgfpoint{\pgf@circ@res@other-\pgf@circ@res@step}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/ccc}\pgf@circ@res@down}}
		{\pgfpoint{\pgf@circ@res@other-\pgf@circ@res@step}{0pt}}
	\pgfpathcurveto
		{\pgfpoint{\pgf@circ@res@other-\pgf@circ@res@step}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/ccc}\pgf@circ@res@up}}
		{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/ddd}\pgf@circ@res@left}{\pgf@circ@res@up}}
		{\pgfpoint{-\pgf@circ@res@other}{\pgf@circ@res@up}}	
		
	\def\pgf@circ@temp{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/distance}\pgf@circ@res@right+}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@temp-\pgf@circ@res@other}{\pgf@circ@res@up}}
	
	\pgfpathcurveto
		{\pgfpoint{\pgf@circ@temp\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/aaa}\pgf@circ@res@left}{.95*\pgf@circ@res@up}}
		{\pgfpoint{\pgf@circ@temp\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/bbb}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/ccc}\pgf@circ@res@up}}
		{\pgfpoint{\pgf@circ@temp\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/bbb}\pgf@circ@res@left}{0pt}}
	\pgfpathcurveto
		{\pgfpoint{\pgf@circ@temp\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/bbb}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/ccc}\pgf@circ@res@down}}
		{\pgfpoint{\pgf@circ@temp\pgfkeysvalueof{/tikz/circuitikz/tripoles/american xnor port/aaa}\pgf@circ@res@left}{.95*\pgf@circ@res@down}}
		{\pgfpoint{\pgf@circ@temp-\pgf@circ@res@other}{.95*\pgf@circ@res@down}}	
		
		
	\pgfpathellipse
		{\pgfpoint{\pgf@circ@res@other-.5\pgf@circ@res@step}{0pt}}
		{\pgfpoint{.5\pgf@circ@res@step}{0pt}}
		{\pgfpoint{0pt}{.5\pgf@circ@res@step}}
				
	\pgfusepath{draw}
}


\pgfdeclareshape{american not port}
	{
	  \anchor{center}{\pgfpointorigin}
	  \savedanchor\northwest{%
		\pgf@y= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/bipoles/not port/height}\pgf@y
		\pgf@y=.5\pgf@y
		\pgf@x= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/bipoles/not port/width}\pgf@x
		\pgf@x=.5\pgf@x
	  }
	  \savedanchor\left{%
	  	\pgf@y=0pt
	  }
	  \anchor{in}{
		\northwest
		\pgf@y=0pt
	  }
	  \anchor{out}{
		\northwest
		\pgf@y=0pt
		\pgf@x=-\pgf@x
	  }
	  \anchor{center}{
	  	\pgfpointorigin
	  }
	  \anchor{east}{
	  	\left
	  	\pgf@x=-.8\pgf@x  
	  }
	  \anchor{west}{
	  	\left
	  }
	  \anchor{south}{
		\northwest
		\pgf@x=0pt
		\pgf@y=-\pgf@y
	  }
	  \anchor{north}{
		\northwest
		\pgf@x=0pt
	  }
	  	  \anchor{south west}{
		\northwest
		\pgf@y=-\pgf@y
	  }
	  \anchor{north east}{
		\northwest
		\pgf@x=-\pgf@x
	  }
	  \anchor{north west}{
		\northwest
	  }
	  \anchor{south east}{
		\northwest
		\pgf@x=-\pgf@x
		\pgf@y=-\pgf@y
	  }	  
	  \backgroundpath{			
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}	
			
			
			\northwest
			\pgf@circ@res@up = \pgf@y 
			\pgf@circ@res@down = -\pgf@y
			\pgf@circ@res@right = -\pgf@x
			\pgf@circ@res@left = \pgf@x
			
		\pgf@circ@res@other = \pgfkeysvalueof{/tikz/circuitikz/bipoles/not port/circle width}\pgf@circ@res@right
						
	\pgfscope
		\pgfsetlinewidth{2\pgflinewidth}
		\pgftransformxshift{.7\pgf@circ@res@left}
		\pgf@circ@res@step=\pgf@circ@res@right
		\advance\pgf@circ@res@step by -\pgf@circ@res@left
		\pgf@circ@res@step=.7\pgf@circ@res@step
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step-\pgf@circ@res@other}{0pt}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@step-\pgf@circ@res@other}{0pt}}
		\pgfusepath{draw}
		\pgfpathellipse
			{\pgfpoint{\pgf@circ@res@step-.5\pgf@circ@res@other}{0pt}}
			{\pgfpoint{.5\pgf@circ@res@other}{0pt}}
			{\pgfpoint{0pt}{.5\pgf@circ@res@other}}
		\pgfusepath{draw}
	\endpgfscope
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0pt}}
		\pgfpathlineto{\pgfpoint{.7\pgf@circ@res@left}{0pt}}
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
		\pgfpathlineto{\pgfpoint{.7\pgf@circ@res@right}{0pt}}
	
		\pgfusepath{draw}
	  
	  }
	}






%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%

% #1 - name
% #2 - text inside
% #3 - number of inputs
% #4 - is it a not

\long\def\pgfcircdeclareeurologicport#1#2#3#4{
	\pgfdeclareshape{european #1 port}
	{
	  \savedanchor\northwest{%
		\pgf@y= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/european #1 port/height}\pgf@y
		\pgf@y=.5\pgf@y
		\pgf@x= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/european #1 port/width}\pgf@x
		\pgf@x=.5\pgf@x
	  }
	  \savedanchor\left{%
	  	\pgf@y=0pt
	  }
	  \savedanchor\inOne{%
		\pgf@y= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/european #1 port/height}\pgf@y
		\pgf@y=.5\pgf@y
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/european #1 port/input height}\pgf@y
		\pgf@x= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/european #1 port/width}\pgf@x
		\pgf@x=.5\pgf@x
	  }	  
	  \anchor{in}{
		\inOne
	  }
	  \anchor{in 1}{
		\inOne
	  }
	  \anchor{in 2}{
		\inOne
		\pgf@y=-\pgf@y
	  }
	  \anchor{out}{
		\northwest
		\pgf@y=0pt
		\pgf@x=-\pgf@x
	  }
  	  \anchor{center}{
		\northwest
		\pgf@y=0pt
		\pgf@x=-.8\pgf@x  
	  }
	  \anchor{east}{
	  	\left
	  	\pgf@x=-.8\pgf@x  
	  }
	  \anchor{west}{
	  	\left
	  }
	  \anchor{south}{
		\northwest
		\pgf@x=0pt
		\pgf@y=-\pgf@y
	  }
	  \anchor{north}{
		\northwest
		\pgf@x=0pt
	  }
	  \anchor{south west}{
		\northwest
		\pgf@y=-\pgf@y
	  }
	  \anchor{north east}{
		\northwest
		\pgf@x=-\pgf@x
	  }
	  \anchor{north west}{
		\northwest
	  }
	  \anchor{south east}{
		\northwest
		\pgf@x=-\pgf@x
		\pgf@y=-\pgf@y
	  }	  
	  \backgroundpath{			
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}	
			\northwest
			\pgf@circ@res@up = \pgf@y 
			\pgf@circ@res@down = -\pgf@y
			\pgf@circ@res@right = -\pgf@x
			\pgf@circ@res@left = \pgf@x
			\def\pgf@temp{1}
			\def\pgf@circ@temp{#3}
			\ifx\pgftemp\pgf@circ@temp % one input
				\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfpathlineto{
					\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/european #1 port/reserved}\pgf@circ@res@left}{0pt}}
			\else % two inputs
				\pgfpathmoveto{
					\pgfpoint{\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/european #1 port/input height}\pgf@circ@res@up}}
				\pgfpathlineto{
					\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/european #1 port/reserved}\pgf@circ@res@left}
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/european #1 port/input height}\pgf@circ@res@up}}
					%
				\pgfpathmoveto{
					\pgfpoint{\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/european #1 port/input height}\pgf@circ@res@down}}
				\pgfpathlineto{
					\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/european #1 port/reserved}\pgf@circ@res@left}
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/european #1 port/input height}\pgf@circ@res@down}}
			\fi%
			%
			%
			\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
			\pgfpathlineto{
				\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/european #1 port/reserved}\pgf@circ@res@right}{0pt}}
			%
			\edef\pgf@temp{not}
			\edef\pgf@circ@temp{#4}
			\ifx\pgf@temp\pgf@circ@temp % is a not
				\pgfpathmoveto{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/european #1 port/not width}\pgf@circ@res@right}{0pt}}
				\pgfpathlineto{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/european #1 port/reserved}\pgf@circ@res@right}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/european #1 port/not height}\pgf@circ@res@up}}
			\fi
			%
			\pgfusepath{draw}
			%
			\pgfpathmoveto{\pgfpointorigin}
			\pgftext{#2}
			%
			%
			%
			\pgfsetlinewidth{2\pgflinewidth}
			\pgfpathrectanglecorners
				{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/european #1 port/reserved}\pgf@circ@res@left}{\pgf@circ@res@up}}
				{\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/european #1 port/reserved}\pgf@circ@res@right}{\pgf@circ@res@down}}
			\pgfusepath{draw}
%
%
	  }
	}
}



\pgfcircdeclareeurologicport{and}{$\&$}{2}{}
\pgfcircdeclareeurologicport{or}{$\ge 1$}{2}{}
\pgfcircdeclareeurologicport{xor}{$=1$}{2}{}
\pgfcircdeclareeurologicport{not}{$1$}{1}{not}
\pgfcircdeclareeurologicport{nand}{$\&$}{2}{not}
\pgfcircdeclareeurologicport{nor}{$\ge 1$}{2}{not}
\pgfcircdeclareeurologicport{xnor}{$=1$}{2}{not}




%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%


\long\def\pgfcircdeclaretransistor#1#2#3{
	\pgfdeclareshape{#1}
	{
	  \anchor{center}{\pgfpointorigin}
	  \savedanchor\northeast{% upper right
		\pgf@y= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/height}\pgf@y
		\pgf@y=.5\pgf@y
		\pgf@x=0pt
	  }
%	  \savedanchor\northeast{%
%		\pgf@y= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
%		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/height}\pgf@y
%		\pgf@y=.5\pgf@y
%		\pgf@x= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
%		\pgf@x=\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/width}\pgf@x
%	  }
	  \savedanchor\left{%center left
	  	\pgf@y=0pt
		\pgf@x= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/width}\pgf@x
	  }
	  \anchor{text}{
		  \northeast
		  \pgfpoint
			  {12\pgf@circ@res@right +0.2*(\pgf@circ@res@right-\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/gate width}\pgf@circ@res@left)}
			  {0.6\pgf@y}
      }
	  %
	  		% pseudo-bipole
		  \anchor{left}{ % south
		  	\northeast
			\pgf@y=-\pgf@y
		  }
		  \anchor{right}{
		  	\northeast
		  }  
		\anchor{north}{
			\northeast
			\pgf@circ@res@step=\pgf@y
			\left
			\pgf@y=\pgf@circ@res@step
			\pgf@x=.5\pgf@x
		}  
		  \anchor{west}{
			\left
		  }
		  \anchor{east}{
		  	\pgf@x=0pt
			\pgf@y=0pt
		  }  
	  \anchor{south}{
			\northeast
			\pgf@circ@res@step=\pgf@y
			\left
			\pgf@y=-\pgf@circ@res@step
			\pgf@x=.5\pgf@x
	  }
	  \anchor{south west}{
			\northeast
			\pgf@circ@res@step=\pgf@y
			\left
			\pgf@y=-\pgf@circ@res@step
	  }
	  \anchor{north east}{
		\northeast
	  }
	  \anchor{north west}{
			\northeast
			\pgf@circ@res@step=\pgf@y
			\left
			\pgf@y=\pgf@circ@res@step
	  }
	  \anchor{south east}{
		\northeast
		\pgf@y=-\pgf@y
	  }	  
	  
	  #2
	  \backgroundpath{			
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}	
			%
			%
			\northeast
			\pgf@circ@res@up = \pgf@y 
			\pgf@circ@res@down = -\pgf@y
			\pgf@circ@res@right = \pgf@x
			\left
			\pgf@circ@res@left = \pgf@x
			%
			#3
	  %
	  }
	}
}






\long\def\pgfcircdeclaremos#1#2#3{
	\pgfcircdeclaretransistor{#1}{
		  \anchor{G}{
			\left
		  }
		  \anchor{gate}{
			\left
		  }
		  \anchor{B}{
			\left
			\pgf@x=\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base width}\pgf@x
		  }
		  \anchor{base}{
			\left
			\pgf@x=\pgfkeysvalueof{/tikz/circuitikz/tripoles/#1/base width}\pgf@x
		  }
		  #2
	  }
	  {#3}
}









\pgfcircdeclaremos{nmos}{
		  \anchor{D}{
			\northeast
		  }
		  \anchor{drain}{
			\northeast
		  }
		  \anchor{S}{
			\northeast
			\pgf@y=-\pgf@y
		  }
		  \anchor{source}{
			\northeast
			\pgf@y=-\pgf@y
		  }
}{%
			\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/nmos/gate height}\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/nmos/base width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/nmos/gate height}\pgf@circ@res@up}}

			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/nmos/base width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/nmos/base height}\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/nmos/base width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/nmos/base height}\pgf@circ@res@down}}

			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/nmos/base width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/nmos/gate height}\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/nmos/gate height}\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}		
			\pgfusepath{draw}
			
			\pgfscope
			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/nmos/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/nmos/gate height}\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/nmos/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/nmos/gate height}\pgf@circ@res@down}}
			\pgfsetlinewidth{2\pgflinewidth}
			\pgfusepath{draw}
			\endpgfscope
			
		\ifpgf@circuit@mos@arrows
			\pgfscope             
			\pgfslopedattimetrue 
			\pgfallowupsidedownattimetrue
			\pgfresetnontranslationattimefalse
			\pgftransformlineattime{.6}{%
				\pgfpoint%
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/nmos/gate width}\pgf@circ@res@left}%
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/nmos/gate height}\pgf@circ@res@down}%
			}{%
				\pgfpoint
					{\pgf@circ@res@right}%
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/nmos/gate height}\pgf@circ@res@down}%
			}
			\pgfnode{currarrow}{center}{}{}{\pgfusepath{stroke}}
			\endpgfscope
		\fi

					
			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/nmos/gate width}\pgf@circ@res@left}
				{\pgf@circ@res@up+\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up+\pgf@circ@res@down}}
			\pgfusepath{draw}
}


\pgfcircdeclaremos{pmos}{
		  \anchor{S}{
			\northeast
		  }
		  \anchor{source}{
			\northeast
		  }
		  \anchor{D}{
			\northeast
			\pgf@y=-\pgf@y
		  }
		  \anchor{drain}{
			\northeast
			\pgf@y=-\pgf@y
		  }
}{%
			\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pmos/gate height}\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pmos/base width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pmos/gate height}\pgf@circ@res@up}}
			\pgfusepath{draw}

		\ifpgf@circuit@mos@arrows
			\pgfscope             
			\pgfslopedattimetrue 
			\pgfallowupsidedownattimetrue
			\pgfresetnontranslationattimefalse
			\pgftransformlineattime{.4}{%
				\pgfpoint%
					{\pgf@circ@res@right}%
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pmos/gate height}\pgf@circ@res@up}%
			}{%
				\pgfpoint
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pmos/gate width}\pgf@circ@res@left}%
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pmos/gate height}\pgf@circ@res@up}%
			}
			\pgfnode{currarrow}{center}{}{}{\pgfusepath{stroke}}
			\endpgfscope
		\fi

			\pgfscope
			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pmos/base width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pmos/base height}\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pmos/base width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pmos/base height}\pgf@circ@res@down}}
			\pgfsetlinewidth{2\pgflinewidth}
			\pgfusepath{draw}
			\endpgfscope
			
			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pmos/base width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pmos/gate height}\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pmos/gate height}\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}		

			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pmos/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pmos/gate height}\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pmos/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pmos/gate height}\pgf@circ@res@down}}
					
					
			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pmos/gate width}\pgf@circ@res@left}
				{\pgf@circ@res@up+\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up+\pgf@circ@res@down}}
			\pgfusepath{draw}
			
			\pgfpathcircle{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pmos/gate width}\pgf@circ@res@left - \pgfkeysvalueof{/tikz/circuitikz/nodes width}*\pgfkeysvalueof{/tikz/circuitikz/bipoles/length}}
				{\pgf@circ@res@up+\pgf@circ@res@down}}{\pgfkeysvalueof{/tikz/circuitikz/nodes width}*\pgfkeysvalueof{/tikz/circuitikz/bipoles/length}}
			\pgfusepath{draw,fill}		

}







\pgfcircdeclaretransistor{pnp}{
		  \anchor{E}{
			\northeast
		  }
		  \anchor{emitter}{
			\northeast
		  }
		  \anchor{B}{
			\left
		  }
		  \anchor{base}{
			\left
		  }		  
		  \anchor{C}{
			\northeast
			\pgf@y=-\pgf@y
		  }
		  \anchor{collector}{
			\northeast
			\pgf@y=-\pgf@y
		  }
}{
			\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pnp/gate height}\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pnp/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pnp/gate height 2}\pgf@circ@res@up}}
			\pgfusepath{draw}

			\pgfscope
			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pnp/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pnp/base height}\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pnp/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pnp/base height}\pgf@circ@res@down}}
			\pgfsetlinewidth{2\pgflinewidth}
			\pgfusepath{draw}
			\endpgfscope
			
			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pnp/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pnp/gate height 2}\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pnp/gate height}\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}		
			\pgfusepath{draw}
	
			\pgfscope             
			\pgfslopedattimetrue 
			\pgfallowupsidedownattimetrue
			\pgfresetnontranslationattimefalse
			\pgftransformlineattime{.5}{%
				\pgfpoint%
					{\pgf@circ@res@right}%
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pnp/gate height}\pgf@circ@res@up}%
			}{%
				\pgfpoint
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pnp/gate width}\pgf@circ@res@left}%
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pnp/gate height 2}\pgf@circ@res@up}%
			}
			\pgfnode{currarrow}{center}{}{}{\pgfusepath{stroke}}
			\endpgfscope
		
			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pnp/gate width}\pgf@circ@res@left}
				{\pgf@circ@res@up+\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up+\pgf@circ@res@down}}
			\pgfusepath{draw}
}






\pgfcircdeclaretransistor{npn}{
		  \anchor{C}{
			\northeast
		  }
		  \anchor{collector}{
			\northeast
		  }
		  \anchor{B}{
			\left
		  }
		  \anchor{base}{
			\left
		  }		  
		  \anchor{E}{
			\northeast
			\pgf@y=-\pgf@y
		  }
		  \anchor{emitter}{
			\northeast
			\pgf@y=-\pgf@y
		  }
}{%
			\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/npn/gate height}\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/npn/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/npn/gate height 2}\pgf@circ@res@up}}
			\pgfusepath{draw}

			\pgfscope
			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/npn/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/npn/base height}\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/npn/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/npn/base height}\pgf@circ@res@down}}
			\pgfsetlinewidth{2\pgflinewidth}
			\pgfusepath{draw}
			\endpgfscope
			
			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/npn/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/npn/gate height 2}\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/npn/gate height}\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}		
			\pgfusepath{draw}
	
			\pgfscope
			\pgfslopedattimetrue
			\pgfallowupsidedownattimetrue
			\pgfresetnontranslationattimefalse
			\pgftransformlineattime{.5}{%
				\pgfpoint%
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/npn/gate width}\pgf@circ@res@left}%
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/npn/gate height 2}\pgf@circ@res@down}%
			}{%
				\pgfpoint{\pgf@circ@res@right}%
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/npn/gate height}\pgf@circ@res@down}%
			}
			\pgfnode{currarrow}{center}{}{}{\pgfusepath{stroke}}
			\endpgfscope
		
			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/npn/gate width}\pgf@circ@res@left}
				{\pgf@circ@res@up+\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up+\pgf@circ@res@down}}
			\pgfusepath{draw}
			
			
}



\pgfcircdeclaretransistor{pigbt}{
		  \anchor{E}{
			\northeast
		  }
		  \anchor{emitter}{
			\northeast
		  }
		  \anchor{B}{
			\left
		  }
		  \anchor{base}{
			\left
		  }		  
		  \anchor{C}{
			\northeast
			\pgf@y=-\pgf@y
		  }
		  \anchor{collector}{
			\northeast
			\pgf@y=-\pgf@y
		  }
}{
			\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigbt/gate height}\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigbt/base width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigbt/gate height 2}\pgf@circ@res@up}}
			\pgfusepath{draw}

			\pgfscope
			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigbt/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigbt/base height}\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigbt/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigbt/base height}\pgf@circ@res@down}}
			%\pgfsetlinewidth{2\pgflinewidth}
			\pgfusepath{draw}
			\endpgfscope
			
			\pgfscope
			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigbt/base width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigbt/base height}\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigbt/base width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigbt/base height}\pgf@circ@res@down}}
			\pgfsetlinewidth{2\pgflinewidth}
			\pgfusepath{draw}
			\endpgfscope
			
			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigbt/base width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigbt/gate height 2}\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigbt/gate height}\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}		
			\pgfusepath{draw}
	
			\pgfscope             
			\pgfslopedattimetrue 
			\pgfallowupsidedownattimetrue
			\pgfresetnontranslationattimefalse
			\pgftransformlineattime{.5}{%
				\pgfpoint%
					{\pgf@circ@res@right}%
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigbt/gate height}\pgf@circ@res@up}%
			}{%
				\pgfpoint
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigbt/base width}\pgf@circ@res@left}%
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigbt/gate height 2}\pgf@circ@res@up}%
			}
			\pgfnode{currarrow}{center}{}{}{\pgfusepath{stroke}}
			\endpgfscope
		
			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigbt/gate width}\pgf@circ@res@left}
				{\pgf@circ@res@up+\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up+\pgf@circ@res@down}}
			\pgfusepath{draw}
			
			
}



\pgfcircdeclaretransistor{nigbt}{
		  \anchor{C}{
			\northeast
		  }
		  \anchor{collector}{
			\northeast
		  }
		  \anchor{B}{
			\left
		  }
		  \anchor{base}{
			\left
		  }		  
		  \anchor{E}{
			\northeast
			\pgf@y=-\pgf@y
		  }
		  \anchor{emitter}{
			\northeast
			\pgf@y=-\pgf@y
		  }
}{
			\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigbt/gate height}\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigbt/base width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigbt/gate height 2}\pgf@circ@res@up}}
			\pgfusepath{draw}

			\pgfscope
			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigbt/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigbt/base height}\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigbt/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigbt/base height}\pgf@circ@res@down}}
			\pgfsetlinewidth{2\pgflinewidth}
			\pgfusepath{draw}
			\endpgfscope
			
			\pgfscope
			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigbt/base width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigbt/base height}\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigbt/base width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigbt/base height}\pgf@circ@res@down}}
			%\pgfsetlinewidth{2\pgflinewidth}
			\pgfusepath{draw}
			\endpgfscope
			
			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigbt/base width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigbt/gate height 2}\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigbt/gate height}\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}		
			\pgfusepath{draw}
	
			\pgfscope
			\pgfslopedattimetrue
			\pgfallowupsidedownattimetrue
			\pgfresetnontranslationattimefalse
			\pgftransformlineattime{.5}{%
				\pgfpoint%
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigbt/base width}\pgf@circ@res@left}%
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigbt/gate height 2}\pgf@circ@res@down}%
			}{%
				\pgfpoint{\pgf@circ@res@right}%
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigbt/gate height}\pgf@circ@res@down}%
			}
			\pgfnode{currarrow}{center}{}{}{\pgfusepath{stroke}}
			\endpgfscope
		
			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigbt/gate width}\pgf@circ@res@left}
				{\pgf@circ@res@up+\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up+\pgf@circ@res@down}}
			\pgfusepath{draw}
			
			
}








%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%%% Contrib


%%
% IGFET (e.g. MOSFET)
\long\def\pgfcircdeclarefet#1#2#3{
  \pgfcircdeclaretransistor{#1}{
      \anchor{B}{
      \left
      \pgf@x=\pgf@circ@res@right
      }
      \anchor{base}{
      \left
      \pgf@x=\pgf@circ@res@right
      }
      #2
    }
    {#3}
}



\pgfcircdeclarefet{nfet}{
      \anchor{D}{
      \northeast
      }
      \anchor{drain}{
      \northeast
      }
      \anchor{S}{
      \northeast
      \pgf@y=-\pgf@y
      }
      \anchor{source}{
      \northeast
      \pgf@y=-\pgf@y
      }
      \anchor{G}{
         \left
      }
      \anchor{gate}{
         \left
      }

}{%
      \pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nfet/gate height}\pgf@circ@res@up}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nfet/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nfet/gate height}\pgf@circ@res@up}}

      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nfet/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nfet/base height}\pgf@circ@res@up}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nfet/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nfet/base height}\pgf@circ@res@up*0.45}}
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nfet/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nfet/base height}\pgf@circ@res@up*0.25}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nfet/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nfet/base height}\pgf@circ@res@down*0.25}}
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nfet/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nfet/base height}\pgf@circ@res@down*0.45}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nfet/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nfet/base height}\pgf@circ@res@down}}

      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nfet/base width}\pgf@circ@res@left}
        {\pgf@circ@res@up+\pgf@circ@res@down}}
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
        {\pgf@circ@res@up+\pgf@circ@res@down}}
      
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nfet/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nfet/gate height}\pgf@circ@res@down}}
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nfet/gate height}\pgf@circ@res@down}}
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}    
      \pgfusepath{draw}
      
      \pgfscope
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nfet/gate width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nfet/gate height}\pgf@circ@res@up}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nfet/gate width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nfet/gate height}\pgf@circ@res@down}}
      \pgfsetlinewidth{2\pgflinewidth}
      \pgfusepath{draw}
      \endpgfscope
      
      \pgfscope
      \pgfslopedattimetrue 
      \pgfallowupsidedownattimetrue
      \pgfresetnontranslationattimefalse
      \pgftransformlineattime{.6}{%
        \pgfpoint
          {\pgf@circ@res@right}%
          {\pgf@circ@res@up+\pgf@circ@res@down}%
      }{%
        \pgfpoint%
          {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/base width}\pgf@circ@res@left}%
          {\pgf@circ@res@up+\pgf@circ@res@down}%
      }
      \pgfnode{currarrow}{center}{}{}{\pgfusepath{stroke}}
      \endpgfscope

          
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nfet/gate width}\pgf@circ@res@left}
        {\pgf@circ@res@up+\pgf@circ@res@down}}
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up+\pgf@circ@res@down}}
      \pgfusepath{draw}
}


\pgfcircdeclarefet{pfet}{
      \anchor{D}{
      \northeast
      }
      \anchor{drain}{
      \northeast
      }
      \anchor{S}{
      \northeast
      \pgf@y=-\pgf@y
      }
      \anchor{source}{
      \northeast
      \pgf@y=-\pgf@y
      }
      \anchor{G}{
         \left
      }
      \anchor{gate}{
         \left
      }

}{%
      \pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pfet/gate height}\pgf@circ@res@up}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pfet/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pfet/gate height}\pgf@circ@res@up}}
	  \pgfusepath{draw}

	 \pgfscope
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pfet/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pfet/base height}\pgf@circ@res@up}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pfet/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pfet/base height}\pgf@circ@res@up*0.45}}
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pfet/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pfet/base height}\pgf@circ@res@up*0.25}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pfet/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pfet/base height}\pgf@circ@res@down*0.25}}
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pfet/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pfet/base height}\pgf@circ@res@down*0.45}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pfet/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pfet/base height}\pgf@circ@res@down}}
	  \pgfsetlinewidth{2\pgflinewidth}
      \pgfusepath{draw}
      \endpgfscope

      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pfet/base width}\pgf@circ@res@left}
        {\pgf@circ@res@up+\pgf@circ@res@down}}
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
        {\pgf@circ@res@up+\pgf@circ@res@down}}
      
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pfet/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pfet/gate height}\pgf@circ@res@down}}
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pfet/gate height}\pgf@circ@res@down}}
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}    
      \pgfusepath{draw}
      
      \pgfscope
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pfet/gate width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pfet/gate height}\pgf@circ@res@up}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pfet/gate width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pfet/gate height}\pgf@circ@res@down}}
      %\pgfsetlinewidth{2\pgflinewidth}
      \pgfusepath{draw}
      \endpgfscope
      
      \pgfscope
      \pgfslopedattimetrue 
      \pgfallowupsidedownattimetrue
      \pgfresetnontranslationattimefalse
      \pgftransformlineattime{.6}{%
        \pgfpoint
          {\pgf@circ@res@right}%
          {\pgf@circ@res@up+\pgf@circ@res@down}%
      }{%
        \pgfpoint%
          {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/base width}\pgf@circ@res@left}%
          {\pgf@circ@res@up+\pgf@circ@res@down}%
      }
	  \pgftransformrotate{180}
      \pgfnode{currarrow}{center}{}{}{\pgfusepath{stroke}}
      \endpgfscope

          
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pfet/gate width}\pgf@circ@res@left}
        {\pgf@circ@res@up+\pgf@circ@res@down}}
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up+\pgf@circ@res@down}}
      \pgfusepath{draw}
}



% N-CHANNEL IGFET ENHANCEMENT TYPE
\pgfcircdeclarefet{nigfete}{
      \anchor{D}{
      \northeast
      }
      \anchor{drain}{
      \northeast
      }
      \anchor{S}{
      \northeast
      \pgf@y=-\pgf@y
      }
      \anchor{source}{
      \northeast
      \pgf@y=-\pgf@y
      }
      \anchor{G}{
         \northeast
         \pgf@circ@res@step=\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/gate height}\pgf@y
         \left
         \pgf@y=-\pgf@circ@res@step
      }
      \anchor{gate}{
         \northeast
         \pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/gate height}\pgf@y
      }
}{%
      \pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
      % DRAIN CONNECTION 
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/gate height}\pgf@circ@res@up}}
      % DRAIN
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/gate height}\pgf@circ@res@up}}

      % GATE, ENHANCEMENT TYPE (DASHED)
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/base height}\pgf@circ@res@up}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/base height}\pgf@circ@res@up*0.45}}
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/base height}\pgf@circ@res@up*0.25}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/base height}\pgf@circ@res@down*0.25}}
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/base height}\pgf@circ@res@down*0.45}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/base height}\pgf@circ@res@down}}

      % BULK
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/base width}\pgf@circ@res@left}
        {\pgf@circ@res@up+\pgf@circ@res@down}}
       \pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
         {\pgf@circ@res@up+\pgf@circ@res@down}}

      % SOURCE
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/gate height}\pgf@circ@res@down}}
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
         {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/gate height}\pgf@circ@res@down}}
      % SOURCE CONNECTION
      \pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}    
      \pgfusepath{draw}
      
      % GATE
      \pgfscope
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/gate width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/gate height}\pgf@circ@res@up}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/gate width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/gate height}\pgf@circ@res@down}}
      \pgfsetlinewidth{2\pgflinewidth}
      \pgfusepath{draw}
      \endpgfscope
      
      % ARROW
      \pgfscope
      \pgfslopedattimetrue 
      \pgfallowupsidedownattimetrue
      \pgfresetnontranslationattimefalse
      \pgftransformlineattime{.6}{%
        \pgfpoint
          {\pgf@circ@res@right}%
          {\pgf@circ@res@up+\pgf@circ@res@down}%
      }{%
        \pgfpoint%
          {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/base width}\pgf@circ@res@left}%
          {\pgf@circ@res@up+\pgf@circ@res@down}%
      }
      \pgfnode{currarrow}{center}{}{}{\pgfusepath{stroke}}
      \endpgfscope

      % GATE CONNECTION
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/gate width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/gate height}\pgf@circ@res@down}}
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/gate height}\pgf@circ@res@down}}
      \pgfusepath{draw}
}

% N-CHANNEL IGFET DEPLETION TYPE
\pgfcircdeclarefet{nigfetd}{
      \anchor{D}{
      \northeast
      }
      \anchor{drain}{
      \northeast
      }
      \anchor{S}{
      \northeast
      \pgf@y=-\pgf@y
      }
      \anchor{source}{
      \northeast
      \pgf@y=-\pgf@y
      }
      \anchor{G}{
         \northeast
         \pgf@circ@res@step=\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/gate height}\pgf@y
         \left
         \pgf@y=-\pgf@circ@res@step
      }
      \anchor{gate}{
         \northeast
         \pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/gate height}\pgf@y
      }

}{%
      \pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
      % DRAIN CONNECTION 
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfetd/gate height}\pgf@circ@res@up}}
      % DRAIN
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfetd/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfetd/gate height}\pgf@circ@res@up}}

      % GATE, DEPLETION TYPE
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfetd/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfetd/base height}\pgf@circ@res@up}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfetd/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfetd/base height}\pgf@circ@res@down}}

      % BULK
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfetd/base width}\pgf@circ@res@left}
        {\pgf@circ@res@up+\pgf@circ@res@down}}
       \pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
         {\pgf@circ@res@up+\pgf@circ@res@down}}

      % SOURCE
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfetd/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfetd/gate height}\pgf@circ@res@down}}
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
         {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfetd/gate height}\pgf@circ@res@down}}
      % SOURCE CONNECTION
      \pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}    
      \pgfusepath{draw}
      
      % GATE
      \pgfscope
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfetd/gate width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfetd/gate height}\pgf@circ@res@up}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfetd/gate width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfetd/gate height}\pgf@circ@res@down}}
      \pgfsetlinewidth{2\pgflinewidth}
      \pgfusepath{draw}
      \endpgfscope
      
      % ARROW
      \pgfscope
      \pgfslopedattimetrue 
      \pgfallowupsidedownattimetrue
      \pgfresetnontranslationattimefalse
      \pgftransformlineattime{.6}{%
        \pgfpoint
          {\pgf@circ@res@right}%
          {\pgf@circ@res@up+\pgf@circ@res@down}%
      }{%
        \pgfpoint%
          {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfetd/base width}\pgf@circ@res@left}%
          {\pgf@circ@res@up+\pgf@circ@res@down}%
      }
      \pgfnode{currarrow}{center}{}{}{\pgfusepath{stroke}}
      \endpgfscope

      % GATE CONNECTION
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfetd/gate width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfetd/gate height}\pgf@circ@res@down}}
      %\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up+\pgf@circ@res@down}}
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfetd/gate height}\pgf@circ@res@down}}
      \pgfusepath{draw}
}

% P-CHANNEL IGFET ENHANCEMENT TYPE
\pgfcircdeclarefet{pigfete}{
      \anchor{D}{
      \northeast
      }
      \anchor{drain}{
      \northeast
      }
      \anchor{S}{
      \northeast
      \pgf@y=-\pgf@y
      }
      \anchor{source}{
      \northeast
      \pgf@y=-\pgf@y
      }
      \anchor{G}{
         \northeast
         \pgf@circ@res@step=\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/gate height}\pgf@y
         \left
         \pgf@y=-\pgf@circ@res@step
      }
      \anchor{gate}{
         \northeast
         \pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/gate height}\pgf@y
      }
}{%
      \pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
      % DRAIN CONNECTION 
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfete/gate height}\pgf@circ@res@up}}
      % DRAIN
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfete/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfete/gate height}\pgf@circ@res@up}}
	  \pgfusepath{draw}
	  
      % GATE, DASHED, BOLD
	  \pgfscope
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfete/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfete/base height}\pgf@circ@res@up}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfete/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfete/base height}\pgf@circ@res@up*0.45}}
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfete/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfete/base height}\pgf@circ@res@up*0.25}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfete/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfete/base height}\pgf@circ@res@down*0.25}}
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfete/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfete/base height}\pgf@circ@res@down*0.45}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfete/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfete/base height}\pgf@circ@res@down}}
	  \pgfsetlinewidth{2\pgflinewidth}
      \pgfusepath{draw}
      \endpgfscope
	  
      % BULK
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfete/base width}\pgf@circ@res@left}
        {\pgf@circ@res@up+\pgf@circ@res@down}}
       \pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
         {\pgf@circ@res@up+\pgf@circ@res@down}}

      % SOURCE
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfete/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfete/gate height}\pgf@circ@res@down}}
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
         {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfete/gate height}\pgf@circ@res@down}}
      % SOURCE CONNECTION
      \pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}    
      \pgfusepath{draw}
      
      % GATE
      \pgfscope
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfete/gate width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfete/gate height}\pgf@circ@res@up}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfete/gate width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfete/gate height}\pgf@circ@res@down}}
      %\pgfsetlinewidth{2\pgflinewidth}
      \pgfusepath{draw}
      \endpgfscope
      
      % ARROW
      \pgfscope
      \pgfslopedattimetrue 
      \pgfallowupsidedownattimetrue
      \pgfresetnontranslationattimefalse
      % Arrow has to be rotated, as this is a p-channel fet
      \pgftransformrotate{180}
      \pgftransformlineattime{-.6}{%
        \pgfpoint
          {\pgf@circ@res@right}%
          {\pgf@circ@res@up+\pgf@circ@res@down}%
      }{%
        \pgfpoint%
          {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfete/base width}\pgf@circ@res@left}%
          {\pgf@circ@res@up+\pgf@circ@res@down}%
      }
      \pgfnode{currarrow}{center}{}{}{\pgfusepath{stroke}}
      \endpgfscope

      % GATE CONNECTION (in line with source)
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfete/gate width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfete/gate height}\pgf@circ@res@down}}
      %\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up+\pgf@circ@res@down}}
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfete/gate height}\pgf@circ@res@down}}
      \pgfusepath{draw}
}

% P-CHANNEL IGFET DEPLETION TYPE
\pgfcircdeclarefet{pigfetd}{
      \anchor{D}{
      \northeast
      }
      \anchor{drain}{
      \northeast
      }
      \anchor{S}{
      \northeast
      \pgf@y=-\pgf@y
      }
      \anchor{source}{
      \northeast
      \pgf@y=-\pgf@y
      }
      \anchor{G}{
         \northeast
         \pgf@circ@res@step=\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/gate height}\pgf@y
         \left
         \pgf@y=-\pgf@circ@res@step
      }
      \anchor{gate}{
         \northeast
         \pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/nigfete/gate height}\pgf@y
      }
}{%
      \pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
      % DRAIN CONNECTION 
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfetd/gate height}\pgf@circ@res@up}}
      % DRAIN
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfetd/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfetd/gate height}\pgf@circ@res@up}}
	  
      \pgfusepath{draw}
      
	  
      % GATE DEPLETION TYPE
	  \pgfscope
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfetd/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfetd/base height}\pgf@circ@res@up}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfetd/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfetd/base height}\pgf@circ@res@down}}
	  \pgfsetlinewidth{2\pgflinewidth}
      \pgfusepath{draw}
      \endpgfscope
	  
      % BULK
	  
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfetd/base width}\pgf@circ@res@left}
        {\pgf@circ@res@up+\pgf@circ@res@down}}
       \pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
         {\pgf@circ@res@up+\pgf@circ@res@down}}

      
      % SOURCE
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfetd/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfetd/gate height}\pgf@circ@res@down}}
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
         {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfetd/gate height}\pgf@circ@res@down}}
      % SOURCE CONNECTION
      \pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}    
      \pgfusepath{draw}
      
      % GATE
      \pgfscope
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfetd/gate width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfetd/gate height}\pgf@circ@res@up}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfetd/gate width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfetd/gate height}\pgf@circ@res@down}}
      %\pgfsetlinewidth{2\pgflinewidth}
      \pgfusepath{draw}
      \endpgfscope
      
      % ARROW
      \pgfscope
      \pgfslopedattimetrue 
      \pgfallowupsidedownattimetrue
      \pgfresetnontranslationattimefalse
      % PFET!
      \pgftransformrotate{180}
      \pgftransformlineattime{-.6}{%
        \pgfpoint
          {\pgf@circ@res@right}%
          {\pgf@circ@res@up+\pgf@circ@res@down}%
      }{%
        \pgfpoint%
          {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfete/base width}\pgf@circ@res@left}%
          {\pgf@circ@res@up+\pgf@circ@res@down}%
      }
      \pgfnode{currarrow}{center}{}{}{\pgfusepath{stroke}}
      \endpgfscope

      % GATE CONNECTION
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfetd/gate width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfetd/gate height}\pgf@circ@res@down}}
      %\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up+\pgf@circ@res@down}}
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pigfetd/gate height}\pgf@circ@res@down}}
      \pgfusepath{draw}
}



%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%

%% Contrib Danilo Piazzalunga






\pgfcircdeclaretransistor{njfet}{
		  \anchor{G}{
			\left
			\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
			\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/njfet/height}\pgf@y
			\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/njfet/gate height 2}\pgf@y
			\pgf@y=-.5\pgf@y
		  }
		  \anchor{gate}{
			\left
			\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
			\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/njfet/height}\pgf@y
			\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/njfet/gate height 2}\pgf@y
			\pgf@y=-.5\pgf@y
		  }
		  \anchor{D}{
			\northeast
		  }
		  \anchor{drain}{
			\northeast
		  }
		  \anchor{S}{
			\northeast
			\pgf@y=-\pgf@y
		  }
		  \anchor{source}{
			\northeast
			\pgf@y=-\pgf@y
		  }
}{%
			\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/njfet/gate height 2}\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/njfet/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/njfet/gate height 2}\pgf@circ@res@up}}

			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/njfet/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/njfet/gate height 2}\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/njfet/gate height 2}\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}		
			\pgfusepath{draw}
			
			\pgfscope
			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/njfet/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/njfet/gate height}\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/njfet/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/njfet/gate height}\pgf@circ@res@down}}
			\pgfsetlinewidth{2\pgflinewidth}
			\pgfusepath{draw}
			\endpgfscope
			
			\pgfscope             
			\pgfslopedattimetrue 
			\pgfallowupsidedownattimetrue
			\pgfresetnontranslationattimefalse
			\pgftransformlineattime{.6}{%
				\pgfpoint{\pgf@circ@res@left}%
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/njfet/gate height 2}\pgf@circ@res@down}%
			}{%
				\pgfpoint
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/njfet/gate width}\pgf@circ@res@left}%
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/njfet/gate height 2}\pgf@circ@res@down}%
			}
			\pgfnode{currarrow}{center}{}{}{\pgfusepath{stroke}}
			\endpgfscope

					
			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/njfet/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/njfet/gate height 2}\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/njfet/gate height 2}\pgf@circ@res@down}}
			\pgfusepath{draw}
}


\pgfcircdeclaretransistor{pjfet}{
		  \anchor{G}{
			\left
			\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
			\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/pjfet/height}\pgf@y
			\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/pjfet/gate height 2}\pgf@y
			\pgf@y=.5\pgf@y
		  }
		  \anchor{gate}{
			\left
			\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
			\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/pjfet/height}\pgf@y
			\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/pjfet/gate height 2}\pgf@y
			\pgf@y=.5\pgf@y
		  }
		  \anchor{S}{
			\northeast
		  }
		  \anchor{source}{
			\northeast
		  }
		  \anchor{D}{
			\northeast
			\pgf@y=-\pgf@y
		  }
		  \anchor{drain}{
			\northeast
			\pgf@y=-\pgf@y
		  }
}{%
			\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pjfet/gate height 2}\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pjfet/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pjfet/gate height 2}\pgf@circ@res@up}}

			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pjfet/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pjfet/gate height 2}\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pjfet/gate height 2}\pgf@circ@res@down}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}		
			\pgfusepath{draw}
			
			\pgfscope
			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pjfet/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pjfet/gate height}\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pjfet/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pjfet/gate height}\pgf@circ@res@down}}
			\pgfsetlinewidth{2\pgflinewidth}
			\pgfusepath{draw}
			\endpgfscope
			
			\pgfscope             
			\pgfslopedattimetrue 
			\pgfallowupsidedownattimetrue
			\pgfresetnontranslationattimefalse
			\pgftransformlineattime{.4}{%
				\pgfpoint%
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pjfet/gate width}\pgf@circ@res@left}%
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pjfet/gate height 2}\pgf@circ@res@up}%
			}{%
				\pgfpoint{\pgf@circ@res@left}%
					{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pjfet/gate height 2}\pgf@circ@res@up}%
			}
			\pgfnode{currarrow}{center}{}{}{\pgfusepath{stroke}}
			\endpgfscope

					
			\pgfpathmoveto{\pgfpoint
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pjfet/gate width}\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pjfet/gate height 2}\pgf@circ@res@up}}
			\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}
				{\pgfkeysvalueof{/tikz/circuitikz/tripoles/pjfet/gate height 2}\pgf@circ@res@up}}
			\pgfusepath{draw}
}








%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%







% ISFET
\pgfcircdeclarefet{isfet}{
      \anchor{D}{
      \northeast
      }
      \anchor{drain}{
      \northeast
      }
      \anchor{S}{
      \northeast
      \pgf@y=-\pgf@y
      }
      \anchor{source}{
      \northeast
      \pgf@y=-\pgf@y
      }
}{%
      \pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
      % DRAIN CONNECTION 
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/gate height}\pgf@circ@res@up}}
      % DRAIN
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/gate height}\pgf@circ@res@up}}
      \pgfusepath{draw}
      
      % GATE, DEPLETION TYPE
      \pgfscope %% added
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/base height}\pgf@circ@res@up}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/base height}\pgf@circ@res@down}}
      \pgfsetlinewidth{2\pgflinewidth} %% added
      \pgfusepath{draw} %% added
      \endpgfscope %% added
      
      % BULK
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/base width}\pgf@circ@res@left}
        {\pgf@circ@res@up+\pgf@circ@res@down}}
       \pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
         {\pgf@circ@res@up+\pgf@circ@res@down}}

      % SOURCE
      \pgfpathmoveto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/base width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/gate height}\pgf@circ@res@down}}
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@right}
         {\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/gate height}\pgf@circ@res@down}}
      % SOURCE CONNECTION
      \pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
      \pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}    
      \pgfusepath{draw}
      
      % GATE
      %\pgfscope
      %\pgfpathmoveto{\pgfpoint
       % {\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/gate width}\pgf@circ@res@left}
       % {\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/gate height}\pgf@circ@res@up}}
      %\pgfpathlineto{\pgfpoint
       % {\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/gate width}\pgf@circ@res@left}
       % {\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/gate height}\pgf@circ@res@down}}
      %\pgfsetlinewidth{2\pgflinewidth}
      %\pgfusepath{draw}
      %\endpgfscope
      
      % ARROW
      \pgfscope
      \pgfslopedattimetrue 
      \pgfallowupsidedownattimetrue
      \pgfresetnontranslationattimefalse
      \pgftransformlineattime{.6}{%
        \pgfpoint
          {\pgf@circ@res@right}%
          {\pgf@circ@res@up+\pgf@circ@res@down}%
      }{%
        \pgfpoint%
          {\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/base width}\pgf@circ@res@left}%
          {\pgf@circ@res@up+\pgf@circ@res@down}%
      }
      \pgfnode{currarrow}{center}{}{}{\pgfusepath{stroke}}
      \endpgfscope
      \pgfusepath{draw}
      
      % Wavy lines
      	\pgfscope
			\pgfpathmoveto{\pgfpoint{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/waves x sep}\pgf@circ@res@up}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/waves y sep}\pgf@circ@res@up}}
			\pgfpathsine{\pgfpoint{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave width}\pgf@circ@res@up}{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave amp}\pgf@circ@res@up}}
			\pgfpathcosine{\pgfpoint{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave width}\pgf@circ@res@up}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave amp}\pgf@circ@res@up}}
			\pgfpathsine{\pgfpoint{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave width}\pgf@circ@res@up}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave amp}\pgf@circ@res@up}}
			\pgfpathcosine{\pgfpoint{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave width}\pgf@circ@res@up}{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave amp}\pgf@circ@res@up}}
			\pgfusepath{draw}

			\pgfpathmoveto{\pgfpoint{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/waves x sep}\pgf@circ@res@up}{0cm}}
			\pgfpathsine{\pgfpoint{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave width}\pgf@circ@res@up}{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave amp}\pgf@circ@res@up}}
			\pgfpathcosine{\pgfpoint{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave width}\pgf@circ@res@up}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave amp}\pgf@circ@res@up}}
			\pgfpathsine{\pgfpoint{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave width}\pgf@circ@res@up}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave amp}\pgf@circ@res@up}}
			\pgfpathcosine{\pgfpoint{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave width}\pgf@circ@res@up}{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave amp}\pgf@circ@res@up}}
			\pgfusepath{draw}

			\pgfpathmoveto{\pgfpoint{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/waves x sep}\pgf@circ@res@up}{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/waves y sep}\pgf@circ@res@up}}
			\pgfpathsine{\pgfpoint{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave width}\pgf@circ@res@up}{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave amp}\pgf@circ@res@up}}
			\pgfpathcosine{\pgfpoint{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave width}\pgf@circ@res@up}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave amp}\pgf@circ@res@up}}
			\pgfpathsine{\pgfpoint{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave width}\pgf@circ@res@up}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave amp}\pgf@circ@res@up}}
			\pgfpathcosine{\pgfpoint{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave width}\pgf@circ@res@up}{-\pgfkeysvalueof{/tikz/circuitikz/tripoles/isfet/wave amp}\pgf@circ@res@up}}
			\pgfusepath{draw}
		\endpgfscope

}














%% Black thyristor

\pgfcircdeclarebipole{
	\anchor{gate}{
		\northeast
	}
	\anchor{anode}{
		\ifpgf@circuit@bipole@reversed\northeast\else\southwest\fi
		\pgf@y=0cm
	}
	\anchor{G}{
		\northeast
	}
	\anchor{cathode}{
		\ifpgf@circuit@bipole@reversed\southwest\else\northeast\fi
		\pgf@y=0cm
	}
}{\ctikzvalof{tripoles/thyristor/height 2}}{thyristor}{\ctikzvalof{tripoles/thyristor/height}}{\ctikzvalof{tripoles/thyristor/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

	\pgf@circ@res@other = \ctikzvalof{tripoles/thyristor/diode width left}\pgf@circ@res@left
	\pgf@circ@res@step = \ctikzvalof{tripoles/thyristor/diode width right}\pgf@circ@res@right

	\pgfscope
		\pgftransformxshift{\pgf@circ@res@other}
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step-\pgf@circ@res@other}{0pt}}
				
		\pgfpathlineto{\pgfpoint{0pt}{-\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}} 
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@step-\pgf@circ@res@other}{0pt}}
		\pgfusepath{draw,fill}
		
		\pgfsetlinewidth{\pgfstartlinewidth}
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step-\pgf@circ@res@other}{0pt}}
		\pgfpathlineto{\pgfpoint{2*\pgf@circ@res@step-2*\pgf@circ@res@other}{\ctikzvalof{tripoles/thyristor/diode height}\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{2*\pgf@circ@res@step-2*\pgf@circ@res@other}{\pgf@circ@res@up}}
		\pgfusepath{draw}
	\endpgfscope
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step}{\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{-\pgf@circ@res@down}}
	
	\pgfusepath{draw}
	
	\pgfsetlinewidth{\pgfstartlinewidth}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@other}{0pt}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{0pt}}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step}{0pt}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{0pt}}
	
	\pgfusepath{draw}
	
}


%% Empty triac

\pgfcircdeclarebipole{
	\anchor{gate}{
		\northeast
	}
	\anchor{G}{
		\northeast
	}
	\anchor{anode}{
		\ifpgf@circuit@bipole@reversed\northeast\else\southwest\fi
		\pgf@y=0cm
	}
	\anchor{cathode}{
		\ifpgf@circuit@bipole@reversed\southwest\else\northeast\fi
		\pgf@y=0cm
	}
}{\ctikzvalof{tripoles/triac/height}}{triac}{\ctikzvalof{tripoles/triac/height}}{\ctikzvalof{tripoles/triac/width}}{

	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}

	\pgf@circ@res@other = \ctikzvalof{tripoles/triac/diode width left}\pgf@circ@res@left
	\pgf@circ@res@step = \ctikzvalof{tripoles/triac/diode width right}\pgf@circ@res@right

	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@other}{0pt}}
	\pgfpathlineto{\pgfpoint{0.95\pgf@circ@res@step}{0.707*(\pgf@circ@res@other-\pgf@circ@res@step)}} % sqrt(1/2)
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{1.414*(\pgf@circ@res@other-\pgf@circ@res@step)}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{-1.414*(\pgf@circ@res@other-\pgf@circ@res@step)}}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step}{0pt}}
	\pgfpathlineto{\pgfpoint{0.95\pgf@circ@res@other}{-0.707*(\pgf@circ@res@other-\pgf@circ@res@step)}} % sqrt(1/2)
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{-1.414*(\pgf@circ@res@other-\pgf@circ@res@step)}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{1.414*(\pgf@circ@res@other-\pgf@circ@res@step)}}
	
	\pgfusepath{draw}
	
	\pgfsetlinewidth{\pgfstartlinewidth}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step}{-0.707*(\pgf@circ@res@other-\pgf@circ@res@step)}} % sqrt(1/2)
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{-1.414*(\pgf@circ@res@other-\pgf@circ@res@step)}} % sqrt(1/2)
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}} % sqrt(1/2)
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@other}{0pt}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{0pt}}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step}{0pt}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{0pt}}
	
	\pgfusepath{draw}
	
}









\pgfcircdeclarebipole{
	\anchor{out 1}{
		\ifpgf@circuit@bipole@reversed\southwest\else\northeast\fi
		\pgf@y=0cm
	}
	\anchor{out 2}{
		\ifpgf@circuit@bipole@reversed\southwest\else\northeast\fi
		\pgf@y=.8\pgf@y
	}
}{\ctikzvalof{tripoles/toggleswitch/height 2}}{toggleswitch}{\ctikzvalof{tripoles/toggleswitch/height}}{\ctikzvalof{tripoles/toggleswitch/width}}{

	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0pt}}
	\pgfpathlineto{\pgfpoint{.3\pgf@circ@res@left}{0pt}}
	\pgfusepath{draw}
	\pgfscope
	\pgfpathmoveto{\pgfpoint{.3\pgf@circ@res@left}{0pt}}
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
	\pgfpathlineto{\pgfpoint{.7\pgf@circ@res@right}{.5\pgf@circ@res@up}}
	\pgfusepath{draw}
	\endpgfscope
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
	\pgfpathlineto{\pgfpoint{.5\pgf@circ@res@right}{0}}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{.8\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{.5\pgf@circ@res@right}{.8\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{.5\pgf@circ@res@right}{.15\pgf@circ@res@up}}
	\pgfusepath{draw}
	
	
	\pgfpathmoveto{\pgfpoint{.2\pgf@circ@res@left}{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{.2\pgf@circ@res@right}{\pgf@circ@res@up}}
	\pgfusepath{draw}
	
	\pgfsetdash{{.08\pgf@circ@res@up}{.04\pgf@circ@res@up}{.7\pgf@circ@res@up}{.04\pgf@circ@res@up}{.8\pgf@circ@res@up}}{0cm}
	\pgfpathmoveto{\pgfpoint{0}{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{0}{.8\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{.2\pgf@circ@res@left}{.6\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{0}{.4\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{0}{.2\pgf@circ@res@up}}
	\pgfusepath{draw}
	\pgfsetdash{}{0cm}
}










\pgfdeclareshape{op amp}
	{
	  \anchor{center}{\pgfpointorigin}
	  \savedanchor\northwest{%
		\pgf@y= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/height}\pgf@y
		\pgf@y=.5\pgf@y
		\pgf@x= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/width}\pgf@x
		\pgf@x=.5\pgf@x
	  }
	  \anchor{south}{
		\northwest
		\pgf@y=-\pgf@y
	  }
	  \anchor{north}{
		\northwest
	  }
	  \savedanchor\left{%
	  	\pgf@y=0pt
	  }
	  \savedanchor\inOne{%
		\pgf@y= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/height}\pgf@y
		\pgf@y=.5\pgf@y
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@y
		\pgf@x= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/width}\pgf@x
		\pgf@x=.5\pgf@x
	  }	  
	  \anchor{-}{
		\inOne
	  }
	  \anchor{+}{
		\inOne
		\pgf@y=-\pgf@y
	  }
	  \savedanchor\up{%
		\pgf@y= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/height}\pgf@y
		\pgf@y=.5\pgf@y
		\pgf@x= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/width}\pgf@x
		\pgf@x=.5\pgf@x
			\pgf@circ@res@up = \pgf@y 
			\pgf@circ@res@right = -\pgf@x
			\pgf@circ@res@left = \pgf@x
	    \pgfpointlineattime{
			\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/up pos}}{
			\pgfpoint{
				\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/port width}\pgf@circ@res@left}
				{\pgf@circ@res@up}}
			{\pgfpoint{.7\pgf@circ@res@right}{0pt}}
	  }
	  \anchor{up}{
		\up
	  }
	  \anchor{down}{
		\up
		\pgf@y=-\pgf@y
	  }
	  \anchor{out}{
		\northwest
		\pgf@y=0pt
		\pgf@x=-\pgf@x
	  }
	  	\anchor{west}{
		  	\left
    	  }
		  \anchor{east}{
		  	\left
		  	\pgf@x=-\pgf@x
		  }  
	  
	  \backgroundpath{			
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}	
			
			
			\northwest
			\pgf@circ@res@up = \pgf@y 
			\pgf@circ@res@down = -\pgf@y
			\pgf@circ@res@right = -\pgf@x
			\pgf@circ@res@left = \pgf@x
			
	\pgfpathmoveto{\pgfpoint
		{\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/port width}\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@up}}
	\pgftext[left, at=\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/port width}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@up}]{\scriptsize\ $-$}
	

	\pgfpathmoveto{\pgfpoint
		{\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/port width}\pgf@circ@res@left}
		{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@down}}
	\pgftext[left, at=\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/port width}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@down}]{\scriptsize\ $+$}
		
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0pt}}
	\pgfpathlineto{\pgfpoint{.7\pgf@circ@res@right}{0pt}}
	
	\pgfusepath{draw}

						
	\pgfscope
		\pgfsetlinewidth{2\pgflinewidth}
		\pgftransformxshift{.7\pgf@circ@res@left}
		\pgf@circ@res@step=\pgf@circ@res@right
		\advance\pgf@circ@res@step by -\pgf@circ@res@left
		\pgf@circ@res@step=.7\pgf@circ@res@step
		
		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@step}{0pt}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{0pt}}
		\pgfusepath{draw}
	\endpgfscope
		
		
	  
	  }
	}
	



%% Potentiometer
\pgfcircdeclarebipole{
	\anchor{wiper}{
		\northeast
		\pgfpoint{0pt}{\pgf@y}
	}
	\anchor{W}{
		\northeast
		\pgfpoint{0pt}{\pgf@y}
	}	
}{\ctikzvalof{bipoles/potentiometer/height 2}}{potentiometer}{\ctikzvalof{bipoles/potentiometer/height}}{\ctikzvalof{bipoles/potentiometer/width}}{
		\pgf@circ@res@step = \ctikzvalof{bipoles/potentiometer/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 12

		\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@zero}}
		\pgf@circ@res@other = \pgf@circ@res@left
		\advance\pgf@circ@res@other by \pgf@circ@res@step 

		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{-\pgf@circ@res@down}}
		\advance\pgf@circ@res@other by 2\pgf@circ@res@step 
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\pgf@circ@res@down}}
		\advance\pgf@circ@res@other by 2\pgf@circ@res@step
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{-\pgf@circ@res@down}}
		\advance\pgf@circ@res@other by 2\pgf@circ@res@step
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\pgf@circ@res@down}}
		\advance\pgf@circ@res@other by 2\pgf@circ@res@step
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{-\pgf@circ@res@down}}
		\advance\pgf@circ@res@other by 2\pgf@circ@res@step
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\pgf@circ@res@down}}
		\advance\pgf@circ@res@other by \pgf@circ@res@step
		\pgfpathlineto{\pgfpoint{\pgf@circ@res@other}{\pgf@circ@res@zero}}
		\pgfusepath{draw} 
		
		\pgfscope
		%\pgfsetlinewidth{\pgfstartlinewidth}
		\pgfsetarrowsend{latex'}
		\pgfpathmoveto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{-\pgf@circ@res@down}}
		\pgfusepath{draw}
		\endpgfscope
}





%% Generic tunable 

\pgfcircdeclarebipole{
	\anchor{wiper}{
		\northeast
		\pgfpoint{0pt}{\pgf@y}
	}
}{\ctikzvalof{bipoles/generic potentiometer/height 2}}{genericpotentiometer}{\ctikzvalof{bipoles/generic potentiometer/height}}{\ctikzvalof{bipoles/generic potentiometer/width}}{

		\pgf@circ@res@step = \ctikzvalof{bipoles/resistor/width}\pgf@circ@Rlen
		\divide \pgf@circ@res@step by 14

		\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{-\pgf@circ@res@down}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
		\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
					
		\pgfusepath{draw} 
		
		\pgfscope
		%\pgfsetlinewidth{\pgfstartlinewidth}
		\pgfsetarrowsend{latex'}
		\pgfpathmoveto{\pgfpoint{0pt}{\pgf@circ@res@up}}
		\pgfpathlineto{\pgfpoint{0pt}{-\pgf@circ@res@down}}
		\pgfusepath{draw}
		\endpgfscope
}


\pgfdeclareshape{circulator}
{
	\savedanchor\northwest{
		\pgf@y= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/circulator/width}\pgf@y
		\pgf@y=.5\pgf@y
		\pgf@x= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/circulator/width}\pgf@x
		\pgf@x=.5\pgf@x
	}
	\anchor{center}{
		\pgfpointorigin
	}
	\anchor{left}{%
		\northwest
	  	\pgf@y=0pt
	}
	\anchor{1}{
		\northwest
		\pgf@y=0pt
	}	  
	\anchor{2}{
		\northwest
		\pgf@y=0pt
		\pgf@x=-\pgf@x
	}
	\anchor{3}{
		\northwest
		\pgf@y=-\pgf@y
		\pgf@x=0pt
	}
	\anchor{east}{
		\northwest
		\pgf@y=0pt
		\pgf@x=-\pgf@x  
	}
	\anchor{west}{
		\northwest
		\pgf@y=0pt
	}
	\anchor{south}{
		\northwest
		\pgf@x=0pt
		\pgf@y=-\pgf@y
	}
	\anchor{north}{
		\northwest
		\pgf@x=0pt
	}
	\anchor{south west}{
		\northwest
		\pgf@y=-\pgf@y
	}
	\anchor{north east}{
		\northwest
		\pgf@x=-\pgf@x
	}
	\anchor{north west}{
		\northwest
	}
	\anchor{south east}{
		\northwest
		\pgf@x=-\pgf@x
		\pgf@y=-\pgf@y
	}
	\backgroundpath{
		\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}	
			
		\pgf@circ@res@step=\ctikzvalof{tripoles/circulator/width}\pgf@circ@Rlen
			
		\pgfscope
			\pgfstartlinewidth=\pgflinewidth
			
			% draw outer circle
			\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
			\pgfpathcircle{\pgfpoint{0}{0}} {0.5\pgf@circ@res@step}
			\pgfusepath{draw}
			
			% inner arrow
			\pgfsetdash{}{0pt}	% always draw solid line for inner symbol
			\pgfsetlinewidth{\pgfstartlinewidth}
			\pgfsetarrowsend{latex}
			\pgfpathmoveto{\pgfpoint{-0.25\pgf@circ@res@step}{0}}
			\pgfpatharc{180}{-90} {0.25\pgf@circ@res@step}
			\pgfpathlineto{\pgfpoint{-5pt}{-0.2\pgf@circ@res@step}}
			\pgfusepath{draw}
		\endpgfscope				  
	}
}


% Wilkinson divider
\pgfdeclareshape{wilkinson}{
		\anchor{center}{
			\northwest
			\pgf@x=0pt
			\pgf@y=0pt
		}
		\savedanchor\northwest{%
			\pgf@y= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
			\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/wilkinson/height}\pgf@y
			\pgf@y=.5\pgf@y
			\pgf@x= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
			\pgf@x=.5\pgf@x
			\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/wilkinson/width}\pgf@x
			}
		\anchor{north}{
			\northwest
			\pgf@x=0pt
		}
		\anchor{south}{
			\northwest
			\pgf@x=0pt
			\pgf@y=-\pgf@y
		}
		\anchor{west}{
			\northwest
			\pgf@y=0pt
		}
		\anchor{east}{
			\northwest
			\pgf@y=0pt
			\pgf@x=-\pgf@x
		}
		\anchor{south west}{
			\northwest
			\pgf@y=-\pgf@y
		}
		\anchor{north east}{
			\northwest
			\pgf@x=-\pgf@x
		}
			\anchor{north west}{
			\northwest
		}
		\anchor{south east}{
			\northwest
			\pgf@x=-\pgf@x
			\pgf@y=-\pgf@y
		}
		\anchor{in}{
			\northwest
			\pgf@y=0pt
		}
		\anchor{out1}{
			\northwest
			\pgf@x=-\pgf@x
			\pgf@y=-0.5\pgf@y
		}
		\anchor{out2}{
			\northwest
			\pgf@x=-\pgf@x
			\pgf@y=0.5\pgf@y
		}
		\anchor{text}{
			\northwest
			\advance \pgf@y by 0.5\ht\pgfnodeparttextbox
			\pgf@x=-.5\wd\pgfnodeparttextbox
		}
		\backgroundpath{			
				\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}	
			
				\northwest
				\pgf@circ@res@up = \pgf@y 
				\pgf@circ@res@down = -\pgf@y
				\pgf@circ@res@right = -\pgf@x
				\pgf@circ@res@left = \pgf@x
			
				\pgfstartlinewidth=\pgflinewidth

				% draw outer box
				\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
				\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
				\pgfusepath{draw}
				
				% draw inner stuff
				\pgfsetlinewidth{\pgfstartlinewidth}
				\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0pt}}
				\pgfpathlineto{\pgfpoint{0.5\pgf@circ@res@left}{0pt}}
				\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{0.5\pgf@circ@res@up}}
				\pgfpathlineto{\pgfpoint{0.5\pgf@circ@res@right}{0.5\pgf@circ@res@up}}
				\pgfpathlineto{\pgfpoint{0.5\pgf@circ@res@left}{0pt}}
				\pgfpathlineto{\pgfpoint{0.5\pgf@circ@res@right}{0.5\pgf@circ@res@down}}
				\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{0.5\pgf@circ@res@down}}				
				
				\pgfusepath{draw}
				
				\pgfsetdash{}{0pt}	% always draw solid line for inner symbol
				% draw inner resisitor - european or american style is recognised
				{
					\pgftransformshift{\pgfpoint{0.5\pgf@circ@res@right}{0pt}}
					\pgftransformrotate{90}
					
					% calculate size of resistor
					\ifpgf@circuit@europeanresistor
						\pgfmathparse{\pgf@circ@res@up / \pgf@circ@Rlen / \ctikzvalof{bipoles/generic/width} / 2}
						\pgftransformscale{\pgfmathresult}
						\pgfnode{genericshape}{center}{}{pgf@generic}{\pgfusepath{fill}}
					\else
						\pgfmathparse{\pgf@circ@res@up / \pgf@circ@Rlen / \ctikzvalof{bipoles/resistor/width} / 2}
						\pgftransformscale{\pgfmathresult}
						\pgfnode{resistorshape}{center}{}{pgf@resistor}{\pgfusepath{fill}}
					\fi
				}
				
				\pgfpathmoveto{\pgfpoint{0.5\pgf@circ@res@right}{0.5\pgf@circ@res@up}}
				\pgfpathlineto{\pgfpoint{0.5\pgf@circ@res@right}{0.25\pgf@circ@res@up}}
				
				\pgfpathmoveto{\pgfpoint{0.5\pgf@circ@res@right}{0.25\pgf@circ@res@down}}
				\pgfpathlineto{\pgfpoint{0.5\pgf@circ@res@right}{0.5\pgf@circ@res@down}}
				\pgfusepath{draw}

		}
}


%%%---------- close: pgfcirctripoles
%%%%%%%%%%% Springe nach pgfcircquadpoles
%%%---------- open: pgfcircquadpoles.tex
% Copyright 2007-2009 by Massimo Redaelli
%
% This file may be distributed and/or modified
%
% 1. under the LaTeX Project Public License and/or
% 2. under the GNU Public License.
%
% See the file doc/LICENSE for more details.

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%% Quadripoles

\long\def\pgfcircdeclarequadpole#1#2#3{
	\pgfdeclareshape{#1}
	{
	  \anchor{center}{
	  	\northwest
		\pgf@x=0pt
	  }
	  \savedanchor\northwest{%
		\pgf@y= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/quadpoles/#1/height}\pgf@y
		\pgf@y=.5\pgf@y
		\pgf@x= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@x=.5\pgf@x
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/quadpoles/#1/width}\pgf@x
	  }
	  \anchor{A2}{
		\northwest
		\pgf@y=-\pgf@y
	  }
	  \anchor{B1}{
		\northwest
		\pgf@x=-\pgf@x
	  }
	  \anchor{A1}{
		\northwest
	  }
	  \anchor{B2}{
		\northwest
		\pgf@x=-\pgf@x
		\pgf@y=-\pgf@y
	  }
	  \anchor{north}{
	  	\northwest
		\pgf@x=0pt
	  }
	  \anchor{south}{
	  	\northwest
		\pgf@x=0pt
		\pgf@y=-\pgf@y
	  }
	  \anchor{west}{
	  	\northwest
		\pgf@y=0pt
	  }
	  \anchor{east}{
	  	\northwest
		\pgf@y=0pt
		\pgf@x=-\pgf@x
	  }
	  \anchor{south west}{
		\northwest
		\pgf@y=-\pgf@y
	  }
	  \anchor{north east}{
		\northwest
		\pgf@x=-\pgf@x
	  }
	  \anchor{north west}{
		\northwest
	  }
	  \anchor{south east}{
		\northwest
		\pgf@x=-\pgf@x
		\pgf@y=-\pgf@y
	  }	  
	  \anchor{base}{
	  	\northwest
		\pgf@x=0pt	  	
	  }
	  #3
	  \backgroundpath{			
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}	
			
			\northwest
			\pgf@circ@res@up = \pgf@y 
			\pgf@circ@res@down = -\pgf@y
			\pgf@circ@res@right = -\pgf@x
			\pgf@circ@res@left = \pgf@x
			
			%\pgf@circ@Rlen=\pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
			
			#2
	  
	  }
	}
}



\def\pgf@circ@drawtransformerbasicanchor{
	\pgfkeysvalueof{/tikz/circuitikz/quadpoles/trans/height}
	 \anchor{AA2}{
		\northwest
		\pgf@x=\pgfkeysvalueof{/tikz/circuitikz/quadpoles/transformer/width1}\pgf@x
		\pgf@x=.7\pgf@x
		\pgf@y=-\pgf@y
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/quadpoles/transformer/height1}\pgf@y
	  }
	  \anchor{BB1}{
		\northwest
		\pgf@x=-\pgf@x
		\pgf@x=\pgfkeysvalueof{/tikz/circuitikz/quadpoles/transformer/width1}\pgf@x
		\pgf@x=.7\pgf@x
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/quadpoles/transformer/height1}\pgf@y
	  }
	  \anchor{AA1}{
		\northwest
		\pgf@x=\pgfkeysvalueof{/tikz/circuitikz/quadpoles/transformer/width1}\pgf@x
		\pgf@x=.7\pgf@x
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/quadpoles/transformer/height1}\pgf@y
	  }
	  \anchor{BB2}{
		\northwest
		\pgf@x=-\pgf@x
		\pgf@x=\pgfkeysvalueof{/tikz/circuitikz/quadpoles/transformer/width1}\pgf@x
		\pgf@x=.7\pgf@x
		\pgf@y=-\pgf@y
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/quadpoles/transformer/height1}\pgf@y
	  }
}

\def\pgf@circ@drawtransformerbasicbody{
	\def\stretto{.4}
	\pgfscope             
			\pgfslopedattimetrue 
			\pgfallowupsidedownattimetrue
			\pgftransformlineattime{.5}{%
				\pgfpoint%
					{\stretto\pgf@circ@res@left}%
					{\pgf@circ@res@up}%
			}{%
				\pgfpoint
					{\stretto\pgf@circ@res@left}%
					{\pgf@circ@res@down}%
			}
			
			\edef\pgf@circ@temp{\ctikzvalof{inductor}}%
			\def\pgf@temp{european}%
			\ifx\pgf@temp\pgf@circ@temp%
				\pgfnode{fullgenericshape}{center}{}{pgf@inductor1}{\pgfusepath{stroke}}
			\else%
				\def\pgf@temp{cute}
				\ifx\pgf@temp\pgf@circ@temp%
					\pgfnode{cuteinductorshape}{center}{}{pgf@inductor1}{\pgfusepath{stroke}}
				\else%
					\pgfnode{americaninductorshape}{center}{}{pgf@inductor1}{\pgfusepath{stroke}}
				\fi%
			\fi%

			
	\endpgfscope
	\pgfscope             
			\pgfslopedattimetrue 
			\pgfallowupsidedownattimetrue
			\pgftransformlineattime{.5}{%
				\pgfpoint%
					{\stretto\pgf@circ@res@right}%
					{\pgf@circ@res@down}%
			}{%
				\pgfpoint
					{\stretto\pgf@circ@res@right}%
					{\pgf@circ@res@up}%
			}

			\edef\pgf@circ@temp{\ctikzvalof{inductor}}%
			\def\pgf@temp{european}%
			\ifx\pgf@temp\pgf@circ@temp%
				\pgfnode{fullgenericshape}{center}{}{pgf@inductor2}{\pgfusepath{stroke}}
			\else%
				\def\pgf@temp{cute} 
				\ifx\pgf@temp\pgf@circ@temp%
					\pgfnode{cuteinductorshape}{center}{}{pgf@inductor2}{\pgfusepath{stroke}}
				\else%
					\pgfnode{americaninductorshape}{center}{}{pgf@inductor2}{\pgfusepath{stroke}}
				\fi%
			\fi%
			
	\endpgfscope
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{\stretto\pgf@circ@res@left}{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpointanchor{pgf@inductor1}{b}}
	
	\pgfpathmoveto{\pgfpointanchor{pgf@inductor1}{a}}
	\pgfpathlineto{\pgfpoint{\stretto\pgf@circ@res@left}{\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@down}}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{\stretto\pgf@circ@res@right}{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpointanchor{pgf@inductor2}{a}}
	
	\pgfpathmoveto{\pgfpointanchor{pgf@inductor2}{b}}
	\pgfpathlineto{\pgfpoint{\stretto\pgf@circ@res@right}{\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
	
	\pgfusepath{draw}
	
}


	
	% contrib Kristofer M. Monisit
	
	\pgfdeclareshape{fd op amp}
	{
	  \anchor{center}{\pgfpointorigin}
	  \savedanchor\northwest{%
		\pgf@y= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/height}\pgf@y
		\pgf@y=.5\pgf@y
		\pgf@x= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/width}\pgf@x
		\pgf@x=.5\pgf@x
	  }
	  \anchor{south}{
		\northwest
		\pgf@y=-\pgf@y
	  }
	  \anchor{north}{
		\northwest
	  }
	  \savedanchor\left{%
	  	\pgf@y=0pt
	  }
	  \savedanchor\inOne{%
		\pgf@y= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/height}\pgf@y
		\pgf@y=.5\pgf@y
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@y
		\pgf@x= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/width}\pgf@x
		\pgf@x=.5\pgf@x
	  }
	  \anchor{-}{
		\inOne
	  }
	  \anchor{+}{
		\inOne
		\pgf@y=-\pgf@y
	  }
	  \savedanchor\up{%
		\pgf@y= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/height}\pgf@y
		\pgf@y=.5\pgf@y
		\pgf@x= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/width}\pgf@x
		\pgf@x=.5\pgf@x
			\pgf@circ@res@up = \pgf@y
			\pgf@circ@res@right = -\pgf@x
			\pgf@circ@res@left = \pgf@x
	    \pgfpointlineattime{
			\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/up pos}}{
			\pgfpoint{
				\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/port width}\pgf@circ@res@left}
				{\pgf@circ@res@up}}
			{\pgfpoint{.7\pgf@circ@res@right}{0pt}}
	  }
	  \anchor{up}{
		\up
	  }
	  \anchor{down}{
		\up
		\pgf@y=-\pgf@y
	  }
	  \anchor{out +}{
		\northwest
		\pgf@y=.5\pgf@y
		\pgf@x=-.7\pgf@x
	  }
	  \anchor{out -}{
		\northwest
		\pgf@y=-.5\pgf@y
		\pgf@x=-.7\pgf@x
	  }
	  \anchor{west}{
	  	\left
      }
		\anchor{east}{
			\left
			\pgf@x=-\pgf@x
		}

	  \backgroundpath{
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}

      \northwest
      \pgf@circ@res@up = \pgf@y
      \pgf@circ@res@down = -\pgf@y
      \pgf@circ@res@right = -\pgf@x
      \pgf@circ@res@left = \pgf@x

      % Negative input terminal
      \pgfpathmoveto{\pgfpoint
        {\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@up}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/port width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@up}}
      \pgftext[left, at=\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/port width}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@up}]{\scriptsize\ $-$}
  

      % Positive input terminal
      \pgfpathmoveto{\pgfpoint
        {\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@down}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/port width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@down}}
      \pgftext[left, at=\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/port width}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@down}]{\scriptsize\ $+$}
  

      % Negative output terminal
      \pgfpathmoveto{\pgfpoint
        {0.7\pgf@circ@res@right}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@down}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/port width}}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@down}}
      \pgftext[left, at=\pgfpoint{0.3\pgf@circ@res@left}{.3\pgf@circ@res@down}]{\scriptsize\ $-$}
  

      % Positive output terminal
      \pgfpathmoveto{\pgfpoint
        {0.7\pgf@circ@res@right}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@up}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/port width}}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@up}}
      \pgftext[left, at=\pgfpoint{0.3\pgf@circ@res@left}{.3\pgf@circ@res@up}]{\scriptsize\ $+$}
  

      % Draw them all!
      \pgfusepath{draw}

      % Triangle
      \pgfscope
        \pgfsetlinewidth{2\pgflinewidth}
        \pgftransformxshift{.7\pgf@circ@res@left}
        \pgf@circ@res@step=\pgf@circ@res@right
        \advance\pgf@circ@res@step by -\pgf@circ@res@left
        \pgf@circ@res@step=.7\pgf@circ@res@step
        \pgfpathmoveto{\pgfpoint{\pgf@circ@res@step}{0pt}}
        \pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
        \pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
        \pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{0pt}}
        \pgfusepath{draw}
      \endpgfscope
	  }
	}




\pgfcircdeclarequadpole{transformer}{

	\pgf@circ@drawtransformerbasicbody

}{\pgf@circ@drawtransformerbasicanchor}

\pgfcircdeclarequadpole{transformer core}{

	\pgf@circ@drawtransformerbasicbody
	
	\pgfmoveto{\pgfpoint%
					{\ctikzvalof{quadpoles/transformer core/core width}\pgf@circ@res@right}%
					{\ctikzvalof{quadpoles/transformer core/core height}\pgf@circ@res@down}%
					}
	\pgflineto{
				\pgfpoint
					{\ctikzvalof{quadpoles/transformer core/core width}\pgf@circ@res@right}%
					{\ctikzvalof{quadpoles/transformer core/core height}\pgf@circ@res@up}%
					}

	\pgfmoveto{\pgfpoint%
					{\ctikzvalof{quadpoles/transformer core/core width}\pgf@circ@res@left}%
					{\ctikzvalof{quadpoles/transformer core/core height}\pgf@circ@res@down}%
					}
	\pgflineto{
				\pgfpoint
					{\ctikzvalof{quadpoles/transformer core/core width}\pgf@circ@res@left}%
					{\ctikzvalof{quadpoles/transformer core/core height}\pgf@circ@res@up}%
					}					
	
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgflinewidth}
	\pgfusepath{draw}
}{\pgf@circ@drawtransformerbasicanchor}


\pgfcircdeclarequadpole{gyrator}{

	\def\stretto{.4}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{\stretto\pgf@circ@res@left}{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{\stretto\pgf@circ@res@left}{\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@down}}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{\stretto\pgf@circ@res@right}{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{\stretto\pgf@circ@res@right}{\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
	
	\pgfusepath{draw}
	
	\pgfsetlinewidth{2\pgflinewidth}
	\pgfpathmoveto{\pgfpoint{\stretto\pgf@circ@res@left}{.7*\stretto\pgf@circ@res@down}}
	\pgfpatharc{90}{270}{.7*\stretto\pgf@circ@res@down}
	
	\pgfpathmoveto{\pgfpoint{\stretto\pgf@circ@res@right}{.7*\stretto\pgf@circ@res@up}}
	\pgfpatharc{-90}{90}{.7*\stretto\pgf@circ@res@down}
	\pgfusepath{draw}

}{}

%% coupler
% defines a general outer box for couplers
% TikZ usage: 
%		\draw (0,0) node[coupler](coup){\SI{-3}{dB}}
%		(coup.port1) to[short,-o] ++(-1,0)
%

\long\def\pgfcircdeclarecoupler#1#2{
	\pgfdeclareshape{#1}{
		\anchor{center}{
			\northwest
			\pgf@x=0pt
			\pgf@y=0pt
		}
		\savedanchor\northwest{%
			\pgf@y= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
			\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/quadpoles/coupler/height}\pgf@y
			\pgf@y=.5\pgf@y
			\pgf@x= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
			\pgf@x=.5\pgf@x
			\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/quadpoles/coupler/width}\pgf@x
			}
		\anchor{north}{
			\northwest
			\pgf@x=0pt
		}
		\anchor{south}{
			\northwest
			\pgf@x=0pt
			\pgf@y=-\pgf@y
		}
		\anchor{west}{
			\northwest
			\pgf@y=0pt
		}
		\anchor{east}{
			\northwest
			\pgf@y=0pt
			\pgf@x=-\pgf@x
		}
		\anchor{south west}{
			\northwest
			\pgf@y=-\pgf@y
		}
		\anchor{north east}{
			\northwest
			\pgf@x=-\pgf@x
		}
			\anchor{north west}{
			\northwest
		}
		\anchor{south east}{
			\northwest
			\pgf@x=-\pgf@x
			\pgf@y=-\pgf@y
		}
		\anchor{port1}{
			\northwest
			\pgf@y=-0.5\pgf@y
		}
		\anchor{port2}{
			\northwest
			\pgf@x=-\pgf@x
			\pgf@y=-0.5\pgf@y
		}
		\anchor{port3}{
			\northwest
			\pgf@x=-\pgf@x
			\pgf@y=0.5\pgf@y
		}
		\anchor{port4}{
			\northwest
			\pgf@y=0.5\pgf@y
		}
		\anchor{1}{
			\northwest
			\pgf@y=-0.5\pgf@y
		}
		\anchor{2}{
			\northwest
			\pgf@x=-\pgf@x
			\pgf@y=-0.5\pgf@y
		}
		\anchor{3}{
			\northwest
			\pgf@x=-\pgf@x
			\pgf@y=0.5\pgf@y
		}
		\anchor{4}{
			\northwest
			\pgf@y=0.5\pgf@y
		}
		\anchor{text}{
			\northwest
			\advance \pgf@y by 0.5\ht\pgfnodeparttextbox
			\pgf@x=-.5\wd\pgfnodeparttextbox
		}
		\backgroundpath{			
				\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}	
			
				\northwest
				\pgf@circ@res@up = \pgf@y 
				\pgf@circ@res@down = -\pgf@y
				\pgf@circ@res@right = -\pgf@x
				\pgf@circ@res@left = \pgf@x
			
				\pgfstartlinewidth=\pgflinewidth

				% draw outer box
				\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
				\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
				\pgfusepath{draw}
				
				% draw inner stuff
				#2

		}
	}
}

% straight coupler
\pgfcircdeclarecoupler{coupler}{
	\pgfsetlinewidth{\pgfstartlinewidth}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0.5\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{0.5\pgf@circ@res@up}}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0.5\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{0.5\pgf@circ@res@down}}
	\pgfusepath{draw}
	
	\pgfpathmoveto{\pgfpoint{0.7\pgf@circ@res@left}{0.4\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{0.7\pgf@circ@res@right}{0.4\pgf@circ@res@up}}
	\pgfsetarrows{latex-latex}
	\pgfusepath{draw}
	\pgfpathmoveto{\pgfpoint{0.7\pgf@circ@res@left}{0.4\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{0.7\pgf@circ@res@right}{0.4\pgf@circ@res@down}}
	\pgfsetarrows{latex-latex}
	\pgfusepath{draw}
}

% "bended" coupler
\pgfcircdeclarecoupler{coupler2}{
	\pgfsetlinewidth{\pgfstartlinewidth}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0.5\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{0.5\pgf@circ@res@up}}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0.5\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{0.5\pgf@circ@res@down}}
	\pgfusepath{draw}
	
	\pgfpathmoveto{\pgfpoint{0.1\pgf@circ@res@left}{0pt}}
	\pgfpatharc{0}{90} {0.4\pgf@circ@res@up}
	\pgfsetarrowsend{latex}
	\pgfusepath{draw}
	\pgfpathmoveto{\pgfpoint{0.1\pgf@circ@res@left}{0pt}}
	\pgfpatharc{0}{-90} {0.4\pgf@circ@res@up}
	\pgfsetarrowsend{latex}
	\pgfusepath{draw}
	
	\pgfpathmoveto{\pgfpoint{0.1\pgf@circ@res@right}{0pt}}
	\pgfpatharc{180}{90} {0.4\pgf@circ@res@up}
	\pgfsetarrowsend{latex}
	\pgfusepath{draw}
	\pgfpathmoveto{\pgfpoint{0.1\pgf@circ@res@right}{0pt}}
	\pgfpatharc{-180}{-90} {0.4\pgf@circ@res@up}
	\pgfsetarrowsend{latex}
	\pgfusepath{draw}
	
	
}

%%%---------- close: pgfcircquadpoles
%%%%%%%%%%% Springe nach pgfcircnpoles
%%%---------- open: pgfcircnpoles.tex
%
% This file may be distributed and/or modified
%
% 1. under the LaTeX Project Public License and/or
% 2. under the GNU Public License.
%
% See the file doc/LICENSE for more details.

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%% N-poles

\pgfkeys{/tikz/circuitikz,lab/.code={
	

}}

\long\def\pgfcircdeclarenpole#1#2#3{
	\pgfdeclareshape{#1}
	{
	  \anchor{center}{
	  	\northwest
		\pgf@x=0pt
	  }
	  \savedanchor\northwest{%
		\pgf@y= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/quadpoles/#1/height}\pgf@y
		\pgf@y=.5\pgf@y
		\pgf@x= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@x=.5\pgf@x
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/quadpoles/#1/width}\pgf@x
	  }
	  \anchor{A2}{
		\northwest
		\pgf@y=-\pgf@y
	  }
	  \anchor{B1}{
		\northwest
		\pgf@x=-\pgf@x
	  }
	  \anchor{A1}{
		\northwest
	  }
	  \anchor{B2}{
		\northwest
		\pgf@x=-\pgf@x
		\pgf@y=-\pgf@y
	  }
	  \anchor{north}{
	  	\northwest
		\pgf@x=0pt
	  }
	  \anchor{south}{
	  	\northwest
		\pgf@x=0pt
		\pgf@y=-\pgf@y
	  }
	  \anchor{west}{
	  	\northwest
		\pgf@y=0pt
	  }
	  \anchor{east}{
	  	\northwest
		\pgf@y=0pt
		\pgf@x=-\pgf@x
	  }
	  \anchor{south west}{
		\northwest
		\pgf@y=-\pgf@y
	  }
	  \anchor{north east}{
		\northwest
		\pgf@x=-\pgf@x
	  }
	  \anchor{north west}{
		\northwest
	  }
	  \anchor{south east}{
		\northwest
		\pgf@x=-\pgf@x
		\pgf@y=-\pgf@y
	  }	  
	  \anchor{base}{
	  	\northwest
		\pgf@x=0pt	  	
	  }
	  #3
	  \backgroundpath{			
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}	
			
			\northwest
			\pgf@circ@res@up = \pgf@y 
			\pgf@circ@res@down = -\pgf@y
			\pgf@circ@res@right = -\pgf@x
			\pgf@circ@res@left = \pgf@x
			
			%\pgf@circ@Rlen=\pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
			
			#2
	  
	  }
	}
}



\def\pgf@circ@drawtransformerbasicanchor{
	\pgfkeysvalueof{/tikz/circuitikz/quadpoles/trans/height}
	 \anchor{AA2}{
		\northwest
		\pgf@x=\pgfkeysvalueof{/tikz/circuitikz/quadpoles/transformer/width1}\pgf@x
		\pgf@x=.7\pgf@x
		\pgf@y=-\pgf@y
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/quadpoles/transformer/height1}\pgf@y
	  }
	  \anchor{BB1}{
		\northwest
		\pgf@x=-\pgf@x
		\pgf@x=\pgfkeysvalueof{/tikz/circuitikz/quadpoles/transformer/width1}\pgf@x
		\pgf@x=.7\pgf@x
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/quadpoles/transformer/height1}\pgf@y
	  }
	  \anchor{AA1}{
		\northwest
		\pgf@x=\pgfkeysvalueof{/tikz/circuitikz/quadpoles/transformer/width1}\pgf@x
		\pgf@x=.7\pgf@x
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/quadpoles/transformer/height1}\pgf@y
	  }
	  \anchor{BB2}{
		\northwest
		\pgf@x=-\pgf@x
		\pgf@x=\pgfkeysvalueof{/tikz/circuitikz/quadpoles/transformer/width1}\pgf@x
		\pgf@x=.7\pgf@x
		\pgf@y=-\pgf@y
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/quadpoles/transformer/height1}\pgf@y
	  }
}

\def\pgf@circ@drawtransformerbasicbody{
	\def\stretto{.4}
	\pgfscope             
			\pgfslopedattimetrue 
			\pgfallowupsidedownattimetrue
			\pgftransformlineattime{.5}{%
				\pgfpoint%
					{\stretto\pgf@circ@res@left}%
					{\pgf@circ@res@up}%
			}{%
				\pgfpoint
					{\stretto\pgf@circ@res@left}%
					{\pgf@circ@res@down}%
			}
			
			\edef\pgf@circ@temp{\ctikzvalof{inductor}}%
			\def\pgf@temp{european}%
			\ifx\pgf@temp\pgf@circ@temp%
				\pgfnode{fullgenericshape}{center}{}{pgf@inductor1}{\pgfusepath{stroke}}
			\else%
				\def\pgf@temp{cute}
				\ifx\pgf@temp\pgf@circ@temp%
					\pgfnode{cuteinductorshape}{center}{}{pgf@inductor1}{\pgfusepath{stroke}}
				\else%
					\pgfnode{americaninductorshape}{center}{}{pgf@inductor1}{\pgfusepath{stroke}}
				\fi%
			\fi%

			
	\endpgfscope
	\pgfscope             
			\pgfslopedattimetrue 
			\pgfallowupsidedownattimetrue
			\pgftransformlineattime{.5}{%
				\pgfpoint%
					{\stretto\pgf@circ@res@right}%
					{\pgf@circ@res@down}%
			}{%
				\pgfpoint
					{\stretto\pgf@circ@res@right}%
					{\pgf@circ@res@up}%
			}

			\edef\pgf@circ@temp{\ctikzvalof{inductor}}%
			\def\pgf@temp{european}%
			\ifx\pgf@temp\pgf@circ@temp%
				\pgfnode{fullgenericshape}{center}{}{pgf@inductor2}{\pgfusepath{stroke}}
			\else%
				\def\pgf@temp{cute} 
				\ifx\pgf@temp\pgf@circ@temp%
					\pgfnode{cuteinductorshape}{center}{}{pgf@inductor2}{\pgfusepath{stroke}}
				\else%
					\pgfnode{americaninductorshape}{center}{}{pgf@inductor2}{\pgfusepath{stroke}}
				\fi%
			\fi%
			
	\endpgfscope
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{\stretto\pgf@circ@res@left}{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpointanchor{pgf@inductor1}{b}}
	
	\pgfpathmoveto{\pgfpointanchor{pgf@inductor1}{a}}
	\pgfpathlineto{\pgfpoint{\stretto\pgf@circ@res@left}{\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@down}}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{\stretto\pgf@circ@res@right}{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpointanchor{pgf@inductor2}{a}}
	
	\pgfpathmoveto{\pgfpointanchor{pgf@inductor2}{b}}
	\pgfpathlineto{\pgfpoint{\stretto\pgf@circ@res@right}{\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
	
	\pgfusepath{draw}
	
}


	
	% contrib Kristofer M. Monisit
	
	\pgfdeclareshape{fd op amp}
	{
	  \anchor{center}{\pgfpointorigin}
	  \savedanchor\northwest{%
		\pgf@y= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/height}\pgf@y
		\pgf@y=.5\pgf@y
		\pgf@x= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/width}\pgf@x
		\pgf@x=.5\pgf@x
	  }
	  \anchor{south}{
		\northwest
		\pgf@y=-\pgf@y
	  }
	  \anchor{north}{
		\northwest
	  }
	  \savedanchor\left{%
	  	\pgf@y=0pt
	  }
	  \savedanchor\inOne{%
		\pgf@y= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/height}\pgf@y
		\pgf@y=.5\pgf@y
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@y
		\pgf@x= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/width}\pgf@x
		\pgf@x=.5\pgf@x
	  }
	  \anchor{-}{
		\inOne
	  }
	  \anchor{+}{
		\inOne
		\pgf@y=-\pgf@y
	  }
	  \savedanchor\up{%
		\pgf@y= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/height}\pgf@y
		\pgf@y=.5\pgf@y
		\pgf@x= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
		\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/width}\pgf@x
		\pgf@x=.5\pgf@x
			\pgf@circ@res@up = \pgf@y
			\pgf@circ@res@right = -\pgf@x
			\pgf@circ@res@left = \pgf@x
	    \pgfpointlineattime{
			\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/up pos}}{
			\pgfpoint{
				\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/port width}\pgf@circ@res@left}
				{\pgf@circ@res@up}}
			{\pgfpoint{.7\pgf@circ@res@right}{0pt}}
	  }
	  \anchor{up}{
		\up
	  }
	  \anchor{down}{
		\up
		\pgf@y=-\pgf@y
	  }
	  \anchor{out +}{
		\northwest
		\pgf@y=.5\pgf@y
		\pgf@x=-.7\pgf@x
	  }
	  \anchor{out -}{
		\northwest
		\pgf@y=-.5\pgf@y
		\pgf@x=-.7\pgf@x
	  }
	  \anchor{west}{
	  	\left
      }
		\anchor{east}{
			\left
			\pgf@x=-\pgf@x
		}

	  \backgroundpath{
			\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}

      \northwest
      \pgf@circ@res@up = \pgf@y
      \pgf@circ@res@down = -\pgf@y
      \pgf@circ@res@right = -\pgf@x
      \pgf@circ@res@left = \pgf@x

      % Negative input terminal
      \pgfpathmoveto{\pgfpoint
        {\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@up}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/port width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@up}}
      \pgftext[left, at=\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/port width}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@up}]{\scriptsize\ $-$}
  

      % Positive input terminal
      \pgfpathmoveto{\pgfpoint
        {\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@down}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/port width}\pgf@circ@res@left}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@down}}
      \pgftext[left, at=\pgfpoint{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/port width}\pgf@circ@res@left}{\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@down}]{\scriptsize\ $+$}
  

      % Negative output terminal
      \pgfpathmoveto{\pgfpoint
        {0.7\pgf@circ@res@right}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@down}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/port width}}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@down}}
      \pgftext[left, at=\pgfpoint{0.3\pgf@circ@res@left}{.3\pgf@circ@res@down}]{\scriptsize\ $-$}
  

      % Positive output terminal
      \pgfpathmoveto{\pgfpoint
        {0.7\pgf@circ@res@right}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@up}}
      \pgfpathlineto{\pgfpoint
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/port width}}
        {\pgfkeysvalueof{/tikz/circuitikz/tripoles/op amp/input height}\pgf@circ@res@up}}
      \pgftext[left, at=\pgfpoint{0.3\pgf@circ@res@left}{.3\pgf@circ@res@up}]{\scriptsize\ $+$}
  

      % Draw them all!
      \pgfusepath{draw}

      % Triangle
      \pgfscope
        \pgfsetlinewidth{2\pgflinewidth}
        \pgftransformxshift{.7\pgf@circ@res@left}
        \pgf@circ@res@step=\pgf@circ@res@right
        \advance\pgf@circ@res@step by -\pgf@circ@res@left
        \pgf@circ@res@step=.7\pgf@circ@res@step
        \pgfpathmoveto{\pgfpoint{\pgf@circ@res@step}{0pt}}
        \pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@up}}
        \pgfpathlineto{\pgfpoint{0pt}{\pgf@circ@res@down}}
        \pgfpathlineto{\pgfpoint{\pgf@circ@res@step}{0pt}}
        \pgfusepath{draw}
      \endpgfscope
	  }
	}




\pgfcircdeclarequadpole{transformer}{

	\pgf@circ@drawtransformerbasicbody

}{\pgf@circ@drawtransformerbasicanchor}

\pgfcircdeclarequadpole{transformer core}{

	\pgf@circ@drawtransformerbasicbody
	
	\pgfmoveto{\pgfpoint%
					{\ctikzvalof{quadpoles/transformer core/core width}\pgf@circ@res@right}%
					{\ctikzvalof{quadpoles/transformer core/core height}\pgf@circ@res@down}%
					}
	\pgflineto{
				\pgfpoint
					{\ctikzvalof{quadpoles/transformer core/core width}\pgf@circ@res@right}%
					{\ctikzvalof{quadpoles/transformer core/core height}\pgf@circ@res@up}%
					}

	\pgfmoveto{\pgfpoint%
					{\ctikzvalof{quadpoles/transformer core/core width}\pgf@circ@res@left}%
					{\ctikzvalof{quadpoles/transformer core/core height}\pgf@circ@res@down}%
					}
	\pgflineto{
				\pgfpoint
					{\ctikzvalof{quadpoles/transformer core/core width}\pgf@circ@res@left}%
					{\ctikzvalof{quadpoles/transformer core/core height}\pgf@circ@res@up}%
					}					
	
	\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgflinewidth}
	\pgfusepath{draw}
}{\pgf@circ@drawtransformerbasicanchor}


\pgfcircdeclarequadpole{gyrator}{

	\def\stretto{.4}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{\stretto\pgf@circ@res@left}{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{\stretto\pgf@circ@res@left}{\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@down}}
	
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{\stretto\pgf@circ@res@right}{\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{\stretto\pgf@circ@res@right}{\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
	
	\pgfusepath{draw}
	
	\pgfsetlinewidth{2\pgflinewidth}
	\pgfpathmoveto{\pgfpoint{\stretto\pgf@circ@res@left}{.7*\stretto\pgf@circ@res@down}}
	\pgfpatharc{90}{270}{.7*\stretto\pgf@circ@res@down}
	
	\pgfpathmoveto{\pgfpoint{\stretto\pgf@circ@res@right}{.7*\stretto\pgf@circ@res@up}}
	\pgfpatharc{-90}{90}{.7*\stretto\pgf@circ@res@down}
	\pgfusepath{draw}

}{}

%% coupler
% defines a general outer box for couplers
% TikZ usage: 
%		\draw (0,0) node[coupler](coup){\SI{-3}{dB}}
%		(coup.port1) to[short,-o] ++(-1,0)
%

\long\def\pgfcircdeclarecoupler#1#2{
	\pgfdeclareshape{#1}{
		\anchor{center}{
			\northwest
			\pgf@x=0pt
			\pgf@y=0pt
		}
		\savedanchor\northwest{%
			\pgf@y= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
			\pgf@y=\pgfkeysvalueof{/tikz/circuitikz/quadpoles/coupler/height}\pgf@y
			\pgf@y=.5\pgf@y
			\pgf@x= \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}
			\pgf@x=.5\pgf@x
			\pgf@x=-\pgfkeysvalueof{/tikz/circuitikz/quadpoles/coupler/width}\pgf@x
			}
		\anchor{north}{
			\northwest
			\pgf@x=0pt
		}
		\anchor{south}{
			\northwest
			\pgf@x=0pt
			\pgf@y=-\pgf@y
		}
		\anchor{west}{
			\northwest
			\pgf@y=0pt
		}
		\anchor{east}{
			\northwest
			\pgf@y=0pt
			\pgf@x=-\pgf@x
		}
		\anchor{south west}{
			\northwest
			\pgf@y=-\pgf@y
		}
		\anchor{north east}{
			\northwest
			\pgf@x=-\pgf@x
		}
			\anchor{north west}{
			\northwest
		}
		\anchor{south east}{
			\northwest
			\pgf@x=-\pgf@x
			\pgf@y=-\pgf@y
		}
		\anchor{port1}{
			\northwest
			\pgf@y=-0.5\pgf@y
		}
		\anchor{port2}{
			\northwest
			\pgf@x=-\pgf@x
			\pgf@y=-0.5\pgf@y
		}
		\anchor{port3}{
			\northwest
			\pgf@x=-\pgf@x
			\pgf@y=0.5\pgf@y
		}
		\anchor{port4}{
			\northwest
			\pgf@y=0.5\pgf@y
		}
		\anchor{1}{
			\northwest
			\pgf@y=-0.5\pgf@y
		}
		\anchor{2}{
			\northwest
			\pgf@x=-\pgf@x
			\pgf@y=-0.5\pgf@y
		}
		\anchor{3}{
			\northwest
			\pgf@x=-\pgf@x
			\pgf@y=0.5\pgf@y
		}
		\anchor{4}{
			\northwest
			\pgf@y=0.5\pgf@y
		}
		\anchor{text}{
			\northwest
			\advance \pgf@y by 0.5\ht\pgfnodeparttextbox
			\pgf@x=-.5\wd\pgfnodeparttextbox
		}
		\backgroundpath{			
				\pgfsetcolor{\pgfkeysvalueof{/tikz/circuitikz/color}}	
			
				\northwest
				\pgf@circ@res@up = \pgf@y 
				\pgf@circ@res@down = -\pgf@y
				\pgf@circ@res@right = -\pgf@x
				\pgf@circ@res@left = \pgf@x
			
				\pgfstartlinewidth=\pgflinewidth

				% draw outer box
				\pgfsetlinewidth{\pgfkeysvalueof{/tikz/circuitikz/bipoles/thickness}\pgfstartlinewidth}
				\pgfpathrectanglecorners{\pgfpoint{\pgf@circ@res@left}{\pgf@circ@res@up}}{\pgfpoint{\pgf@circ@res@right}{\pgf@circ@res@down}}
				\pgfusepath{draw}
				
				% draw inner stuff
				#2

		}
	}
}

% straight coupler
\pgfcircdeclarecoupler{coupler}{
	\pgfsetlinewidth{\pgfstartlinewidth}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0.5\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{0.5\pgf@circ@res@up}}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0.5\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{0.5\pgf@circ@res@down}}
	\pgfusepath{draw}
	
	\pgfpathmoveto{\pgfpoint{0.7\pgf@circ@res@left}{0.4\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{0.7\pgf@circ@res@right}{0.4\pgf@circ@res@up}}
	\pgfsetarrows{latex-latex}
	\pgfusepath{draw}
	\pgfpathmoveto{\pgfpoint{0.7\pgf@circ@res@left}{0.4\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{0.7\pgf@circ@res@right}{0.4\pgf@circ@res@down}}
	\pgfsetarrows{latex-latex}
	\pgfusepath{draw}
}

% "bended" coupler
\pgfcircdeclarecoupler{coupler2}{
	\pgfsetlinewidth{\pgfstartlinewidth}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0.5\pgf@circ@res@up}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{0.5\pgf@circ@res@up}}
	\pgfpathmoveto{\pgfpoint{\pgf@circ@res@left}{0.5\pgf@circ@res@down}}
	\pgfpathlineto{\pgfpoint{\pgf@circ@res@right}{0.5\pgf@circ@res@down}}
	\pgfusepath{draw}
	
	\pgfpathmoveto{\pgfpoint{0.1\pgf@circ@res@left}{0pt}}
	\pgfpatharc{0}{90} {0.4\pgf@circ@res@up}
	\pgfsetarrowsend{latex}
	\pgfusepath{draw}
	\pgfpathmoveto{\pgfpoint{0.1\pgf@circ@res@left}{0pt}}
	\pgfpatharc{0}{-90} {0.4\pgf@circ@res@up}
	\pgfsetarrowsend{latex}
	\pgfusepath{draw}
	
	\pgfpathmoveto{\pgfpoint{0.1\pgf@circ@res@right}{0pt}}
	\pgfpatharc{180}{90} {0.4\pgf@circ@res@up}
	\pgfsetarrowsend{latex}
	\pgfusepath{draw}
	\pgfpathmoveto{\pgfpoint{0.1\pgf@circ@res@right}{0pt}}
	\pgfpatharc{-180}{-90} {0.4\pgf@circ@res@up}
	\pgfsetarrowsend{latex}
	\pgfusepath{draw}
	
	
}

%%%---------- close: pgfcircnpoles

%%%%%%%%%%% Springe nach pgfcirclabel
%%%---------- open: pgfcirclabel.tex
% Copyright 2007-2009 by Massimo Redaelli
%
% This file may be distributed and/or modified
%
% 1. under the LaTeX Project Public License and/or
% 2. under the GNU Public License.
%
% See the file doc/LICENSE for more details.

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%% Bipole label positioning

%% Options
\ctikzset{label/.style = { l=#1 } }
\ctikzset{l/.code = { 
	\pgfkeys{/tikz/circuitikz/bipole/label/name=#1}
	\ctikzsetvalof{bipole/label/unit}{}
	\ifpgf@circ@siunitx 
		\pgf@circ@handleSI{#1}
		\ifpgf@circ@siunitx@res 
			\edef\pgf@temp{\pgf@circ@handleSI@val}
			\pgfkeyslet{/tikz/circuitikz/bipole/label/name}{\pgf@temp}
			\edef\pgf@temp{\pgf@circ@handleSI@unit}
			\pgfkeyslet{/tikz/circuitikz/bipole/label/unit}{\pgf@temp}
		\else
		\fi
	\else
	\fi
}}

\ctikzset{label above/.code = { 
	l=#1, 
	\circuitikzbasekey/bipole/label/position=90 }
}
\ctikzset{l^/.style = { 
	l=#1,
	\circuitikzbasekey/bipole/label/position=90 } 
}

\ctikzset{label below/.code = { 
	l=#1,
	\circuitikzbasekey/bipole/label/position=-90 } 
}
\ctikzset{l_/.style = { 
	l=#1,
	\circuitikzbasekey/bipole/label/position=-90 } 
}



\def\pgf@circ@drawlabel{
		\pgfextra{
			\edef\pgf@temp{\ctikzvalof{label/align}}
			\def\pgf@circ@temp{straight}
		}
		\ifx\pgf@temp\pgf@circ@temp %straight
			\pgf@circ@drawreglabel
		\else
			\pgfextra{\def\pgf@circ@temp{rotate}}
			\ifx\pgf@temp\pgf@circ@temp %rotate
				\pgf@circ@drawrotlabel
			\else % smart
				\pgf@circ@drawsmartlabel				
			\fi
		\fi
}

\def\pgf@circ@drawsmartlabel{
	\pgfextra{
		%\pgfmathadd{\pgf@circ@direction}{360}
		\pgfmathmod{\pgf@circ@direction}{90}
		\edef\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgfmathresult\pgf@nil}
	}
	\ifnum \pgfcircmathresult > 20 
		\ifnum \pgfcircmathresult < 70 % NON quasi retto
			\pgf@circ@drawrotlabel
		\else
			\pgf@circ@drawreglabel
		\fi
	\else 
		\pgf@circ@drawreglabel
	\fi
}

%% Output routing
%% #1 - node name

\def\pgf@circ@drawrotlabel{
	\pgfextra{
		% calcolo rotazione label
		\def\pgf@circ@temp{\ctikzvalof{bipole/label/position}} %%% àncora label
		\edef\pgfcirclabrot{\pgf@circ@direction} % primo e quarto quadrante
		\edef\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgf@circ@direction\pgf@nil}
		\ifnum \pgfcircmathresult > 90 \ifnum \pgfcircmathresult < 270 % terzo e secondo
			\pgfmathsubtract{\pgf@circ@direction}{180}
			\edef\pgfcirclabrot{\expandafter\pgf@circ@stripdecimals\pgfmathresult\pgf@nil}
			\pgfmathadd{\pgf@circ@temp}{180} %%%
			\edef\pgf@circ@temp{\expandafter\pgf@circ@stripdecimals\pgfmathresult\pgf@nil} %%%
		\fi\fi
		
		\ifnum \ctikzvalof{mirror value} = -1
			\pgfmathadd{\pgf@circ@temp}{180}
			\edef\pgf@circ@temp{\expandafter\pgf@circ@stripdecimals\pgfmathresult\pgf@nil}
		\fi
	}
	coordinate (labelcoor) at ($(\ctikzvalof{bipole/name})!2!(\ctikzvalof{bipole/name}.north)$)
	(labelcoor) node [rotate=\pgfcirclabrot] {\pgf@circ@finallabel{}} % c'era un transform shape
}

\def\pgf@circ@drawreglabel{
	\pgfextra{
		\pgfmathsubtract{\pgf@circ@direction}{90}
		\edef\pgf@circ@labanc{\expandafter\pgf@circ@stripdecimals\pgfmathresult\pgf@nil}
		
		\edef\pgf@circ@temp{\ctikzvalof{bipole/label/position}} %%% àncora label
		\ifnum \pgf@circ@temp < 0
			\pgfmathadd{\pgf@circ@labanc}{180}
			\edef\pgf@circ@labanc{\expandafter\pgf@circ@stripdecimals\pgfmathresult\pgf@nil}
		\fi
		
		\ifnum \ctikzvalof{mirror value} = -1
			\pgfmathadd{\pgf@circ@labanc}{180}
			\edef\pgf@circ@labanc{\expandafter\pgf@circ@stripdecimals\pgfmathresult\pgf@nil}
		\fi
	}
	node [ anchor = \pgf@circ@labanc] 
	  at (\ctikzvalof{bipole/name}.\pgf@circ@temp) {\pgf@circ@finallabel{}}
}


\ctikzset{text/.style = { t=#1 } }
\ctikzset{t/.code = { 
	\ctikzsetvalof{bipoles/twoport/text}{#1}
}}

%%%---------- close: pgfcirclabel
%%%%%%%%%%% Springe nach pgfcircvoltage
%%%---------- open: pgfcircvoltage.tex
% Copyright 2007-2009 by Massimo Redaelli
%
% This file may be distributed and/or modified
%
% 1. under the LaTeX Project Public License and/or
% 2. under the GNU Public License.
%
% See the file doc/LICENSE for more details.

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%%  Voltage management


\ctikzset{v^>/.style = {
		v = #1,
		\circuitikzbasekey/bipole/voltage/direction = forward,
		\circuitikzbasekey/bipole/voltage/position = above
	}
}

\ctikzset{v^</.style = {
		v = #1,
		\circuitikzbasekey/bipole/voltage/direction = backward,
		\circuitikzbasekey/bipole/voltage/position = above
	}
}

\ctikzset{v_>/.style = {
		v = #1,
		\circuitikzbasekey/bipole/voltage/direction = forward,
		\circuitikzbasekey/bipole/voltage/position = below
	} 
}

\ctikzset{v_</.style = {
		v = #1,
		\circuitikzbasekey/bipole/voltage/direction = backward,
		\circuitikzbasekey/bipole/voltage/position = below
	} 
}


% Default position varies whether the component is a voltage source
% or not
\ctikzset{v/.code = {
			\ifpgf@circuit@bipole@isvoltage
				\pgfkeys{\circuitikzbasekey/bipole/voltage/position=above,
					\circuitikzbasekey/bipole/voltage/direction=forward}
			\else
				\pgfkeys{\circuitikzbasekey/bipole/voltage/position=below,
					\circuitikzbasekey/bipole/voltage/direction=backward}
			\fi
	\pgfkeys{/tikz/circuitikz/bipole/voltage/label/name=#1}
	\ctikzsetvalof{bipole/voltage/label/unit}{}
	\ifpgf@circ@siunitx 
		\pgf@circ@handleSI{#1}
		\ifpgf@circ@siunitx@res 
			\edef\pgf@temp{\pgf@circ@handleSI@val}
			\pgfkeyslet{/tikz/circuitikz/bipole/voltage/label/name}{\pgf@temp}
			\edef\pgf@temp{\pgf@circ@handleSI@unit}
			\pgfkeyslet{/tikz/circuitikz/bipole/voltage/label/unit}{\pgf@temp}
		\else
		\fi
	\else
	\fi
	} 
}

\ctikzset{v_/.style = {v = #1, \circuitikzbasekey/bipole/voltage/position = below} }
\ctikzset{v^/.style = {v = #1, \circuitikzbasekey/bipole/voltage/position  = above} }
\ctikzset{v>/.style = {v = #1, \circuitikzbasekey/bipole/voltage/direction = forward} }
\ctikzset{v</.style = {v = #1, \circuitikzbasekey/bipole/voltage/direction = backward} }


%% Output routine for generic bipoles

\def\pgf@circ@drawvoltagegeneric{
	\pgfextra{
		\ifnum \ctikzvalof{mirror value}=-1
						\ifpgf@circuit@bipole@voltage@below\pgf@circuit@bipole@voltage@belowfalse\else\pgf@circuit@bipole@voltage@belowtrue\fi
		\fi
		
		\ifpgf@circuit@bipole@voltage@below
			\def\pgf@circ@voltage@angle{90}
		\else
			\def\pgf@circ@voltage@angle{-90} 
		\fi	
		
		\edef\pgf@temp{/tikz/circuitikz/bipoles/\pgfkeysvalueof{/tikz/circuitikz/bipole/kind}/voltage/distance from node}
		\pgfkeysifdefined{\pgf@temp}
			{ \edef\distacefromnode{\ctikzvalof{bipoles/\pgfkeysvalueof{/tikz/circuitikz/bipole/kind}/voltage/distance from node}} }
			{ \edef\distacefromnode{\ctikzvalof{voltage/distance from node}} }
		\edef\pgf@temp{/tikz/circuitikz/bipoles/\pgfkeysvalueof{/tikz/circuitikz/bipole/kind}/voltage/bump b}
		\pgfkeysifdefined{\pgf@temp}
			{ \edef\bumpb{\ctikzvalof{bipoles/\pgfkeysvalueof{/tikz/circuitikz/bipole/kind}/voltage/bump b}} }
			{ \edef\bumpb{\ctikzvalof{voltage/bump b}} }
	}

	coordinate (pgfcirc@mid) at ($(\tikztostart) ! \distacefromnode ! (\ctikzvalof{bipole/name}.left)$)
	coordinate (pgfcirc@Vfrom) at ($(pgfcirc@mid) ! -\ctikzvalof{voltage/distance from line}\pgf@circ@Rlen ! \pgf@circ@voltage@angle:(\ctikzvalof{bipole/name}.left)$) 
   
	coordinate (pgfcirc@mid) at ($(\tikztotarget) ! \distacefromnode ! (\ctikzvalof{bipole/name}.right)$)
	coordinate (pgfcirc@Vto) at ($(pgfcirc@mid) ! \ctikzvalof{voltage/distance from line}\pgf@circ@Rlen ! \pgf@circ@voltage@angle : (\ctikzvalof{bipole/name}.right)$)

	\ifpgf@circuit@bipole@voltage@below
		coordinate (pgfcirc@Vcont1) at ($(\ctikzvalof{bipole/name}.center) ! \bumpb ! (\ctikzvalof{bipole/name}.-110)$)
		coordinate (pgfcirc@Vcont2) at ($(\ctikzvalof{bipole/name}.center) ! \bumpb ! (\ctikzvalof{bipole/name}.-70)$)
	\else
		coordinate (pgfcirc@Vcont1) at ($(\ctikzvalof{bipole/name}.center) ! \bumpb ! (\ctikzvalof{bipole/name}.110)$)
		coordinate (pgfcirc@Vcont2) at ($(\ctikzvalof{bipole/name}.center) ! \bumpb ! (\ctikzvalof{bipole/name}.70)$)
	\fi

	\ifpgf@circuit@europeanvoltage
		\ifpgf@circuit@bipole@voltage@backward
			(pgfcirc@Vto) .. controls (pgfcirc@Vcont2)  and (pgfcirc@Vcont1) .. 
				node[currarrow, sloped,  allow upside down, pos=1] {} 
			(pgfcirc@Vfrom) 
		\else
			(pgfcirc@Vfrom) .. controls (pgfcirc@Vcont1)  and (pgfcirc@Vcont2) ..
				node[currarrow, sloped,  allow upside down, pos=1] {}
			(pgfcirc@Vto) 	
		\fi	
	\else
		\ifpgf@circuit@bipole@voltage@backward
			(pgfcirc@Vfrom) node[inner sep=0, anchor=\pgf@circ@bipole@voltage@label@anchor]{\scriptsize$+$}   
			(pgfcirc@Vto) node[inner sep=0, anchor=\pgf@circ@bipole@voltage@label@anchor]{$-$}
		\else
			(pgfcirc@Vfrom) node[inner sep=0, anchor=\pgf@circ@bipole@voltage@label@anchor]{\scriptsize$-$}   
			(pgfcirc@Vto) node[inner sep=0, anchor=\pgf@circ@bipole@voltage@label@anchor]{$+$}
		\fi	
	\fi
}

%% Output routine for voltage sources

\def\pgf@circ@drawvoltagegenerator{
	\ifpgf@circuit@bipole@voltage@below
		coordinate (pgfcirc@Vcont1) at ($(\ctikzvalof{bipole/name}.center) ! \ctikzvalof{voltage/bump a} ! (\ctikzvalof{bipole/name}.-120)$)
		coordinate (pgfcirc@Vcont2) at ($(\ctikzvalof{bipole/name}.center) ! \ctikzvalof{voltage/bump a} ! (\ctikzvalof{bipole/name}.-60)$)
	\else
		coordinate (pgfcirc@Vcont1) at ($ (\ctikzvalof{bipole/name}.center) ! \ctikzvalof{voltage/bump a} ! (\ctikzvalof{bipole/name}.120)$)
		coordinate (pgfcirc@Vcont2) at ($ (\ctikzvalof{bipole/name}.center) ! \ctikzvalof{voltage/bump a} ! (\ctikzvalof{bipole/name}.60)$)
	\fi

	\ifpgf@circuit@europeanvoltage
		\ifpgf@circuit@bipole@voltage@backward
			(pgfcirc@Vcont2)  -- node[currarrow, sloped,  allow upside down, pos=1] {} (pgfcirc@Vcont1)
		\else
			(pgfcirc@Vcont1)  -- node[currarrow, sloped,  allow upside down, pos=1] {} (pgfcirc@Vcont2)
		\fi
	
	\else % american voltage
		
		\pgfextra{
			\def\pgf@temp{\pgfkeysvalueof{/tikz/circuitikz/bipole/kind}}
			\def\pgf@circ@temp{battery}
			\ifx\pgf@temp\pgf@circ@temp
				\edef\pgf@circ@batteria{battery}
			\else
				\def\pgf@circ@temp{battery1}
				\ifx\pgf@temp\pgf@circ@temp
					\edef\pgf@circ@batteria{battery}
				\else
					\edef\pgf@circ@batteria{false}
				\fi
			\fi
			\edef\pgf@circ@temp{battery}
		}
		
		\ifx\pgf@circ@batteria\pgf@circ@temp % if it is a battery, must put + and -
			\ifpgf@circuit@bipole@voltage@backward
				(pgfcirc@Vcont2)  node {$-$}  (pgfcirc@Vcont1) node {$+$}
			\else
				(pgfcirc@Vcont1)  node {$-$}  (pgfcirc@Vcont2) node {$+$}
			\fi
		\fi
		
	\fi
}

%% Output routine

\def\pgf@circ@drawvoltage{   % node name 
	\pgfextra{
		\edef\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgf@circ@direction\pgf@nil}

		\ifnum\pgfcircmathresult >4 \ifnum\pgfcircmathresult <86
			\ifpgf@circuit@bipole@voltage@below
				\def\pgf@circ@bipole@voltage@label@anchor{north west} 
			\else \def\pgf@circ@bipole@voltage@label@anchor{south east}
			\fi
		\fi\fi
		\ifnum\pgfcircmathresult >85 \ifnum\pgfcircmathresult <95
			\ifpgf@circuit@bipole@voltage@below
				\def\pgf@circ@bipole@voltage@label@anchor{west} 
			\else \def\pgf@circ@bipole@voltage@label@anchor{east} 
			\fi
		\fi\fi
		\ifnum\pgfcircmathresult >94 \ifnum\pgfcircmathresult <176
			\ifpgf@circuit@bipole@voltage@below
				 \def\pgf@circ@bipole@voltage@label@anchor{south west}
			\else \def\pgf@circ@bipole@voltage@label@anchor{north east}
			\fi
		\fi\fi
		\ifnum\pgfcircmathresult >175 \ifnum\pgfcircmathresult <185
			\ifpgf@circuit@bipole@voltage@below
				  \def\pgf@circ@bipole@voltage@label@anchor{south}
			\else\def\pgf@circ@bipole@voltage@label@anchor{north}
			\fi
		\fi\fi
		\ifnum\pgfcircmathresult >184 \ifnum\pgfcircmathresult <266
			\ifpgf@circuit@bipole@voltage@below
				 \def\pgf@circ@bipole@voltage@label@anchor{south east}
			\else\def\pgf@circ@bipole@voltage@label@anchor{north west}
			\fi
		\fi\fi
		\ifnum\pgfcircmathresult >265 \ifnum\pgfcircmathresult <275
			\ifpgf@circuit@bipole@voltage@below
				 \def\pgf@circ@bipole@voltage@label@anchor{east}
			\else \def\pgf@circ@bipole@voltage@label@anchor{west}
			\fi
		\fi\fi
		\ifnum\pgfcircmathresult >284 \ifnum\pgfcircmathresult <356
			\ifpgf@circuit@bipole@voltage@below
				  \def\pgf@circ@bipole@voltage@label@anchor{north east}
			\else\def\pgf@circ@bipole@voltage@label@anchor{south west}
			\fi
		\fi\fi
		\ifnum\pgfcircmathresult >-1 \ifnum\pgfcircmathresult <5
			\ifpgf@circuit@bipole@voltage@below
				 \def\pgf@circ@bipole@voltage@label@anchor{north}
			\else\def\pgf@circ@bipole@voltage@label@anchor{south} 
			\fi
		\fi\fi
		\ifnum\pgfcircmathresult >355 \ifnum\pgfcircmathresult <361
			\ifpgf@circuit@bipole@voltage@below
				  \def\pgf@circ@bipole@voltage@label@anchor{north}
			\else\def\pgf@circ@bipole@voltage@label@anchor{south}
			\fi
		\fi\fi

		\ifpgf@circuit@bipole@voltage@below
			\def\pgf@circ@bipole@voltage@label@where{-90}
		\else
			\def\pgf@circ@bipole@voltage@label@where{90}
		\fi
		
		\edef\pgf@temp{/tikz/circuitikz/bipoles/\pgfkeysvalueof{/tikz/circuitikz/bipole/kind}/voltage/european label distance}
		\pgfkeysifdefined{\pgf@temp}
			{ \edef\eudist{\ctikzvalof{bipoles/\pgfkeysvalueof{/tikz/circuitikz/bipole/kind}/voltage/european label distance}} }
			{ \edef\eudist{\ctikzvalof{voltage/european label distance}} }
	}

		\ifpgf@circuit@bipole@isvoltage
			\pgf@circ@drawvoltagegenerator 
		\else
			\pgf@circ@drawvoltagegeneric 
		\fi
		(\ctikzvalof{bipole/name}.\pgf@circ@bipole@voltage@label@where)
		coordinate (Vlab) at ($(\ctikzvalof{bipole/name}.center) !
			\ifpgf@circuit@europeanvoltage\eudist\else\ctikzvalof{voltage/american label distance}\fi !
			(\ctikzvalof{bipole/name}.\pgf@circ@bipole@voltage@label@where)$)
		node [anchor=\pgf@circ@bipole@voltage@label@anchor, inner sep=0] 
			  at (Vlab) { \pgf@circ@finallabel{voltage/} }
}





%		coordinate (pgfcirc@Vcont1) at ($ (\ctikzvalof{bipole/name}.center) ! 
%			\ctikzvalof{voltage/bump b} !
%			(\ctikzvalof{bipole/name}.-110) $)
%		coordinate (pgfcirc@Vcont2) at ($ (\ctikzvalof{bipole/name}.center) ! 
%			\ctikzvalof{voltage/bump b} ! 
%			(\ctikzvalof{bipole/name}.-70) $)
%	\else
%		coordinate (pgfcirc@Vcont1) at ($ (\ctikzvalof{bipole/name}.center) ! 
%			\ctikzvalof{voltage/bump b} !
%			(\ctikzvalof{bipole/name}.110) $)
%		coordinate (pgfcirc@Vcont2) at ($ (\ctikzvalof{bipole/name}.center) ! 
%			\ctikzvalof{voltage/bump b} ! 
%			(\ctikzvalof{bipole/name}.70) $)
%	\fi
%%%---------- close: pgfcircvoltage
%%%%%%%%%%% Springe nach pgfcirccurrent
%%%---------- open: pgfcirccurrent.tex
% Copyright 2007-2009 by Massimo Redaelli
%
% This file may be distributed and/or modified
%
% 1. under the LaTeX Project Public License and/or
% 2. under the GNU Public License.
%
% See the file doc/LICENSE for more details.

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%% Current handling

%% Options


\ctikzset{i^>/.style = {
		i = #1,
		\circuitikzbasekey/bipole/current/direction = forward,
		\circuitikzbasekey/bipole/current/x position = after,
		\circuitikzbasekey/bipole/current/y position = above
	}
}

\ctikzset{i_>/.style = {
		i = #1,
		\circuitikzbasekey/bipole/current/direction = forward,
		\circuitikzbasekey/bipole/current/x position = after,
		\circuitikzbasekey/bipole/current/y position = below
	}
}

\ctikzset{i>^/.style = {
		i = #1,
		\circuitikzbasekey/bipole/current/direction = forward,
		\circuitikzbasekey/bipole/current/x position = before,
		\circuitikzbasekey/bipole/current/y position = above
	}
}

\ctikzset{i>_/.style = {
		i = #1,
		\circuitikzbasekey/bipole/current/direction = forward,
		\circuitikzbasekey/bipole/current/x position = before,
		\circuitikzbasekey/bipole/current/y position = below
	}
}

\ctikzset{i^</.style = {
		i = #1,
		\circuitikzbasekey/bipole/current/direction = backward,
		\circuitikzbasekey/bipole/current/x position = after,
		\circuitikzbasekey/bipole/current/y position = above
	}
}

\ctikzset{i_</.style = {
		i = #1,
		\circuitikzbasekey/bipole/current/direction = backward,
		\circuitikzbasekey/bipole/current/x position = after,
		\circuitikzbasekey/bipole/current/y position = below
	}
}

\ctikzset{i<^/.style = {
		i = #1,
		\circuitikzbasekey/bipole/current/direction = backward,
		\circuitikzbasekey/bipole/current/x position = before,
		\circuitikzbasekey/bipole/current/y position = above
	}
}

\ctikzset{i<_/.style = {
		i = #1,
		\circuitikzbasekey/bipole/current/direction = backward,
		\circuitikzbasekey/bipole/current/x position = before,
		\circuitikzbasekey/bipole/current/y position = below
	}
}

\ctikzset{i/.code = {
%			\ifpgf@circuit@bipole@iscurrent
%				\pgfkeys{\circuitikzbasekey/bipole/current/position=above}
%			\else
%				\pgfkeys{\circuitikzbasekey/bipole/current/position=below}
%			\fi
			\pgfkeys{\circuitikzbasekey/bipole/current/direction = forward,
					\circuitikzbasekey/bipole/current/x position = after,
					\circuitikzbasekey/bipole/current/y position = above }
	\pgfkeys{/tikz/circuitikz/bipole/current/label/name=#1}
	\ctikzsetvalof{bipole/current/label/unit}{}
	\ifpgf@circ@siunitx 
		\pgf@circ@handleSI{#1}
		\ifpgf@circ@siunitx@res 
			\edef\pgf@temp{\pgf@circ@handleSI@val}
			\pgfkeyslet{/tikz/circuitikz/bipole/current/label/name}{\pgf@temp}
			\edef\pgf@temp{\pgf@circ@handleSI@unit}
			\pgfkeyslet{/tikz/circuitikz/bipole/current/label/unit}{\pgf@temp}
		\else
		\fi
	\else
	\fi
}
}

\ctikzset{i</.style = { i = #1, \circuitikzbasekey/bipole/current/direction = backward } }
\ctikzset{i_/.style = { i = #1, \circuitikzbasekey/bipole/current/y position = below } }
\ctikzset{i>/.style = {i = #1, \circuitikzbasekey/bipole/current/direction = forward } }
\ctikzset{i^/.style = { i= #1, \circuitikzbasekey/bipole/current/y position = above } }


\def\pgf@circ@drawnormalcurrent{
			\ifpgf@circuit@bipole@current@before
				\ifpgf@circuit@bipole@current@backward
					{  (\ctikzvalof{bipole/name}.left) -- 
							node [currarrow, pos=\ctikzvalof{current/distance}, sloped,  allow upside down] (Iarrow) {} 
						(\tikztostart)  
					}
				\else
					{  (\tikztostart) -- 
							node [currarrow, pos=\ctikzvalof{current/distance}, sloped,  allow upside down] (Iarrow) {} 
						(\ctikzvalof{bipole/name}.left)  
					}
				\fi
			\else
				\ifpgf@circuit@bipole@current@backward
					{ 	(\tikztotarget) -- 
							node [currarrow, pos=\ctikzvalof{current/distance}, sloped,  allow upside down] (Iarrow) {} 
						(\ctikzvalof{bipole/name}.right)  
					}
				\else
					{ 	(\ctikzvalof{bipole/name}.right) -- 
							node [currarrow, pos=\ctikzvalof{current/distance}, sloped,  allow upside down] (Iarrow) {}
						(\tikztotarget)  
					}
				\fi
			\fi
}

%% Output routine 
%% #1 - node name

\def\pgf@circ@drawcurrent{
	\pgfextra{
		\edef\pgf@circ@ffffff{\pgf@circ@direction}
		\def\pgfcircmathresult{\expandafter\pgf@circ@stripdecimals\pgf@circ@ffffff\pgf@nil}

		\ifnum\pgfcircmathresult >4 \ifnum\pgfcircmathresult <86
			\ifpgf@circuit@bipole@current@below
				\def\pgf@circ@dir{north west} \else \def\pgf@circ@dir{south east}
			\fi
		\fi\fi
		\ifnum\pgfcircmathresult >85 \ifnum\pgfcircmathresult <95
			\ifpgf@circuit@bipole@current@below
				\def\pgf@circ@dir{west} \else \def\pgf@circ@dir{east} 
			\fi
		\fi\fi
		\ifnum\pgfcircmathresult >94 \ifnum\pgfcircmathresult <176
			\ifpgf@circuit@bipole@current@below
				 \def\pgf@circ@dir{south west}\else \def\pgf@circ@dir{north east}
			\fi
		\fi\fi
		\ifnum\pgfcircmathresult >175 \ifnum\pgfcircmathresult <185
			\ifpgf@circuit@bipole@current@below
				  \def\pgf@circ@dir{south}\else\def\pgf@circ@dir{north}
			\fi
		\fi\fi
		\ifnum\pgfcircmathresult >184 \ifnum\pgfcircmathresult <266
			\ifpgf@circuit@bipole@current@below
				 \def\pgf@circ@dir{south east}\else\def\pgf@circ@dir{north west}
			\fi
		\fi\fi
		\ifnum\pgfcircmathresult >265 \ifnum\pgfcircmathresult <275
			\ifpgf@circuit@bipole@current@below
				 \def\pgf@circ@dir{east}\else \def\pgf@circ@dir{west}
			\fi
		\fi\fi
		\ifnum\pgfcircmathresult >284 \ifnum\pgfcircmathresult <356
			\ifpgf@circuit@bipole@current@below
				  \def\pgf@circ@dir{north east}\else\def\pgf@circ@dir{south west}
			\fi
		\fi\fi
		\ifnum\pgfcircmathresult <5
			\ifpgf@circuit@bipole@current@below
				 \def\pgf@circ@dir{north}\else\def\pgf@circ@dir{south} 
			\fi
		\fi
		\ifnum\pgfcircmathresult >355
			\ifpgf@circuit@bipole@current@below
				 \def\pgf@circ@dir{north}\else\def\pgf@circ@dir{south} 
			\fi
		\fi
		
		\ifpgf@circuit@bipole@current@below
			\def\pgf@circ@bipole@current@label@where{-90}
		\else
			\def\pgf@circ@bipole@current@label@where{+90}
		\fi
	}

	
		\pgfextra{	\def\pgf@temp{short} \edef\pgf@circ@temp{\ctikzvalof{bipole/kind}} }
		
		\ifx\pgf@circ@temp\pgf@temp % caso di corrente (centrata) su un corto
			\ifpgf@circuit@bipole@current@backward
				{ (\tikztotarget) -- 
					node [currarrow, pos=\ctikzvalof{current/distance}, sloped,  allow upside down] (Iarrow) {} 
				  (\tikztostart)  }
			\else
				{ (\tikztostart) -- 
					node [currarrow, pos=\ctikzvalof{current/distance}, sloped,  allow upside down] (Iarrow) {} 
				  (\tikztotarget)  }
			\fi
			
		\else % altri bipoli - e quindi tra nodo e target

			\ifpgf@circuit@bipole@iscurrent
				\ifpgf@circuit@europeancurrent
					\pgf@circ@drawnormalcurrent
				\else 
				\fi
			\else
				\pgf@circ@drawnormalcurrent
			\fi
		\fi

	\ifpgf@circuit@bipole@iscurrent
		 node [anchor=\pgf@circ@dir] at (\ctikzvalof{bipole/name}.\pgf@circ@bipole@current@label@where) 
		 	{ \pgf@circ@finallabel{current/} }
	\else
		(Iarrow.\pgf@circ@bipole@current@label@where) node [anchor=\pgf@circ@dir] 	
			{ \pgf@circ@finallabel{current/} } 
	\fi

}




%%%---------- close: pgfcirccurrent
%%%%%%%%%%% Springe nach pgfcircinputarrows
%%%---------- open: pgfcircinputarrows.tex
% Copyright 2013 by Stefan Erhardt
%
% This file may be distributed and/or modified
%
% 1. under the LaTeX Project Public License and/or
% 2. under the GNU Public License.
%
% See the file doc/LICENSE for more details.

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%% Show input arrows for selected parts


\ctikzset{>/.style = {
		\circuitikzbasekey/inputarrow = true
	}
}





%%%---------- close: pgfcircinputarrows




%%%---------- close: circuitikz.code

\ExecuteOptions{europeancurrents,europeanvoltages,americanports,americanresistors,cuteinductors,europeangfsurgearrester,nosiunitx,noarrowmos,smartlabels,nocompatibility}

\ProcessOptions\relax

\ifpgf@circ@siunitx
    \RequirePackage{xstring}[2009/03/13]
	%\expandafter\let\csname angstrom\endcsname\relax
	\RequirePackage{siunitx}
\fi

%%%%%%%%%%% Springe nach circuitikz1.code
%%%---------- open: circuitikz1.code.tex
%%%%%%%%%%%%
%% Dimensions

% coordinate bipoli
\newdimen\pgf@circ@res@up \newdimen\pgf@circ@res@down \newdimen\pgf@circ@res@zero
\newdimen\pgf@circ@res@left \newdimen\pgf@circ@res@right
\newdimen\pgf@circ@res@other
\newdimen\pgf@circ@res@step

% thickness iniziale
\newdimen \pgfstartlinewidth

\pgf@circ@Rlen = \pgfkeysvalueof{/tikz/circuitikz/bipoles/length}



% Names
\ctikzset{name/.style = { n=#1 } }
\ctikzset{n/.code = { 
	\pgfkeys{/tikz/circuitikz/bipole/name=#1}
}}

% Reflect the node along
\ctikzset{mirrored/.is choice}
\ctikzset{mirror value/.initial=1}
\ctikzset{mirrored/true/.code = {\ctikzsetvalof{mirror value}{-1}} }
\ctikzset{mirrored/false/.code = {\ctikzsetvalof{mirror value}{1}} }
\ctikzset{mirror/.style = {/tikz/circuitikz/mirrored=true}}

% Initialize paths
\def\pgfcircresetpath{
	\ctikzset{bipole/name=, bipole/label/name=, bipole/label/position=90, 
		bipole/reversed=false, bipole/kind=,
	  	bipole/voltage/direction=backward, bipole/voltage/label/name=, bipole/voltage/position=below,
	  	bipole/nodes/left=none, bipole/nodes/right=none, bipole/is voltage=false,
		bipole/is current=false, bipole/current/label/name=, bipole/current/x position=after,
		bipole/current/y position=above, bipole/current/direction=forward, 
		mirrored=false
   }
}


%% Generic bipole path
\def\pgf@circ@bipole@path#1#2{
	\pgfextra{
		\ctikzset{bipole/kind = #1}
		
		\edef\pgf@temp{\pgfkeysvalueof{/tikz/circuitikz/bipole/name}}
		\def\pgf@circ@temp{}
		\ifx\pgf@temp\pgf@circ@temp % if it has not a name
			\pgfmathrandominteger{\pgf@circ@rand}{1000}{9999}
			\ctikzset{bipole/name = #2\pgf@circ@rand} % create it
		\fi

		\def\pgf@temp{open}
		\def\pgf@circ@temp{#1}
	}
	\ifpgf@circuit@bipole@reversed
		(\tikztostart) node[coordinate] (\ctikzvalof{bipole/name}end) {}
		(\tikztotarget) node[coordinate] (\ctikzvalof{bipole/name}start) {} 	
	\else
		(\tikztostart) node[coordinate] (\ctikzvalof{bipole/name}start) {}
		(\tikztotarget) node[coordinate] (\ctikzvalof{bipole/name}end) {} 
	\fi
	\pgfextra{
		\pgf@circ@slope{\pgfpointanchor{\ctikzvalof{bipole/name}start}{center}}
					   {\pgfpointanchor{\ctikzvalof{bipole/name}end}{center}}
		\edef\pgf@circ@direction{\pgfmathresult}		
	}
	($(\tikztostart) ! .5 ! (\tikztotarget)$) 
		node[#1shape, rotate=\pgf@circ@direction, yscale=\ctikzvalof{mirror value}] 
			(\ctikzvalof{bipole/name}) {}
	\ifx\pgf@temp\pgf@circ@temp  % if it is an open
	\else
		(\ctikzvalof{bipole/name}start.center) -- (\ctikzvalof{bipole/name}.left) 
		(\ctikzvalof{bipole/name}.right)  -- (\ctikzvalof{bipole/name}end.center) 
	\fi
	\pgf@circ@ifkeyempty{bipole/label/name}\else\pgf@circ@drawlabel\fi
	\drawpoles
	\pgf@circ@ifkeyempty{bipole/voltage/label/name}\else\pgf@circ@drawvoltage\fi
	\pgf@circ@ifkeyempty{bipole/current/label/name}\else\pgf@circ@drawcurrent\fi
	% reset
	\pgfextra{
		\pgfcircresetpath
	}  
	(\tikztotarget) 	\tikztonodes  % e si continua
}


%% Path definitions

\def\pgf@circ@resistor@path#1{\ifpgf@circuit@europeanresistor\pgf@circ@bipole@path{generic}{#1}\else\pgf@circ@bipole@path{resistor}{#1}\fi}
\def\pgf@circ@vresistor@path#1{\ifpgf@circuit@europeanresistor\pgf@circ@bipole@path{tgeneric}{#1}\else\pgf@circ@bipole@path{vresistor}{#1}\fi}
\def\pgf@circ@potentiometer@path#1{\ifpgf@circuit@europeanresistor\pgf@circ@bipole@path{genericpotentiometer}{#1}\else\pgf@circ@bipole@path{potentiometer}{#1}\fi}
\def\pgf@circ@thermistor@path#1{\pgf@circ@bipole@path{thermistor}{#1}}
\def\pgf@circ@thermistorptc@path#1{\pgf@circ@bipole@path{thermistorptc}{#1}}
\def\pgf@circ@thermistorntc@path#1{\pgf@circ@bipole@path{thermistorntc}{#1}}
\def\pgf@circ@varistor@path#1{\pgf@circ@bipole@path{varistor}{#1}}
\def\pgf@circ@capacitor@path#1{\pgf@circ@bipole@path{capacitor}{#1}}
\def\pgf@circ@polarcapacitor@path#1{\pgf@circ@bipole@path{polarcapacitor}{#1}}
\def\pgf@circ@vcapacitor@path#1{\pgf@circ@bipole@path{vcapacitor}{#1}}
\def\pgf@circ@battery@path#1{\pgf@circ@bipole@path{battery}{#1}}
\def\pgf@circ@battery1@path#1{\pgf@circ@bipole@path{battery1}{#1}}
\def\pgf@circ@europeaninductor@path#1{\pgf@circ@bipole@path{fullgeneric}{#1}}
\def\pgf@circ@americaninductor@path#1{\pgf@circ@bipole@path{americaninductor}{#1}}
\def\pgf@circ@cuteinductor@path#1{\pgf@circ@bipole@path{cuteinductor}{#1}}
\def\pgf@circ@inductor@path#1{%
	\pgfextra{
		\edef\pgf@circ@temp{\ctikzvalof{inductor}}%
		\def\pgf@temp{european}%
	}
	\ifx\pgf@temp\pgf@circ@temp%
		\pgf@circ@europeaninductor@path{#1}%
	\else%
		\pgfextra{	\def\pgf@temp{cute} }%
		\ifx\pgf@temp\pgf@circ@temp%
			\pgf@circ@cuteinductor@path{#1}%
		\else%
			\pgf@circ@americaninductor@path{#1}%
		\fi%
	\fi%
}
\def\pgf@circ@vinductor@path#1{
	\pgfextra{
		\edef\pgf@circ@temp{\ctikzvalof{inductor}}%
		\def\pgf@temp{european}%
	}
	\ifx\pgf@temp\pgf@circ@temp%
		\pgf@circ@veuropeaninductor@path{#1}%
	\else%
		\pgfextra{	\def\pgf@temp{cute} }%
		\ifx\pgf@temp\pgf@circ@temp%
			\pgf@circ@vcuteinductor@path{#1}%
		\else%
			\pgf@circ@vamericaninductor@path{#1}%
		\fi%
	\fi%
}
\def\pgf@circ@veuropeaninductor@path#1{\pgf@circ@bipole@path{tfullgeneric}{#1}}
\def\pgf@circ@vamericaninductor@path#1{\pgf@circ@bipole@path{vamericaninductor}{#1}}
\def\pgf@circ@vcuteinductor@path#1{\pgf@circ@bipole@path{vcuteinductor}{#1}}
\def\pgf@circ@lamp@path#1{\pgf@circ@bipole@path{lamp}{#1}}
\def\pgf@circ@vsource@path#1{\pgf@circ@bipole@path{vsource}{#1}}
\def\pgf@circ@vsourceam@path#1{\pgf@circ@bipole@path{vsourceAM}{#1}}
\def\pgf@circ@vsourcesin@path#1{\pgf@circ@bipole@path{vsourcesin}{#1}}
\def\pgf@circ@isource@path#1{\pgf@circ@bipole@path{isource}{#1}}
\def\pgf@circ@isourcesin@path#1{\pgf@circ@bipole@path{isourcesin}{#1}}
\def\pgf@circ@vsourcesquare@path#1{\pgf@circ@bipole@path{vsourcesquare}{#1}}
\def\pgf@circ@isourceam@path#1{\pgf@circ@bipole@path{isourceAM}{#1}}
\def\pgf@circ@cvsource@path#1{\pgf@circ@bipole@path{cvsource}{#1}}
\def\pgf@circ@cvsourceam@path#1{\pgf@circ@bipole@path{cvsourceAM}{#1}}
\def\pgf@circ@cvsourcesin@path#1{\pgf@circ@bipole@path{cvsourcesin}{#1}}
\def\pgf@circ@cisource@path#1{\pgf@circ@bipole@path{cisource}{#1}}
\def\pgf@circ@cisourceam@path#1{\pgf@circ@bipole@path{cisourceAM}{#1}}
\def\pgf@circ@cisourcesin@path#1{\pgf@circ@bipole@path{cisourcesin}{#1}}
\def\pgf@circ@fulldiode@path#1{\pgf@circ@bipole@path{fulldiode}{#1}}
\def\pgf@circ@fullzdiode@path#1{\pgf@circ@bipole@path{fullzdiode}{#1}}
\def\pgf@circ@fullsdiode@path#1{\pgf@circ@bipole@path{fullsdiode}{#1}}
\def\pgf@circ@fulltdiode@path#1{\pgf@circ@bipole@path{fulltdiode}{#1}}
\def\pgf@circ@fulllediode@path#1{\pgf@circ@bipole@path{fulllediode}{#1}}
\def\pgf@circ@fullpdiode@path#1{\pgf@circ@bipole@path{fullpdiode}{#1}}
\def\pgf@circ@fullvarcap@path#1{\pgf@circ@bipole@path{fullvarcap}{#1}}
\def\pgf@circ@emptydiode@path#1{\pgf@circ@bipole@path{emptydiode}{#1}}
\def\pgf@circ@emptyzdiode@path#1{\pgf@circ@bipole@path{emptyzdiode}{#1}}
\def\pgf@circ@emptysdiode@path#1{\pgf@circ@bipole@path{emptysdiode}{#1}}
\def\pgf@circ@emptytdiode@path#1{\pgf@circ@bipole@path{emptytdiode}{#1}}
\def\pgf@circ@emptylediode@path#1{\pgf@circ@bipole@path{emptylediode}{#1}}
\def\pgf@circ@emptypdiode@path#1{\pgf@circ@bipole@path{emptypdiode}{#1}}
\def\pgf@circ@emptyvarcap@path#1{\pgf@circ@bipole@path{emptyvarcap}{#1}}
\def\pgf@circ@short@path#1{\pgf@circ@bipole@path{short}{#1}}
\def\pgf@circ@cspst@path#1{\pgf@circ@bipole@path{cspst}{#1}}
\def\pgf@circ@ospst@path#1{\pgf@circ@bipole@path{ospst}{#1}}
\def\pgf@circ@pushbutton@path#1{\pgf@circ@bipole@path{pushbutton}{#1}}
\def\pgf@circ@open@path#1{\pgf@circ@bipole@path{open}{#1}}
\def\pgf@circ@generic@path#1{\pgf@circ@bipole@path{generic}{#1}}
\def\pgf@circ@ageneric@path#1{\pgf@circ@bipole@path{ageneric}{#1}}
\def\pgf@circ@tgeneric@path#1{\pgf@circ@bipole@path{tgeneric}{#1}}
\def\pgf@circ@fullgeneric@path#1{\pgf@circ@bipole@path{fullgeneric}{#1}}
\def\pgf@circ@tfullgeneric@path#1{\pgf@circ@bipole@path{tfullgeneric}{#1}}
\def\pgf@circ@ammeter@path#1{\pgf@circ@bipole@path{ammeter}{#1}}
\def\pgf@circ@voltmeter@path#1{\pgf@circ@bipole@path{voltmeter}{#1}}
\def\pgf@circ@empty@path#1{}
\def\pgf@circ@photoresistor@path#1{\pgf@circ@bipole@path{photoresistor}{#1}}
\def\pgf@circ@thyristor@path#1{\pgf@circ@bipole@path{thyristor}{#1}}
\def\pgf@circ@toggleswitch@path#1{\pgf@circ@bipole@path{toggleswitch}{#1}}
\def\pgf@circ@memristor@path#1{\pgf@circ@bipole@path{memristor}{#1}}
\def\pgf@circ@triac@path#1{\pgf@circ@bipole@path{triac}{#1}}
\def\pgf@circ@tline@path#1{\pgf@circ@bipole@path{tline}{#1}}
\def\pgf@circ@squid@path#1{\pgf@circ@bipole@path{squid}{#1}}
\def\pgf@circ@barrier@path#1{\pgf@circ@bipole@path{barrier}{#1}}
\def\pgf@circ@thermocouple@path#1{\pgf@circ@bipole@path{thermocouple}{#1}}
\def\pgf@circ@fuse@path#1{\pgf@circ@bipole@path{fuse}{#1}}
\def\pgf@circ@afuse@path#1{\pgf@circ@bipole@path{afuse}{#1}}

\def\pgf@circ@twoport@path#1{\pgf@circ@bipole@path{twoport}{#1}}
\def\pgf@circ@vco@path#1{\pgf@circ@bipole@path{vco}{#1}}
\def\pgf@circ@bandpass@path#1{\pgf@circ@bipole@path{bandpass}{#1}}
\def\pgf@circ@highpass@path#1{\pgf@circ@bipole@path{highpass}{#1}}
\def\pgf@circ@lowpass@path#1{\pgf@circ@bipole@path{lowpass}{#1}}
\def\pgf@circ@adc@path#1{\pgf@circ@bipole@path{adc}{#1}}
\def\pgf@circ@dac@path#1{\pgf@circ@bipole@path{dac}{#1}}
\def\pgf@circ@dsp@path#1{\pgf@circ@bipole@path{dsp}{#1}}
\def\pgf@circ@fft@path#1{\pgf@circ@bipole@path{fft}{#1}}
\def\pgf@circ@amp@path#1{\pgf@circ@bipole@path{amp}{#1}}
\def\pgf@circ@vamp@path#1{\pgf@circ@bipole@path{vamp}{#1}}
\def\pgf@circ@piattenuator@path#1{\pgf@circ@bipole@path{piattenuator}{#1}}
\def\pgf@circ@vpiattenuator@path#1{\pgf@circ@bipole@path{vpiattenuator}{#1}}
\def\pgf@circ@tattenuator@path#1{\pgf@circ@bipole@path{tattenuator}{#1}}
\def\pgf@circ@vtattenuator@path#1{\pgf@circ@bipole@path{vtattenuator}{#1}}
\def\pgf@circ@phaseshifter@path#1{\pgf@circ@bipole@path{phaseshifter}{#1}}
\def\pgf@circ@vphaseshifter@path#1{\pgf@circ@bipole@path{vphaseshifter}{#1}}
\def\pgf@circ@detector@path#1{\pgf@circ@bipole@path{detector}{#1}}


%% Styles

%% Aggiungere per thyristor e tripoli semplici

%\def\ctikzsetbipole#1#2{%
%	\tikzset{#1/.style= {to path=#2, \circuitikzbasekey, l=##1}}%
%}
%\ctikzsetbipole{resistor}{\pgf@circ@resistor@path}

\tikzset{resistor/.style= {\circuitikzbasekey, /tikz/to path=\pgf@circ@resistor@path, l=#1}}
\tikzset{american resistor/.style= {\circuitikzbasekey, /tikz/to path=\pgf@circ@bipole@path{resistor}{#1}, l=#1}}
\tikzset{european resistor/.style= {\circuitikzbasekey, /tikz/to path=\pgf@circ@bipole@path{generic}{#1}, l=#1}}
\tikzset{ammeter/.style= {\circuitikzbasekey, /tikz/to path=\pgf@circ@ammeter@path, l=#1}}
\tikzset{voltmeter/.style= {\circuitikzbasekey, /tikz/to path=\pgf@circ@voltmeter@path, l=#1}}
\tikzset{potentiometer/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@potentiometer@path, l=#1}}
\tikzset{varistor/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@varistor@path, l=#1}}
\tikzset{photoresistor/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@photoresistor@path, l=#1}}
\tikzset{thermistor/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@thermistor@path, l=#1}}
\tikzset{thermistor ptc/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@thermistorptc@path, l=#1}}
\tikzset{thermistor ntc/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@thermistorntc@path, l=#1}}
\tikzset{american potentiometer/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@bipole@path{potentiometer}{#1}, l=#1}}
\tikzset{european potentiometer/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@bipole@path{genericpotentiometer}{#1}, l=#1}}
\tikzset{variable resistor/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@vresistor@path, l=#1}}
\tikzset{variable american resistor/.style= {\circuitikzbasekey, /tikz/to path=\pgf@circ@bipole@path{vresistor}{#1}, l=#1}}
\tikzset{variable european resistor/.style= {\circuitikzbasekey, /tikz/to path=\pgf@circ@bipole@path{tgeneric}{#1}, l=#1}}
\tikzset{capacitor/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@capacitor@path, l=#1}}
\tikzset{polar capacitor/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@polarcapacitor@path, l=#1}}
\tikzset{variable capacitor/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@vcapacitor@path, l=#1}}
\tikzset{battery/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@battery@path, \circuitikzbasekey/bipole/is voltage=true, v=#1}}
\tikzset{battery1/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@battery1@path, \circuitikzbasekey/bipole/is voltage=true, v=#1}}
\tikzset{inductor/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@inductor@path, l=#1}}
\tikzset{american inductor/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@americaninductor@path, l=#1}}
\tikzset{cute inductor/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@cuteinductor@path, l=#1}}
\tikzset{european inductor/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@europeaninductor@path, l=#1}}
\tikzset{variable inductor/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@vinductor@path, l=#1}}
\tikzset{variable european inductor/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@veuropeaninductor@path, l=#1}}
\tikzset{variable american inductor/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@vamericaninductor@path, l=#1}}
\tikzset{variable cute inductor/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@vcuteinductor@path, l=#1}}
\tikzset{tline/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@tline@path, l=#1}}
\tikzset{transmission line/.style = {tline = #1}}
\tikzset{TL/.style = {tline = #1}}
\tikzset{european voltage source/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@vsource@path, \circuitikzbasekey/bipole/is voltage=true, v=#1}}
\tikzset{american voltage source/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@vsourceam@path, \circuitikzbasekey/bipole/is voltage=true, v=#1}}
\tikzset{european current source/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@isource@path, \circuitikzbasekey/bipole/is current=true, i=#1}}
\tikzset{american current source/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@isourceam@path, \circuitikzbasekey/bipole/is current=true, i=#1}}
\tikzset{european controlled voltage source/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@cvsource@path, \circuitikzbasekey/bipole/is voltage=true, v=#1}}
\tikzset{american controlled voltage source/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@cvsourceam@path, \circuitikzbasekey/bipole/is voltage=true, v=#1}}
\tikzset{european controlled current source/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@cisource@path, \circuitikzbasekey/bipole/is current=true, i=#1}}
\tikzset{american controlled current source/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@cisourceam@path, \circuitikzbasekey/bipole/is current=true, i=#1}}
\tikzset{sinusoidal voltage source/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@vsourcesin@path, \circuitikzbasekey/bipole/is voltage=true, v=#1 }}
\tikzset{square voltage source/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@vsourcesquare@path, \circuitikzbasekey/bipole/is voltage=true, v=#1 }}
\tikzset{sinusoidal current source/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@isourcesin@path, \circuitikzbasekey/bipole/is current=true, i=#1}}
\tikzset{controlled sinusoidal voltage source/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@cvsourcesin@path, \circuitikzbasekey/bipole/is voltage=true, v=#1}}
\tikzset{controlled sinusoidal current source/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@cisourcesin@path, \circuitikzbasekey/bipole/is current=true, i=#1}}

\tikzset{voltage source/.style = {\ifpgf@circuit@europeanvoltage european \else american \fi voltage source, \circuitikzbasekey/bipole/is voltage=true, v=#1}}
\tikzset{current source/.style = {\ifpgf@circuit@europeancurrent european \else american \fi current source, \circuitikzbasekey/bipole/is current=true, i=#1}}
\tikzset{controlled voltage source/.style = {\ifpgf@circuit@europeanvoltage european \else american \fi controlled voltage source, \circuitikzbasekey/bipole/is voltage=true, v=#1}}
\tikzset{controlled current source/.style = {\ifpgf@circuit@europeancurrent european \else american \fi controlled current source, \circuitikzbasekey/bipole/is current=true, i=#1}}


\tikzset{generic/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@generic@path, l=#1}}
\tikzset{ageneric/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@ageneric@path, l=#1}}
\tikzset{tgeneric/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@tgeneric@path, l=#1}}
\tikzset{fullgeneric/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@fullgeneric@path, l=#1}}
\tikzset{tfullgeneric/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@tfullgeneric@path, l=#1}}
\tikzset{short/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@short@path}}
\tikzset{open/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@open@path}}

\tikzset{lamp/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@lamp@path}}

\tikzset{squid/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@squid@path}}
\tikzset{barrier/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@barrier@path}}
\tikzset{thermocouple/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@thermocouple@path}}
\tikzset{fuse/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@fuse@path}}
\tikzset{asymmetric fuse/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@afuse@path}}

\tikzset{twoport/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@twoport@path}}
\tikzset{vco/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@vco@path}}
\tikzset{bandpass/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@bandpass@path}}
\tikzset{highpass/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@highpass@path}}
\tikzset{lowpass/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@lowpass@path}}
\tikzset{adc/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@adc@path}}
\tikzset{dac/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@dac@path}}
\tikzset{dsp/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@dsp@path}}
\tikzset{fft/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@fft@path}}
\tikzset{amp/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@amp@path}}
\tikzset{vamp/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@vamp@path}}
\tikzset{piattenuator/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@piattenuator@path}}
\tikzset{vpiattenuator/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@vpiattenuator@path}}
\tikzset{tattenuator/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@tattenuator@path}}
\tikzset{vtattenuator/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@vtattenuator@path}}
\tikzset{phaseshifter/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@phaseshifter@path}}
\tikzset{vphaseshifter/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@vphaseshifter@path}}
\tikzset{detector/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@detector@path}}



\tikzset{full diode/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@fulldiode@path}}
\tikzset{full Schottky diode/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@fullsdiode@path}}
\tikzset{full Zener diode/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@fullzdiode@path}}
\tikzset{full tunnel diode/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@fulltdiode@path}}
\tikzset{full photodiode/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@fullpdiode@path}}
\tikzset{full led/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@fulllediode@path}}
\tikzset{full varcap/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@fullvarcap@path}}

\tikzset{empty diode/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@emptydiode@path}}
\tikzset{empty Schottky diode/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@emptysdiode@path}}
\tikzset{empty Zener diode/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@emptyzdiode@path}}
\tikzset{empty tunnel diode/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@emptytdiode@path}}
\tikzset{empty photodiode/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@emptypdiode@path}}
\tikzset{empty led/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@emptylediode@path}}
\tikzset{empty varcap/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@emptyvarcap@path}}

	\tikzset{Schottky diode/.style = {\ifpgf@circuit@fulldiode full \else empty \fi Schottky diode}}
	\tikzset{Zener diode/.style = {\ifpgf@circuit@fulldiode full \else empty \fi Zener diode}}
	\tikzset{tunnel diode/.style = {\ifpgf@circuit@fulldiode full \else empty \fi tunnel diode}}
	\tikzset{photodiode/.style = {\ifpgf@circuit@fulldiode full \else empty \fi photodiode}}
	\tikzset{led/.style = {\ifpgf@circuit@fulldiode full \else empty \fi led}}
	\tikzset{varcap/.style = {\ifpgf@circuit@fulldiode full \else empty \fi varcap}}
	\tikzset{diode/.style = {\ifpgf@circuit@fulldiode full \else empty \fi diode}}
	
\tikzset{thyristor/.style =  {\circuitikzbasekey, /tikz/to path=\pgf@circ@thyristor@path}}
\tikzset{memristor/.style =  {\circuitikzbasekey, /tikz/to path=\pgf@circ@memristor@path}}
\tikzset{triac/.style =  {\circuitikzbasekey, /tikz/to path=\pgf@circ@triac@path}}

\tikzset{closing switch/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@cspst@path, l=#1}}
\tikzset{opening switch/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@ospst@path, l=#1}}
\tikzset{push button/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@pushbutton@path, l=#1}}
\tikzset{toggle switch/.style =  {\circuitikzbasekey, /tikz/to path=\pgf@circ@toggleswitch@path}}

\tikzset{ammeter/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@ammeter@path}}
\tikzset{voltmeter/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@voltmeter@path}}

% short forms
\tikzset{vsource/.style = {voltage source = #1}}
\tikzset{isource/.style = {current source = #1}}
\tikzset{cisource/.style = {controlled current source = #1}}
\tikzset{cvsource/.style = {controlled voltage source = #1}}
\tikzset{vsourcesin/.style = {sinusoidal voltage source = #1}}
\tikzset{vsourcesquare/.style = {square voltage source = #1}}
\tikzset{isourcesin/.style = {sinusoidal current source = #1}}
\tikzset{cisourcesin/.style = {controlled sinusoidal current source = #1}}
\tikzset{cvsourcesin/.style = {controlled sinusoidal  voltage source = #1}}

\tikzset{controlled vsource/.style = {controlled voltage source = #1}}
\tikzset{controlled isource/.style = {controlled current source = #1}}
\tikzset{controlled vsourcesin/.style = {controlled sinusoidal  voltage source = #1}}
\tikzset{controlled isourcesin/.style = {controlled sinusoidal current source = #1}}

\tikzset{R/.style= {resistor = #1}}
\tikzset{vR/.style= {variable resistor = #1}}
\tikzset{phR/.style= {photoresistor = #1}}
\tikzset{thR/.style= {thermistor = #1}}
\tikzset{thRp/.style= {thermistor ptc= #1}}
\tikzset{thRn/.style= {thermistor ntc= #1}}
\tikzset{pR/.style= {potentiometer = #1}}
\tikzset{C/.style = {capacitor = #1}}
\tikzset{pC/.style = {polar capacitor = #1}}
\tikzset{vC/.style = {variable capacitor = #1}}
\tikzset{L/.style = {inductor = #1}}
\tikzset{vL/.style = {variable inductor = #1}}
\tikzset{V/.style = {voltage source = #1}}
\tikzset{cV/.style = {controlled voltage source = #1}}
\tikzset{sV/.style = {sinusoidal voltage source = #1}}
\tikzset{sqV/.style = {square voltage source = #1}}
\tikzset{csV/.style = {controlled sinusoidal voltage source = #1}}
\def\pgf@temp#1{ 
	\tikzset{V#1/.style = {voltage source, v#1=##1} } 
	\tikzset{cV#1/.style = {controlled  voltage source, v#1=##1} } 
	\tikzset{sV#1/.style = {sinusoidal  voltage source, v#1=##1} } 
	\tikzset{csV#1/.style = {controlled sinusoidal voltage source, v#1=##1} } 
}
\pgf@temp{_>} \pgf@temp{_<} \pgf@temp{^>} \pgf@temp{^<} 
\pgf@temp{>} \pgf@temp{<} \pgf@temp{^} \pgf@temp{_} 
\tikzset{I/.style = {current source = #1}}
\tikzset{cI/.style = {controlled current source = #1}}
\tikzset{sI/.style = {sinusoidal current source = #1}}
\tikzset{csI/.style = {controlled sinusoidal current source = #1}}
\def\pgf@temp#1{ 
	\tikzset{I#1/.style = {current source, i#1=##1} } 
	\tikzset{cI#1/.style = {controlled current source, i#1=##1} } 
	\tikzset{sI#1/.style = {sinusoidal current source, i#1=##1} } 
	\tikzset{csI#1/.style = {controlled sinusoidal current source, i#1=##1} } 
}
\pgf@temp{_>} \pgf@temp{_<} \pgf@temp{^>} \pgf@temp{^<} 
\pgf@temp{>_} \pgf@temp{<_} \pgf@temp{>^} \pgf@temp{<^} 
\pgf@temp{>} \pgf@temp{<} \pgf@temp{^} \pgf@temp{_} 
\tikzset{Do/.style = {empty diode}}
\tikzset{tDo/.style = {empty tunnel diode}}
\tikzset{zDo/.style = {empty Zener diode}}
\tikzset{sDo/.style = {empty Schottky diode}}
\tikzset{pDo/.style = {empty photodiode}}
\tikzset{leDo/.style = {empty led}}
\tikzset{VCo/.style = {empty varcap}}
\tikzset{D*/.style = {full diode}}
\tikzset{tD*/.style = {full tunnel diode}}
\tikzset{zD*/.style = {full Zener diode}}
\tikzset{sD*/.style = {full Schottky diode}}
\tikzset{pD*/.style = {full photodiode}}
\tikzset{leD*/.style = {full led}}
\tikzset{VC*/.style = {full varcap}}
\tikzset{D/.style = {diode}}
\tikzset{tD/.style = {tunnel diode}}
\tikzset{zD/.style = {Zener diode}}
\tikzset{sD/.style = {Schottky diode}}
\tikzset{pD/.style = {photodiode}}
\tikzset{leD/.style = {led}}
\tikzset{VC/.style = {varcap}}

\tikzset{Tr/.style = {triac}}
\tikzset{Mr/.style = {memristor}}
\tikzset{Ty/.style = {thyristor}}

\tikzset{cspst/.style = {closing switch = #1}}
\tikzset{ospst/.style = {opening switch = #1}}

\tikzset{afuse/.style = {asymmetric fuse=#1}}


\def\inheritlogicport#1#2{
	\pgfdeclareshape{#2 port}{
		\inheritsavedanchors[from=#1 #2 port]
		\inheritbackgroundpath[from=#1 #2 port]
		\inheritanchor[from=#1 #2 port]{in}
		\inheritanchor[from=#1 #2 port]{in 1}
		\inheritanchor[from=#1 #2 port]{in 2}
		\inheritanchor[from=#1 #2 port]{out}
		\inheritanchor[from=#1 #2 port]{center}
		\inheritanchor[from=#1 #2 port]{left}
	}
}

\ifpgf@circuit@europeanlogicport
	\inheritlogicport{european}{and}
	\inheritlogicport{european}{or}
	\inheritlogicport{european}{xor}
	\inheritlogicport{european}{not}
	\inheritlogicport{european}{nand}
	\inheritlogicport{european}{nor}
	\inheritlogicport{european}{xnor}
\else
	\inheritlogicport{american}{and}
	\inheritlogicport{american}{or}
	\inheritlogicport{american}{xor}
	\inheritlogicport{american}{not}
	\inheritlogicport{american}{nand}
	\inheritlogicport{american}{nor}
	\inheritlogicport{american}{xnor}
\fi

% Transistor like bipoles

\def\pgf@circ@trans@path#1#2{
	\pgfextra{
		\edef\pgf@temp{\pgfkeysvalueof{/tikz/circuitikz/bipole/name}}
		\def\pgf@circ@temp{#2}
		\ifx\pgf@temp\pgf@circ@temp % if it has not a name
			\pgfmathrandominteger{\pgf@circ@rand}{1000}{9999}
			\ctikzset{bipole/name = trans\pgf@circ@rand} % create it
		\fi
	}
	\ifpgf@circuit@bipole@reversed
		(\tikztostart) node[coordinate] (\ctikzvalof{bipole/name}end) {}
		(\tikztotarget) node[coordinate] (\ctikzvalof{bipole/name}start) {} 	
	\else
		(\tikztostart) node[coordinate] (\ctikzvalof{bipole/name}start) {}
		(\tikztotarget) node[coordinate] (\ctikzvalof{bipole/name}end) {} 
	\fi
	\pgfextra{
		\pgf@circ@slope{\pgfpointanchor{\ctikzvalof{bipole/name}start}{center}}
					   {\pgfpointanchor{\ctikzvalof{bipole/name}end}{center}}
		\pgfmathadd{\pgfmathresult}{-90}
		\edef\pgf@circ@direction{\pgfmathresult}
	}
	($(\tikztostart) ! .5 ! (\tikztotarget)$) 
		node[#1, /tikz/rotate=\pgf@circ@direction, xscale=\ctikzvalof{mirror value}] 
			(\ctikzvalof{bipole/name}) {} node {\ctikzvalof{bipole/label/name}}
	(\ctikzvalof{bipole/name}start.center) -- (\ctikzvalof{bipole/name}.left) 
	(\ctikzvalof{bipole/name}.right)  -- (\ctikzvalof{bipole/name}end.center) 
	\pgfextra{
		\pgfcircresetpath
	}  
	(\tikztotarget) 	\tikztonodes  % e si continua
}


\def\pgf@circ@definetranspath#1{
	\tikzset{T#1/.style = {\circuitikzbasekey, /tikz/to path=\pgf@circ@trans@path{#1}{}, l=##1}}
}

\pgf@circ@definetranspath{nmos}
\pgf@circ@definetranspath{pmos}
\pgf@circ@definetranspath{npn}
\pgf@circ@definetranspath{pnp}
\pgf@circ@definetranspath{nfet}
\pgf@circ@definetranspath{nigfete}
\pgf@circ@definetranspath{nigfetd}
\pgf@circ@definetranspath{pfet}
\pgf@circ@definetranspath{pigfete}
\pgf@circ@definetranspath{pigfetd}
\pgf@circ@definetranspath{njfet}
\pgf@circ@definetranspath{pjfet}
\pgf@circ@definetranspath{pigbt}
\pgf@circ@definetranspath{nigbt}
%%%---------- close: circuitikz1.code

\newenvironment{circuitikz}{\begin{tikzpicture}}{\end{tikzpicture}}


\endinput

